{"text_format":"1","workbook":"xlsx","n_sheets":105,"sheets":["Summary Table","509 Fabrications-Optimum","HHH-Accentra-2","HHH-Accentra 52i-TC","HHH-Allure 50","US Stove 6041","AES Baby","AES 3500P ","AES Little Rascal","APR 100","APR Baywin","APR Previa","EvenTemp Eclipse","EvenTemp Ashby","EvenTemp Prescott EXP","EvenTemp Hastings","HHT Santa FE-C","HHT PP60-B","HHT PP70","HHT PPC90","HHT PP130","HHT Classic Bay 1200 iC","HHT Classic Bay 1200C","HHT PS35-C","HHT P43-C","HHT CAB50-C","HHT P61-C","HHT P68-C","HHT Absolute 43-C","HHT Absolute 63","HHT Mt. Vernon E2-C","HHT XXV-TC","HHT P35i-C","HHT PH50PS-B","Castle Serenity","Englander CAB80","Englander CB120","Englander 25-CB PAH","Englanders 25-CBEP","Englander 25-PDVC","Englander 25-SSP","Enviro M55","Enviro Mini P3","Enviro Meridian & GF55","Enviro MAXX-1","HRSW Chatham","SMG HP21","SMG HP22","SMG HP61","Travis Fox Fire","Travis Deerfield","Travis AGP Insert","Travis AGP PS","True North 40","USSC 4840","USSC SP24","USSC SP2047","USSC SP1000","United States Stove-5780 Series","United States Stove - 5770","United States Stove - 5660E","United States Stove - 5710 ","United States Stove - KP60","United States Stove - GW1949","United States Stoves - 5520","United States Stove - KP130","Enerco Group - PSBF66W","LMF B-100","Ravelli - RV100 Classic","Ravelli - RV80","Enerco Group - PS130W","Sierra Products - EasyFire","Enerco Group - PS60W","Heat Tech - HTP 26 Bay","Heat Tech - HTP 26 Standard","LIA Pellet Stove","Monia 2.0","Sabrina 2.0","Enerco 20kw","Ravelli Roma","SBI Osburn","Thermorossi slim9","Thermorossi slim 11","SMG HP54","SMG HP55","SPA 3.4","SPA 4.5","SPA 5.2","Lamonox Jessica air","Laminox Jessica Natural","PAC True North 40i","Even Temp Element P","Paramax Rafael 55a","Thermorossi Pair11","Ravelli 120 touch","Thelin Company Gnome","Thelin Company Parlour 3000","US Stove 5780e","US Stove KP5513","PS20W","PS60W","PS130W","PSBF66W","Whitney","Meridian II"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary Table","index":0,"n_rows":106,"n_cols":11,"rows_kept":106,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"Tab #","Manufacturer","Model","Test Method","Preliminary","Final","AK List Status","Why"]
[null,null,null,1,{"$f":"'509 Fabrications-Optimum'!$B$2","v":"509 Fabrications, Inc."},{"$f":"'509 Fabrications-Optimum'!$B$3","v":"509-1 Optimum"},"Other (ATM)",{"$f":"'509 Fabrications-Optimum'!$B$4","v":"Requires a more thorough review"},{"$f":"'509 Fabrications-Optimum'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('509 Fabrications-Optimum'!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
["Start Sheet Number",6,null,2,{"$f":"'HHH-Accentra-2'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHH-Accentra-2'!$B$3","v":"Accentra-2"},"ASTM 2779",{"$f":"'HHH-Accentra-2'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHH-Accentra-2'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHH-Accentra-2'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR"}]
[null,null,null,3,{"$f":"'HHH-Accentra 52i-TC'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHH-Accentra 52i-TC'!$B$3","v":"Accentra 52i- TC"},"ASTM 2779",{"$f":"'HHH-Accentra 52i-TC'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHH-Accentra 52i-TC'!$B$6","v":"Pending - Minor"},"No Determination List",{"$f":" SUBSTITUTE('HHH-Accentra 52i-TC'!$I$6,\"Basis: \",\"\")","v":"MD, IR"}]
[null,null,null,4,{"$f":"'HHH-Allure 50'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHH-Allure 50'!$B$3","v":"Allure 50"},"ASTM 2779",{"$f":"'HHH-Allure 50'!$B$4","v":"Disapproved"},{"$f":"'HHH-Allure 50'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHH-Allure 50'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR"}]
[null,null,null,5,{"$f":"'US Stove 6041'!$B$2","v":"United States Stove Company"},{"$f":"'US Stove 6041'!$B$3","v":"6041, 6041I, and SP6000"},"ASTM 2779",{"$f":"'US Stove 6041'!$B$4","v":"Requires a more thorough review"},{"$f":"'US Stove 6041'!$B$6","v":"Pending - Minor"},"Approved List - Pending",{"$f":" SUBSTITUTE('US Stove 6041'!$I$6,\"Basis: \",\"\")","v":"MD, IR"}]
[null,null,null,6,{"$f":"'AES Baby'!$B$2","v":"American Energy Systems (AES)"},{"$f":"'AES Baby'!$B$3","v":"Magnum Baby Countryside"},"ASTM 2779",{"$f":"'AES Baby'!$B$4","v":"Disapproved"},{"$f":"'AES Baby'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('AES Baby'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,7,{"$f":"'AES 3500P '!$B$2","v":"American Energy Systems (AES)"},{"$f":"'AES 3500P '!$B$3","v":"3500P, 35001, and 3502"},"ASTM 2779",{"$f":"'AES 3500P '!$B$4","v":"Disapproved"},{"$f":"'AES 3500P '!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('AES 3500P '!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,8,{"$f":"'AES Little Rascal'!$B$2","v":"American Energy Systems (AES)"},{"$f":"'AES Little Rascal'!$B$3","v":"Little Rascal"},"ASTM 2779",{"$f":"'AES Little Rascal'!$B$4","v":"Disapproved"},{"$f":"'AES Little Rascal'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('AES Little Rascal'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,9,{"$f":"'APR 100'!$B$2","v":"APR Industries Ltd."},{"$f":"'APR 100'!$B$3","v":"Kozi 100 Free Standing and Insert and KSH 120"},"ASTM 2779",{"$f":"'APR 100'!$B$4","v":"Disapproved"},{"$f":"'APR 100'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('APR 100'!$I$6,\"Basis: \",\"\")","v":"M1, MD, IR, NR"}]
[null,null,null,10,{"$f":"'APR Baywin'!$B$2","v":"APR Industries Ltd."},{"$f":"'APR Baywin'!$B$3","v":"BayWin Free Standing and Insert"},"ASTM 2779",{"$f":"'APR Baywin'!$B$4","v":"Disapproved"},{"$f":"'APR Baywin'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('APR Baywin'!$I$6,\"Basis: \",\"\")","v":"M1, MD, IR, NR"}]
[null,null,null,11,{"$f":"'APR Previa'!$B$2","v":"APR Industries Ltd."},{"$f":"'APR Previa'!$B$3","v":"Previa"},"ASTM 2779",{"$f":"'APR Previa'!$B$4","v":"Disapproved"},{"$f":"'APR Previa'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('APR Previa'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,12,{"$f":"'EvenTemp Eclipse'!$B$2","v":"Even Temp, Inc."},{"$f":"'EvenTemp Eclipse'!$B$3","v":"Eclipse"},"ASTM 2779",{"$f":"'EvenTemp Eclipse'!$B$4","v":"Disapproved"},{"$f":"'EvenTemp Eclipse'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('EvenTemp Eclipse'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,13,{"$f":"'EvenTemp Ashby'!$B$2","v":"Even Temp, Inc."},{"$f":"'EvenTemp Ashby'!$B$3","v":"Ashby - P"},"ASTM 2779",{"$f":"'EvenTemp Ashby'!$B$4","v":"Disapproved"},{"$f":"'EvenTemp Ashby'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('EvenTemp Ashby'!$I$6,\"Basis: \",\"\")","v":"M1, MD, IR, NR"}]
[null,null,null,14,{"$f":"'EvenTemp Prescott EXP'!$B$2","v":"Even Temp, Inc."},{"$f":"'EvenTemp Prescott EXP'!$B$3","v":"Prescott EXP"},"ASTM 2779",{"$f":"'EvenTemp Prescott EXP'!$B$4","v":"Disapproved"},{"$f":"'EvenTemp Prescott EXP'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('EvenTemp Prescott EXP'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,15,{"$f":"'EvenTemp Hastings'!$B$2","v":"Even Temp, Inc."},{"$f":"'EvenTemp Hastings'!$B$3","v":"Hastings"},"ASTM 2779",{"$f":"'EvenTemp Hastings'!$B$4","v":"Disapproved"},{"$f":"'EvenTemp Hastings'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('EvenTemp Hastings'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,16,{"$f":"'HHT Santa FE-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Quadra fire"},{"$f":"'HHT Santa FE-C'!$B$3","v":"Santa Fe-C, Santa Fe I-C, Castile-C, Castile I-C"},"ASTM 2779",{"$f":"'HHT Santa FE-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Santa FE-C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT Santa FE-C'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,17,{"$f":"'HHT PP60-B'!$B$2","v":"Hearth and Home Technologies, LLC "},{"$f":"'HHT PP60-B'!$B$3","v":"Pel-Pro PP60-B and Pleasant Hearth PH35PS-B"},"ASTM 2779",{"$f":"'HHT PP60-B'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT PP60-B'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT PP60-B'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,18,{"$f":"'HHT PP70'!$B$2","v":"Hearth and Home Technologies, LLC  "},{"$f":"'HHT PP70'!$B$3","v":"Pelpro PP70"},"ASTM 2779",{"$f":"'HHT PP70'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT PP70'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT PP70'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,19,{"$f":"'HHT PPC90'!$B$2","v":"Hearth and Home Technologies, LLC "},{"$f":"'HHT PPC90'!$B$3","v":"PelPro PPC90, PelPro TSC90, and Pleasant Hearth PHC90"},"ASTM 2779",{"$f":"'HHT PPC90'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT PPC90'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT PPC90'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,20,{"$f":"'HHT PP130'!$B$2","v":"Hearth and Home Technologies, LLC dba Pelpro"},{"$f":"'HHT PP130'!$B$3","v":"PP130-B"},"ASTM 2779",{"$f":"'HHT PP130'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT PP130'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT PP130'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR"}]
[null,null,null,21,{"$f":"'HHT Classic Bay 1200 iC'!$B$2","v":"Hearth and Home Technologies, LLC dba Quadra fire"},{"$f":"'HHT Classic Bay 1200 iC'!$B$3","v":"Classic Bay 1200 i-C"},"ASTM 2779",{"$f":"'HHT Classic Bay 1200 iC'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Classic Bay 1200 iC'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT Classic Bay 1200 iC'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,22,{"$f":"'HHT Classic Bay 1200C'!$B$2","v":"Hearth and Home Technologies, LLC dba Quadra fire"},{"$f":"'HHT Classic Bay 1200C'!$B$3","v":"Classic Bay 1200 -C "},"ASTM 2779",{"$f":"'HHT Classic Bay 1200C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Classic Bay 1200C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT Classic Bay 1200C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,23,{"$f":"'HHT PS35-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Heatilator EcoChoice"},{"$f":"'HHT PS35-C'!$B$3","v":"PS35-C, ECO Choice PS35-C, Quadra-Fire PS35-C"},"ASTM 2779",{"$f":"'HHT PS35-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT PS35-C'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT PS35-C'!$I$6,\"Basis: \",\"\")","v":"IDU, IR"}]
[null,null,null,24,{"$f":"'HHT P43-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Pelpro"},{"$f":"'HHT P43-C'!$B$3","v":"P43-C"},"ASTM 2779",{"$f":"'HHT P43-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT P43-C'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT P43-C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,25,{"$f":"'HHT CAB50-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Heatilator EcoChoice"},{"$f":"'HHT CAB50-C'!$B$3","v":"ECO CAB50-C and ECO PS50-C"},"ASTM 2779",{"$f":"'HHT CAB50-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT CAB50-C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT CAB50-C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR"}]
[null,null,null,26,{"$f":"'HHT P61-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT P61-C'!$B$3","v":"P61-C"},"ASTM 2779",{"$f":"'HHT P61-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT P61-C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT P61-C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU,  IR, NR"}]
[null,null,null,27,{"$f":"'HHT P68-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT P68-C'!$B$3","v":"P68-C"},"ASTM 2779",{"$f":"'HHT P68-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT P68-C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT P68-C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU,  IR, NR"}]
[null,null,null,28,{"$f":"'HHT Absolute 43-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT Absolute 43-C'!$B$3","v":"Absolute 43-C"},"ASTM 2779",{"$f":"'HHT Absolute 43-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Absolute 43-C'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT Absolute 43-C'!$I$6,\"Basis: \",\"\")","v":"MD, IR"}]
[null,null,null,29,{"$f":"'HHT Absolute 63'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT Absolute 63'!$B$3","v":"Absolute 63"},"ASTM 2779",{"$f":"'HHT Absolute 63'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Absolute 63'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT Absolute 63'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,30,{"$f":"'HHT Mt. Vernon E2-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Quadra fire"},{"$f":"'HHT Mt. Vernon E2-C'!$B$3","v":"Quadra Fire Mount Vernon E2-C, Quadra Fire Mount Vernon E2-C Insert, Trekker, Trekker Insert"},"ASTM 2779",{"$f":"'HHT Mt. Vernon E2-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT Mt. Vernon E2-C'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT Mt. Vernon E2-C'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, NR, IR"}]
[null,null,null,31,{"$f":"'HHT XXV-TC'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT XXV-TC'!$B$3","v":"XXV-TC"},"ASTM 2779",{"$f":"'HHT XXV-TC'!$B$4","v":"Disapproved"},{"$f":"'HHT XXV-TC'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('HHT XXV-TC'!$I$6,\"Basis: \",\"\")","v":"ES1, MD, IR, NR"}]
[null,null,null,32,{"$f":"'HHT P35i-C'!$B$2","v":"Hearth and Home Technologies, LLC dba Harman"},{"$f":"'HHT P35i-C'!$B$3","v":"P35i-C"},"ASTM 2779",{"$f":"'HHT P35i-C'!$B$4","v":"Requires a more thorough review"},{"$f":"'HHT P35i-C'!$B$6","v":"Pending - Minor"},"Approved List - Pending",{"$f":" SUBSTITUTE('HHT P35i-C'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,33,{"$f":"'HHT PH50PS-B'!$B$2","v":"Hearth and Home Technologies, LLC dba Pleasant Hearth"},{"$f":"'HHT PH50PS-B'!$B$3","v":"PH50PS-B, PH50CABPS-B"},"ASTM 2779",{"$f":"'HHT PH50PS-B'!$B$4","v":"Disapproved"},{"$f":"'HHT PH50PS-B'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HHT PH50PS-B'!$I$6,\"Basis: \",\"\")","v":"IR,  NR"}]
[null,null,null,34,{"$f":"'Castle Serenity'!$B$2","v":"ARDISAM, Inc."},{"$f":"'Castle Serenity'!$B$3","v":"Serenity Castle"},"ASTM 2779",{"$f":"'Castle Serenity'!$B$4","v":"Requires a more thorough review"},{"$f":"'Castle Serenity'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Castle Serenity'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,35,{"$f":"'Englander CAB80'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englander CAB80'!$B$3","v":"25CAB80, 55-SHPCAB80, 55-TRPCAB80, 55-SHPCAB80S, 55-RPCAB80S"},"ASTM 2779",{"$f":"'Englander CAB80'!$B$4","v":"Disapproved"},{"$f":"'Englander CAB80'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Englander CAB80'!$I$6,\"Basis: \",\"\")","v":"NR, IR"}]
[null,null,null,36,{"$f":"'Englander CB120'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englander CB120'!$B$3","v":"25-CB120, 55-SHPCB120, 55-TRPCB120"},"ASTM 2779",{"$f":"'Englander CB120'!$B$4","v":"Disapproved"},{"$f":"'Englander CB120'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Englander CB120'!$I$6,\"Basis: \",\"\")","v":"IDU"}]
[null,null,null,37,{"$f":"'Englander 25-CB PAH'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englander 25-CB PAH'!$B$3","v":"25-CBPAH, 55-SHPCBPAH, 55-TRCBPAH"},"ASTM 2779",{"$f":"'Englander 25-CB PAH'!$B$4","v":"Requires a more thorough review"},{"$f":"'Englander 25-CB PAH'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Englander 25-CB PAH'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,38,{"$f":"'Englanders 25-CBEP'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englanders 25-CBEP'!$B$3","v":"25-CBEP, 55-SHPCBEP, 55-TRPCBEP"},"ASTM 2779",{"$f":"'Englanders 25-CBEP'!$B$4","v":"Requires a more thorough review"},{"$f":"'Englanders 25-CBEP'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Englanders 25-CBEP'!$I$6,\"Basis: \",\"\")","v":"NR, IR"}]
[null,null,null,39,{"$f":"'Englander 25-PDVC'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englander 25-PDVC'!$B$3","v":"25-PDVC, 25-PDVCH, 55-SHP10, 55-SHP10L, and 55-TRP10"},"ASTM 2779",{"$f":"'Englander 25-PDVC'!$B$4","v":"Requires a more thorough review"},{"$f":"'Englander 25-PDVC'!$B$6","v":"Pending - Major"},"Disapproved List",{"$f":" SUBSTITUTE('Englander 25-PDVC'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,40,{"$f":"'Englander 25-SSP'!$B$2","v":"England Stove Works Inc"},{"$f":"'Englander 25-SSP'!$B$3","v":"25-SSP01,25-SSP01S,55-SHSSP01,55SHSSP01S, 55-TRSSP01, and 55TRSSP01S"},"ASTM 2779",{"$f":"'Englander 25-SSP'!$B$4","v":"Requires a more thorough review"},{"$f":"'Englander 25-SSP'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Englander 25-SSP'!$I$6,\"Basis: \",\"\")","v":"M1, MD, IR"}]
[null,null,null,41,{"$f":"'Enviro M55'!$B$2","v":"Sherwood Industries Ltd dba Enviro"},{"$f":"'Enviro M55'!$B$3","v":"M55 FS, M55C-FPI and Regency Greenfire – GC60, GCI60"},"ASTM 2779",{"$f":"'Enviro M55'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enviro M55'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Enviro M55'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR, NR"}]
[null,null,null,42,{"$f":"'Enviro Mini P3'!$B$2","v":"Sherwood Industries Ltd dba Enviro"},{"$f":"'Enviro Mini P3'!$B$3","v":"Mini, P3 and Regency Greenfire – GF40"},"ASTM 2779",{"$f":"'Enviro Mini P3'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enviro Mini P3'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Enviro Mini P3'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,43,{"$f":"'Enviro Meridian & GF55'!$B$2","v":"Sherwood Industries Ltd dba Enviro"},{"$f":"'Enviro Meridian & GF55'!$B$3","v":"Meridian-1, FPI, Cast Iron, GF55, GF155"},"ASTM 2779",{"$f":"'Enviro Meridian & GF55'!$B$4","v":"Disapproved"},{"$f":"'Enviro Meridian & GF55'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Enviro Meridian & GF55'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,44,{"$f":"'Enviro MAXX-1'!$B$2","v":"Sherwood Industries Ltd dba Enviro"},{"$f":"'Enviro MAXX-1'!$B$3","v":"MAXX-1"},"ASTM 2779",{"$f":"'Enviro MAXX-1'!$B$4","v":"Disapproved"},{"$f":"'Enviro MAXX-1'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Enviro MAXX-1'!$I$6,\"Basis: \",\"\")","v":"ES1, MD, IDU, IR, NR"}]
[null,null,null,45,{"$f":"'HRSW Chatham'!$B$2","v":"Sherwood Industries Ltd dba Hudson River Stove Works"},{"$f":"'HRSW Chatham'!$B$3","v":"EF2-1, Chatham-1, Davenport-1, and Kinderhook-1"},"ASTM 2779",{"$f":"'HRSW Chatham'!$B$4","v":"Disapproved"},{"$f":"'HRSW Chatham'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('HRSW Chatham'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,46,{"$f":"'SMG HP21'!$B$2","v":"SMG Hearth & Home dba Comfortbilt"},{"$f":"'SMG HP21'!$B$3","v":"HP21"},"ASTM 2779",{"$f":"'SMG HP21'!$B$4","v":"Disapproved"},{"$f":"'SMG HP21'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('SMG HP21'!$I$6,\"Basis: \",\"\")","v":"NR, IR"}]
[null,null,null,47,{"$f":"'SMG HP22'!$B$2","v":"SMG Hearth & Home dba Comfortbilt "},{"$f":"'SMG HP22'!$B$3","v":" ComfortBilt HP22N, HP22, and HP22i Insert"},"ASTM 2779",{"$f":"'SMG HP22'!$B$4","v":"Disapproved"},{"$f":"'SMG HP22'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('SMG HP22'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,48,{"$f":"'SMG HP61'!$B$2","v":"SMG Hearth & Home dba Comfortbilt"},{"$f":"'SMG HP61'!$B$3","v":"HP61"},"ASTM 2779",{"$f":"'SMG HP61'!$B$4","v":"Disapproved"},{"$f":"'SMG HP61'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('SMG HP61'!$I$6,\"Basis: \",\"\")","v":"NR, IR"}]
[null,null,null,49,{"$f":"'Travis Fox Fire'!$B$2","v":"Travis Industries, Inc"},{"$f":"'Travis Fox Fire'!$B$3","v":"Fox Fire"},"ASTM 2779",{"$f":"'Travis Fox Fire'!$B$4","v":"Requires a more thorough review"},{"$f":"'Travis Fox Fire'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Travis Fox Fire'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,50,{"$f":"'Travis Deerfield'!$B$2","v":"Travis Industries, Inc"},{"$f":"'Travis Deerfield'!$B$3","v":"Deerfield"},"ASTM 2779",{"$f":"'Travis Deerfield'!$B$4","v":"Requires a more thorough review"},{"$f":"'Travis Deerfield'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Travis Deerfield'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,51,{"$f":"'Travis AGP Insert'!$B$2","v":"Travis Industries, Inc"},{"$f":"'Travis AGP Insert'!$B$3","v":"AGP Insert"},"ASTM 2779",{"$f":"'Travis AGP Insert'!$B$4","v":"Requires a more thorough review"},{"$f":"'Travis AGP Insert'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Travis AGP Insert'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,52,{"$f":"'Travis AGP PS'!$B$2","v":"Travis Industries, Inc"},{"$f":"'Travis AGP PS'!$B$3","v":"AGP PS"},"ASTM 2779",{"$f":"'Travis AGP PS'!$B$4","v":"Disapproved"},{"$f":"'Travis AGP PS'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Travis AGP PS'!$I$6,\"Basis: \",\"\")","v":"ES1, IR"}]
[null,null,null,53,{"$f":"'True North 40'!$B$2","v":"Pacific Energy Fireplace Products Limited dba True North"},{"$f":"'True North 40'!$B$3","v":"TN40"},"ASTM 2779",{"$f":"'True North 40'!$B$4","v":"Requires a more thorough review"},{"$f":"'True North 40'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('True North 40'!$I$6,\"Basis: \",\"\")","v":"M1, IR, NR"}]
[null,null,null,54,{"$f":"'USSC 4840'!$B$2","v":"United States Stove Company"},{"$f":"'USSC 4840'!$B$3","v":"4840, KP500, AP5000"},"ASTM 2779",{"$f":"'USSC 4840'!$B$4","v":"Requires a more thorough review"},{"$f":"'USSC 4840'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('USSC 4840'!$I$6,\"Basis: \",\"\")","v":"MD, IR "}]
[null,null,null,55,{"$f":"'USSC SP24'!$B$2","v":"United States Stove Company dba Breckwell"},{"$f":"'USSC SP24'!$B$3","v":"SP22(i), SP23(i), SP24(i),\nSP2000(i), AP2000(i), SP2700, SP4000,\nSPC4000, APC4000 and 5040(i)"},"ASTM 2779",{"$f":"'USSC SP24'!$B$4","v":"Requires a more thorough review"},{"$f":"'USSC SP24'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('USSC SP24'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,56,{"$f":"'USSC SP2047'!$B$2","v":"United States Stove Company dba Breckwell"},{"$f":"'USSC SP2047'!$B$3","v":"SP2047, GW7400"},"Other (ATM)",{"$f":"'USSC SP2047'!$B$4","v":"Requires a more thorough review"},{"$f":"'USSC SP2047'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('USSC SP2047'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,57,{"$f":"'USSC SP1000'!$B$2","v":"United States Stove Company dba Breckwell"},{"$f":"'USSC SP1000'!$B$3","v":"SP1000"},"ASTM 2779",{"$f":"'USSC SP1000'!$B$4","v":"Requires a more thorough review"},{"$f":"'USSC SP1000'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('USSC SP1000'!$I$6,\"Basis: \",\"\")","v":"MD, IDU, IR"}]
[null,null,null,58,{"$f":"'United States Stove-5780 Series'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove-5780 Series'!$B$3","v":"5780, AP5780, VG5780, SP5780, and SP58"},"ASTM 2779",{"$f":"'United States Stove-5780 Series'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove-5780 Series'!$B$6","v":"Pending - Minor"},"No Determination List",{"$f":" SUBSTITUTE('United States Stove-5780 Series'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,59,{"$f":"'United States Stove - 5770'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - 5770'!$B$3","v":"5770, 5770i, VG5770, VG5770i, AP5770, AP5770i, DNMP577, DNMP577(i), 5790, VG5790, AP5790, and DNMP579 "},"ASTM 2779",{"$f":"'United States Stove - 5770'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - 5770'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('United States Stove - 5770'!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
[null,null,null,60,{"$f":"'United States Stove - 5660E'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - 5660E'!$B$3","v":"5660E, AP5660, AP5660L, AP5660PE and DNMP566"},"ASTM 2779",{"$f":"'United States Stove - 5660E'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - 5660E'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('United States Stove - 5660E'!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
[null,null,null,61,{"$f":"'United States Stove - 5710 '!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - 5710 '!$B$3","v":"5710, AP5710, VG5710, 5501S, AP5501S, VG5501S"},"ASTM 2779",{"$f":"'United States Stove - 5710 '!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - 5710 '!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('United States Stove - 5710 '!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
[null,null,null,62,{"$f":"'United States Stove - KP60'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - KP60'!$B$3","v":"King KP60, Ashley AP60, Vogelzang VG60"},"ASTM 2779",{"$f":"'United States Stove - KP60'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - KP60'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('United States Stove - KP60'!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
[null,null,null,63,{"$f":"'United States Stove - GW1949'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - GW1949'!$B$3","v":"GW1949, AP77, SW1117"},"ASTM 2779",{"$f":"'United States Stove - GW1949'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - GW1949'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('United States Stove - GW1949'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,64,{"$f":"'United States Stoves - 5520'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stoves - 5520'!$B$3","v":5520},"ASTM 2779",{"$f":"'United States Stoves - 5520'!$B$4","v":"Disapproved"},{"$f":"'United States Stoves - 5520'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('United States Stoves - 5520'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,65,{"$f":"'United States Stove - KP130'!$B$2","v":"United States Stove Company"},{"$f":"'United States Stove - KP130'!$B$3","v":"KP130, AP130, VG130, 5502M, 5500, 5500M, and 5500XL"},"ASTM 2779",{"$f":"'United States Stove - KP130'!$B$4","v":"Requires a more thorough review"},{"$f":"'United States Stove - KP130'!$B$6","v":"Pending - Minor"},"Approved List - Pending",{"$f":" SUBSTITUTE('United States Stove - KP130'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,66,{"$f":"'Enerco Group - PSBF66W'!$B$2","v":"Enerco Group, Inc."},{"$f":"'Enerco Group - PSBF66W'!$B$3","v":"PSBF66W"},"ASTM 2779",{"$f":"'Enerco Group - PSBF66W'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enerco Group - PSBF66W'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Enerco Group - PSBF66W'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,67,{"$f":"'LMF B-100'!$B$2","v":"LMF Manufacturing Ltd dba America's Heat"},{"$f":"'LMF B-100'!$B$3","v":"America's Heat B-100"},"ASTM 2779",{"$f":"'LMF B-100'!$B$4","v":"Requires a more thorough review"},{"$f":"'LMF B-100'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('LMF B-100'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,68,{"$f":"'Ravelli - RV100 Classic'!$B$2","v":"Ravelli "},{"$f":"'Ravelli - RV100 Classic'!$B$3","v":"RV100 Classic"},"ASTM 2779",{"$f":"'Ravelli - RV100 Classic'!$B$4","v":"Disapproved"},{"$f":"'Ravelli - RV100 Classic'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Ravelli - RV100 Classic'!$I$6,\"Basis: \",\"\")","v":"IDU, IR, NR"}]
[null,null,null,69,{"$f":"'Ravelli - RV80'!$B$2","v":"Ravelli"},{"$f":"'Ravelli - RV80'!$B$3","v":"Monica 2015, Francesca 2015, RV80 CERAMICA"},"ASTM 2779",{"$f":"'Ravelli - RV80'!$B$4","v":"Requires a more thorough review"},{"$f":"'Ravelli - RV80'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Ravelli - RV80'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,70,{"$f":"'Enerco Group - PS130W'!$B$2","v":"Enerco Group, Inc."},{"$f":"'Enerco Group - PS130W'!$B$3","v":"PS130W"},"ASTM 2779",{"$f":"'Enerco Group - PS130W'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enerco Group - PS130W'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Enerco Group - PS130W'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,71,{"$f":"'Sierra Products - EasyFire'!$B$2","v":"Sierra Product, Inc."},{"$f":"'Sierra Products - EasyFire'!$B$3","v":"EasyFire Pellet Stove, EF3801, EF5001, EF4001"},"ASTM 2779",{"$f":"'Sierra Products - EasyFire'!$B$4","v":"Requires a more thorough review"},{"$f":"'Sierra Products - EasyFire'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Sierra Products - EasyFire'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,72,{"$f":"'Enerco Group - PS60W'!$B$2","v":"Enerco Group, Inc."},{"$f":"'Enerco Group - PS60W'!$B$3","v":"PS60W"},"ASTM 2779",{"$f":"'Enerco Group - PS60W'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enerco Group - PS60W'!$B$6","v":"Pending - Major"},"Approved List - Pending",{"$f":" SUBSTITUTE('Enerco Group - PS60W'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,73,{"$f":"'Heat Tech - HTP 26 Bay'!$B$2","v":"Heat Tech Industries, LLC."},{"$f":"'Heat Tech - HTP 26 Bay'!$B$3","v":"HTP 26 Bay, HTP26 Bay Pedestal/Insert"},"ASTM 2779",{"$f":"'Heat Tech - HTP 26 Bay'!$B$4","v":"Requires a more thorough review"},{"$f":"'Heat Tech - HTP 26 Bay'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Heat Tech - HTP 26 Bay'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,74,{"$f":"'Heat Tech - HTP 26 Standard'!$B$2","v":"Heat Tech Industries, LLC."},{"$f":"'Heat Tech - HTP 26 Standard'!$B$3","v":"HTP 26 Standard"},"ASTM 2779",{"$f":"'Heat Tech - HTP 26 Standard'!$B$4","v":"Requires a more thorough review"},{"$f":"'Heat Tech - HTP 26 Standard'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Heat Tech - HTP 26 Standard'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,75,{"$f":"'LIA Pellet Stove'!$B$2","v":"Gruppo Piazzetta S.P.A."},{"$f":"'LIA Pellet Stove'!$B$3","v":"LIA"},"ASTM 2779",{"$f":"'LIA Pellet Stove'!$B$4","v":"Requires a more thorough review"},{"$f":"'LIA Pellet Stove'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('LIA Pellet Stove'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,76,{"$f":"'Monia 2.0'!$B$2","v":"Gruppo Piazzetta S.P.A."},{"$f":"'Monia 2.0'!$B$3","v":"Monia 2.0, Marcella 2.0, Maya 2.0, Monica 2.0"},"ASTM 2779",{"$f":"'Monia 2.0'!$B$4","v":"Disapproved"},{"$f":"'Monia 2.0'!$B$6","v":"Disapproved"},"No Determination List",{"$f":" SUBSTITUTE('Monia 2.0'!$I$6,\"Basis: \",\"\")","v":"M1, MD, IR, NR"}]
[null,null,null,77,{"$f":"'Sabrina 2.0'!$B$2","v":"Gruppo Piazzetta S.P.A."},{"$f":"'Sabrina 2.0'!$B$3","v":"Sabrina 2.0, Sally 2.0, Solange 2.0, Sveva 2.0"},"ASTM 2779",{"$f":"'Sabrina 2.0'!$B$4","v":"Requires a more thorough review"},{"$f":"'Sabrina 2.0'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Sabrina 2.0'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,78,{"$f":"'Enerco 20kw'!$B$2","v":"Enerco"},{"$f":"'Enerco 20kw'!$B$3","v":"Cleveland Iron Works Model PS20W"},"ASTM 2779",{"$f":"'Enerco 20kw'!$B$4","v":"Requires a more thorough review"},{"$f":"'Enerco 20kw'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Enerco 20kw'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,79,{"$f":"'Ravelli Roma'!$B$2","v":"Ravelli"},{"$f":"'Ravelli Roma'!$B$3","v":"Roma"},"ASTM 2779",{"$f":"'Ravelli Roma'!$B$4","v":0},{"$f":"'Ravelli Roma'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Ravelli Roma'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,80,{"$f":"'SBI Osburn'!$B$2","v":"Stove Builder International"},{"$f":"'SBI Osburn'!$B$3","v":"Osburn 2500, ECO-55"},"ASTM 2779",{"$f":"'SBI Osburn'!$B$4","v":0},{"$f":"'SBI Osburn'!$B$6","v":"Pending - Minor"},"No Determination List",{"$f":" SUBSTITUTE('SBI Osburn'!$I$6,\"Basis: \",\"\")","v":"MD, IR"}]
[null,null,null,81,{"$f":"'Thermorossi slim9'!$B$2","v":"Thermorossi"},{"$f":"'Thermorossi slim9'!$B$3","v":"SlimQuatro  9 "},"ASTM 2779",{"$f":"'Thermorossi slim9'!$B$4","v":0},{"$f":"'Thermorossi slim9'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Thermorossi slim9'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,82,{"$f":"'Thermorossi slim 11'!$B$2","v":"Thermorossi"},{"$f":"'Thermorossi slim 11'!$B$3","v":"Slimquadro 11"},"ASTM 2779",{"$f":"'Thermorossi slim 11'!$B$4","v":0},{"$f":"'Thermorossi slim 11'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Thermorossi slim 11'!$I$6,\"Basis: \",\"\")","v":"IR, NR"}]
[null,null,null,83,{"$f":"'SMG HP54'!$B$2","v":"SMG Hearth & Home LLC"},{"$f":"'SMG HP54'!$B$3","v":"HP54"},"ASTM 2779",{"$f":"'SMG HP54'!$B$4","v":0},{"$f":"'SMG HP54'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('SMG HP54'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,84,{"$f":"'SMG HP55'!$B$2","v":"SMG Hearth & Home LLC"},{"$f":"'SMG HP55'!$B$3","v":"HP55"},"ASTM 2779",{"$f":"'SMG HP55'!$B$4","v":0},{"$f":"'SMG HP55'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('SMG HP55'!$I$6,\"Basis: \",\"\")","v":"MD, IR, NR"}]
[null,null,null,85,{"$f":"'SPA 3.4'!$B$2","v":"Extraflame S.P.A."},{"$f":"'SPA 3.4'!$B$3","v":"V3.4"},"Not reported",{"$f":"'SPA 3.4'!$B$4","v":0},{"$f":"'SPA 3.4'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('SPA 3.4'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,86,{"$f":"'SPA 4.5'!$B$2","v":"Extraflame S.P.A."},{"$f":"'SPA 4.5'!$B$3","v":"V4.5"},"Not reported",{"$f":"'SPA 4.5'!$B$4","v":0},{"$f":"'SPA 4.5'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('SPA 4.5'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,87,{"$f":"'SPA 5.2'!$B$2","v":"Extraflame S.P.A."},{"$f":"'SPA 5.2'!$B$3","v":"V5.2"},"Not reported",{"$f":"'SPA 5.2'!$B$4","v":0},{"$f":"'SPA 5.2'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('SPA 5.2'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,88,{"$f":"'Lamonox Jessica air'!$B$2","v":"Laminox"},{"$f":"'Lamonox Jessica air'!$B$3","v":"Jessica 11air and Veronica 11 air"},"Not reported",{"$f":"'Lamonox Jessica air'!$B$4","v":0},{"$f":"'Lamonox Jessica air'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Lamonox Jessica air'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,89,{"$f":"'Laminox Jessica Natural'!$B$2","v":"Laminox"},{"$f":"'Laminox Jessica Natural'!$B$3","v":"Jessica Natural and Veronica Natural"},"Not reported",{"$f":"'Laminox Jessica Natural'!$B$4","v":0},{"$f":"'Laminox Jessica Natural'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Laminox Jessica Natural'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,90,{"$f":"'PAC True North 40i'!$B$2","v":"Pacific Energy Fireplace Products Limited dba True North"},{"$f":"'PAC True North 40i'!$B$3","v":"True North 40 Insert"},"Not reported",{"$f":"'PAC True North 40i'!$B$4","v":0},{"$f":"'PAC True North 40i'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('PAC True North 40i'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,91,{"$f":"'Even Temp Element P'!$B$2","v":"Even Temp"},{"$f":"'Even Temp Element P'!$B$3","v":"Element Model P"},"Not reported",{"$f":"'Even Temp Element P'!$B$4","v":0},{"$f":"'Even Temp Element P'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Even Temp Element P'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,92,{"$f":"'Paramax Rafael 55a'!$B$2","v":"Paramax International"},{"$f":"'Paramax Rafael 55a'!$B$3","v":"Rafael 55a, Europa 75a"},"Not reported",{"$f":"'Paramax Rafael 55a'!$B$4","v":0},{"$f":"'Paramax Rafael 55a'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Paramax Rafael 55a'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,93,{"$f":"'Thermorossi Pair11'!$B$2","v":"Thermorossi"},{"$f":"'Thermorossi Pair11'!$B$3","v":"Pair 11, Pair11Plus"},"Not reported",{"$f":"'Thermorossi Pair11'!$B$4","v":0},{"$f":"'Thermorossi Pair11'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Thermorossi Pair11'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,94,{"$f":"'Ravelli 120 touch'!$B$2","v":"Ravelli"},{"$f":"'Ravelli 120 touch'!$B$3","v":"RV120Touch"},"ASTM 2779",{"$f":"'Ravelli 120 touch'!$B$4","v":0},{"$f":"'Ravelli 120 touch'!$B$6","v":"Pending - Major"},"No Determination List",{"$f":" SUBSTITUTE('Ravelli 120 touch'!$I$6,\"Basis: \",\"\")","v":"IR"}]
[null,null,null,95,{"$f":"'Thelin Company Gnome'!$B$2","v":"Thelin Company"},{"$f":"'Thelin Company Gnome'!$B$3","v":"Gnome"},"Not reported",{"$f":"'Thelin Company Gnome'!$B$4","v":0},{"$f":"'Thelin Company Gnome'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Thelin Company Gnome'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,96,{"$f":"'Thelin Company Parlour 3000'!$B$2","v":"Thelin Company"},{"$f":"'Thelin Company Parlour 3000'!$B$3","v":"Parlour 3000"},"Not reported",{"$f":"'Thelin Company Parlour 3000'!$B$4","v":0},{"$f":"'Thelin Company Parlour 3000'!$B$6","v":"Disapproved"},"Disapproved List",{"$f":" SUBSTITUTE('Thelin Company Parlour 3000'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,97,{"$f":"'US Stove 5780e'!$B$2","v":"United States Stove Company"},{"$f":"'US Stove 5780e'!$B$3","v":"5780e,  AP5780E, VG5780E, \nSP5780E, SP58E"},"ASTM 2779",{"$f":"'US Stove 5780e'!$B$4","v":0},{"$f":"'US Stove 5780e'!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE('US Stove 5780e'!$I$6,\"Basis: \",\"\")","v":"NTR"}]
[null,null,null,98,{"$f":"'US Stove KP5513'!$B$2","v":"United States Stove Company "},{"$f":"'US Stove KP5513'!$B$3","v":"KP5513, KP5513-P, KP5513-L, \nUS5513, US5513-P, US5513-L, AP5613, \nAP5613-P, AP5613-L, VG5713, \nVG5713-P, VG5713-L, Little E (SP500), \n5501S-XH"},"ASTM 2779",{"$f":"'US Stove KP5513'!$B$4","v":0},{"$f":"'US Stove KP5513'!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE('US Stove KP5513'!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,99,{"$f":"PS20W!$B$2","v":"Enerco Group Inc"},{"$f":"PS20W!$B$3","v":"PS20W, PS20WTS, C30XL, H30XL, J30XL, N30XL"},"ASTM 2779",{"$f":"PS20W!$B$4","v":0},{"$f":"PS20W!$B$6","v":0},"Disapproved List",{"$f":" SUBSTITUTE(PS20W!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,100,{"$f":"PS60W!$B$2","v":"Enerco Group Inc"},{"$f":"PS60W!$B$3","v":"PS60W, PS60WTS, C80XL, H80XL, J80XL, N80XL"},"ASTM 2779",{"$f":"PS60W!$B$4","v":0},{"$f":"PS60W!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE(PS60W!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,101,{"$f":"PS130W!$B$2","v":"Enerco Group Inc"},{"$f":"PS130W!$B$3","v":"PS130W, PS130WTS, C140XL, H140XL, J140XL, N140XL"},"ASTM 2779",{"$f":"PS130W!$B$4","v":0},{"$f":"PS130W!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE(PS130W!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,102,{"$f":"PSBF66W!$B$2","v":"Enerco Group Inc."},{"$f":"PSBF66W!$B$3","v":"PSBF66W, PSBF66WTS, C3W80XL, H3W80XL, J3W80XL, N3W80XL"},"ASTM 2779",{"$f":"PSBF66W!$B$4","v":0},{"$f":"PSBF66W!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE(PSBF66W!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,103,{"$f":"Whitney!$B$2","v":"Sun Mountain Stove Works Inc"},{"$f":"Whitney!$B$3","v":"Whitney"},"ASTM 2779",{"$f":"Whitney!$B$4","v":0},{"$f":"Whitney!$B$6","v":0},"No Determination List",{"$f":" SUBSTITUTE(Whitney!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,104,{"$f":"'Meridian II'!$B$2","v":"Sherwood Industries Ltd."},{"$f":"'Meridian II'!$B$3","v":"Enviro Meridian-2, Meridian FPI-2, Meridian Cast Iron-2, Regency Greenfire – GF55-2, GFI55-2"},0,{"$f":"'Meridian II'!$B$4","v":0},{"$f":"'Meridian II'!$B$6","v":0},"Disapproved List",{"$f":" SUBSTITUTE('Meridian II'!$I$6,\"Basis: \",\"\")","v":""}]
[null,null,null,105,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},0,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},"Disapproved List",{"$f":" SUBSTITUTE(#REF!,\"Basis: \",\"\")","v":{"$error":"#REF!"}}]

{"sheet":"509 Fabrications-Optimum","index":1,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","509 Fabrications, Inc.",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","509 Fabrications, Inc.",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","509 Fabrications, Inc.",null,null,null,null,null,null,"2021-03-31"]
["Model","509-1 Optimum",null,null,null,null,null,null,null,null,null,"Model","509-1 Optimum",null,null,null,null,null,null,"No date - est before 2/16",null,null,"Model","509-1 Optimum"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",8,"Orange flags",null,9,"Yellow flags",null,6,null,null,null,"Red flags",8,"Orange flags",null,9,"Yellow flags",null,6,null,null,null,"Red flags",8,"Orange flags",null,9,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Other (ATM)",null,null,null,null,null,null,"ATM - R1 was 2779, R2 ATM changed order of burn phases",null,null,"Test method","Other (ATM)",null,null,null,null,null,null,"ATM - R1 was 2779, R2 ATM changed order of burn phases",null,null,"Test method","Other (ATM)",null,null,null,null,null,null,"ATM - R1 was 2779, R2 ATM changed order of burn phases"]
["Test Lab","OMNI",null,null,null,null,null,null,"originally tested by myren consulting",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"originally tested by myren consulting",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"originally tested by myren consulting"]
["Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI"]
["Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES\r (Jared Sorenson & Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES\r (Jared Sorenson & Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES\n (Jared Sorenson & Sebastian Button)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.5,null,"PM Highest 1-hr (g/hr)",null,null,1.52,null,null,null,null,"Overall PM emissions (g/hr)",1.5,null,"PM Highest 1-hr (g/hr)",null,null,1.52,null,null,null,null,"Overall PM emissions (g/hr)",1.5,null,"PM Highest 1-hr (g/hr)",null,null,1.52]
["Overall HHV efficiency (%)",78.8,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",78.8,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",78.8]
["Overall heat output (Btu/hr)",25878,null,null,null,null,null,null,40000,null,null,"Overall heat output (Btu/hr)",25878,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",25878]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.5899999999999999},null,"Overall CO (g/min)",null,null,2.6499999999999999E-2,null,"co g/min not reported in report ",null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":1.5899999999999999},null,"Overall CO (g/min)",null,null,2.6499999999999999E-2,null,"co g/min not reported in report",null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":1.5899999999999999},null,"Overall CO (g/min)",null,null,2.6499999999999999E-2,null,"co g/min not reported in report"]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"completed 12/28/2016 through 1/1/17",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"completed 12/28/2016 through 1/1/17",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"completed 12/28/2016 through 1/1/17"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Aging data include in report on page 77. Included required information. Only 27 of the 51 hours are within (+/-0.5kg/hr) of average medium burn rate.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Aging data include in report on page 77. Included required information. Only 27 of the 51 hours are within (+/-0.5kg/hr) of average medium burn rate.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Aging data include in report on page 77. Included required information. Only 27 of the 51 hours are within (+/-0.5kg/hr) of average medium burn rate."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that in the test report #1 (4/24/2017), all the test run was appropriate ",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that in the test report #1 (4/24/2017), all the test run was appropriate "]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that the test report #1 (4/24/2017), the rest run was valid, no specific language located in the report.",null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that the test report #1 (4/24/2017), the rest run was valid, no specific language located in the report."]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that in the test report #1 (4/24/2017), there were test run anomalies, no specific language located in the report.",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that in the test report #1 (4/24/2017), there were test run anomalies, no specific language located in the report."]
["Doc. of run burn rates","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that \"The test run identified as Test Run # 2 in Test Report #2, dated 9/21/2017, was conducted following all of the criteria found in the relevant test methods and specified in the letters received from EPA.\" , no specific language located in the report.",null,null,"Doc. of run burn rates","Not reported",null,null,null,null,null,null,"Myren consulting, Inc., in their response, dated 1/1/2021, stated that \"The test run identified as Test Run # 2 in Test Report #2, dated 9/21/2017, was conducted following all of the criteria found in the relevant test methods and specified in the letters received from EPA.\" , no specific language located in the report."]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2,"not sure why an ATM needed, medium",null,null,"Run #",null,1,1,1,2,2,2,"not sure why an ATM needed, medium",null,null,"Run #",null,1,1,1,2,2,2,"not sure why an ATM needed, medium"]
["Run Category",null,"High","Medium","Low","High","Medium","Low","ouput in R1 has a burn rate 50% higher",null,null,"Run Category",null,"High","Medium","Low ","High","Medium","Low","ouput in R1 has a burn rate 50% higher",null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low","ouput in R1 has a burn rate 50% higher"]
["Burn rate (kg/hr)",null,2.3199999999999998,2.9,1.76,1.98,1.55,1.05,"than the high burn rate in R2.",null,null,"Burn rate (kg/hr)",null,2.3199999999999998,2.9,1.76,1.98,1.55,1.05,"In their response, Myren stated that the medium data for two sets of run vary because the test burn sequence was reversed.",null,null,"Burn rate (kg/hr)",null,2.3199999999999998,2.9,1.76,1.98,1.55,1.05,"In their response, Myren stated that the medium data for two sets of run vary because the test burn sequence was reversed."]
["Heat output (Btu/hr)",null,33114,42099,25198,27834,14856,19573,40000,null,null,"Heat output (Btu/hr)",null,33114,42099,25198,27834,14856,19573,40000,null,null,"Heat output (Btu/hr)",null,33114,42099,25198,27834,14856,19573,40000]
["CO (g/min)",null,1.18,1.61,1.75,1.97,1.7,1.42,null,null,null,"CO (g/min)",null,1.18,1.61,1.75,1.97,1.7,1.42,null,null,null,"CO (g/min)",null,1.18,1.61,1.75,1.97,1.7,1.42]
["HHV efficiency (%)",null,78.3,79.599999999999994,79.5,77.2,79.3,78.5,null,null,null,"HHV efficiency (%)",null,78.3,79.599999999999994,79.5,77.2,79.3,78.5,null,null,null,"HHV efficiency (%)",null,78.3,79.599999999999994,79.5,77.2,79.3,78.5]
["Overall PM emissions (g/hr)",1.5,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.5,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.5]
["PM 1-hr filter pull (g/hr)",1.52,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.52,null,null,null,null,null,null,"Myren did note in their response that the 1.52 is average of two filter pulls",null,null,"PM 1-hr filter pull (g/hr)",1.52,null,null,null,null,null,null,"Myren did note in their response that the 1.52 is average of two filter pulls"]
["Filter data","Not reported",null,null,null,null,null,null,"unable to locate in report",null,null,"Filter data","Not reported",null,null,null,null,null,null,"Myren stated that 110 mm filters (instead of 47 mm) were used and provided a detailed explanation of filter data which the reviewer was unable to locate in either report",null,null,"Filter data","Not reported",null,null,null,null,null,null,"Myren stated that 110 mm filters (instead of 47 mm) were used and provided a detailed explanation of filter data which the reviewer was unable to locate in either report"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Myren stated that the train precision, T1 and T2, are reported as 4.5% and 5.57%, respectively on the far right column on page 4 with the title \"Summary of ASTM 2515 Particuate Emissions Sampling Train Performance\", although the reviewer was unable to located in report",null,null,"Train precision (%)","yes",null,null,null,null,null,null,null,null,null,"Train precision (%)","yes"]
["Negative weights","Cannot be determined",null,null,null,null,null,null,"Myren stated the negative of -0.0014 g shown severally on the woodstove data sheets #5s was accounted for in the acetone wash catch. Therefore, there were no actual negative weights for the ampling trains used for the testing of the device.",null,null,"Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Myren stated that since test run #2 was done on a reversed burn sequence, it was assumed that the dry burn rate is close to the minmum burn rate possible. Also, they said that the lowest burn rate reported (1.05 kg/h) is below 1.15 kg/h required for the ASTM E3053 and close to 1.0 kg/hr minimum DBR required for crib fuel",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Myren stated that since test run #2 was done on a reversed burn sequence, it was assumed that the dry burn rate is close to the minmum burn rate possible. Also, they said that the lowest burn rate reported (1.05 kg/h) is below 1.15 kg/h required for the ASTM E3053 and close to 1.0 kg/hr minimum DBR required for crib fuel"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Myren stated that the densified fuel logs are blends materials obtained from local wood products companied. They also metioned that first page contains the ultimate analysis performed on the North Idaho Energy log.",null,null,"Pellet species/type","Blend",null,null,null,null,null,null,null,null,null,"Pellet species/type","Blend"]
["Pellet fuel certification","Not reported",null,null,null,null,null,null,"Myren claimed that they are unaware of any certification program for densified fuel logs ",null,null,"Pellet fuel certification","No certification for fuel logs",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","No certification for fuel logs"]
["Source of the pellet specification","Not reported",null,null,null,null,null,null,"They stated that the densified fuel logs are products of North Idaho Energy loacted in Moyes Spring, ID",null,null,"Source of the pellet specification","No certification for fuel logs",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","No certification for fuel logs"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"not specifically called improper fuels warning but mentioned do not burn items",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,"Myren said by addressing the response, the issue will be resolved",null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,"Myren said by addressing the response, the issue will be resolved"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","1/9/17 & 9/5/17",null,null,null,null,null,null,null,null,null,"Test dates","1/9/17 & 9/5/17",null,null,null,null,null,null,null,null,null,"Test dates","1/9/17 & 9/5/17"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"Myren stated in the response that the 30-day notice titled \"Wood Heater 30-Day Advance Certification Test Notification\" is in the first paragraph on page xii",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"Myren stated that the 30-day notice in the test report #1 indicated that the test would start sometime beginning the week of January 9, 2017, and the actual test was done on 1/9/2017. They also said that in the 30-day notice in test report # 2 it was stated the test would occur on September  4. 2017, but because it was national holiday (Labor Day), the test wa done on 9/5/2017",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No",null,null,null,null,null,null,"Myren indicated that the tests were either done on 1/9/2017 in the test report #1, or 9/5/2017 in the test report #2",null,null,"Tested in one day","No",null,null,null,null,null,null,"Myren indicated that the tests were either done on 1/9/2017 in the test report #1, or 9/5/2017 in the test report #2"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No",null,null,null,null,null,null,"Myren stated that while reporting of the testing was passed the 60-day mark for the test report #1 because of circumstances beyond them, they said that they shipped the report for the test report #2 on 9/5/2020. a day after the testing. They said what happened after shipping the report to OMNI was beyong their control ",null,null,"60 Day report to EPA","No",null,null,null,null,null,null,"Myren stated that while reporting of the testing was passed the 60-day mark for the test report #1 because of circumstances beyond them, they said that they shipped the report for the test report #2 on 9/5/2020. a day after the testing. They said what happened after shipping the report to OMNI was beyong their control "]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Colville, Washington"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2016-12-28"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2017-01-09",null,null,null,null,null,null,"Second run completed on 9/5/2017"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no",null,null,null,null,null,null,"refer to pg 104 in report pdf"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negative values"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negative values"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negative values"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negative values"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change","no"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification",null,null,null,null,null,null,"pg 238  of report pdf"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",51,null,null,null,null,null,null,"pg 78 of pdf report"]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",51]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",21,null,null,null,null,null,null,"refer to cell I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2,null,null,null,null,null,null,"integrated runs  one in January and one in September"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,"done per EPA Guidance but using a run with a different method and averaging raises questions."]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes",null,null,null,null,null,null,"Pg 406 of report - only 4 calibrations reported "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-09-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2017-09-18","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2022-09-18"]

{"sheet":"HHH-Accentra-2","index":2,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,null,null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,null,null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman"]
["Model","Accentra-2",null,null,null,null,null,null,null,null,null,"Model","Accentra-2",null,null,null,null,null,null,null,null,null,"Model","Accentra-2"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,3,"Yellow flags",null,6,null,null,null,"Red flags",3,"Orange flags",null,3,"Yellow flags",null,6,null,null,null,"Red flags",3,"Orange flags",null,3,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"tested at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"tested at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"tested at Omni facility"]
["Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI"]
["Report certified","Not reported",null,null,null,null,null,null,"unable to locate certification within report, only authurized by OMNI Staff.",null,null,"Report certified","Not reported",null,null,null,null,null,null,"unable to locate certification within report, only authurized by OMNI Staff.",null,null,"Report certified","Not reported",null,null,null,null,null,null,"unable to locate certification within report, only authurized by OMNI Staff."]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.62,null,"PM Highest 1-hr (g/hr)",null,null,1.73,null,null,null,null,"Overall PM emissions (g/hr)",0.62,null,"PM Highest 1-hr (g/hr)",null,null,1.73,null,null,null,null,"Overall PM emissions (g/hr)",0.62,null,"PM Highest 1-hr (g/hr)",null,null,1.73]
["Overall HHV efficiency (%)",71.2,null,null,null,null,null,null,78.099999999999994,null,null,"Overall HHV efficiency (%)",71.2,null,null,null,null,null,null,78.099999999999994,null,null,"Overall HHV efficiency (%)",71.2,null,null,null,null,null,null,78.099999999999994]
["Overall heat output (Btu/hr)",25210,null,null,null,null,null,null,40000,null,null,"Overall heat output (Btu/hr)",25210,null,null,null,null,null,null,40000,null,null,"Overall heat output (Btu/hr)",25210,null,null,null,null,null,null,40000]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"compl 4/15, 5/1, 5/12, ",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"compl 4/15, 5/1, 5/12, ",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"compl 4/15, 5/1, 5/12, "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Flue temp data only. Missing time and weight for all fuel added.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Flue temp data only. Missing time and weight for all fuel added.",null,null,"Conditioning data","Reported",null,null,null,null,null,null,"included in updated report"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"no mention fo run appropriateness",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"no mention fo run appropriateness",null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,"no mention of run validity ",null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,"no mention of run validity ",null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"there may have been none",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"there may have been none",null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,"AIR SETTING DATA REPORTED",null,null,"Run #",null,1,1,1,null,null,null,"AIR SETTING DATA REPORTED",null,null,"Run #",null,1,1,1,null,null,null,"AIR SETTING DATA REPORTED"]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.95,0.8,0.49,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.95,0.8,0.49,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.95,0.8,0.49]
["Heat output (Btu/hr)",null,25210,9050,6253,null,null,null,40000,null,null,"Heat output (Btu/hr)",null,25210,9050,6253,null,null,null,40000,null,null,"Heat output (Btu/hr)",null,25210,9050,6253,null,null,null,40000]
["CO (g/min)",null,0.39600000000000002,1.0999999999999999E-2,0,null,null,null,null,null,null,"CO (g/min)",null,0.39600000000000002,1.0999999999999999E-2,0,null,null,null,null,null,null,"CO (g/min)",null,0.39600000000000002,1.0999999999999999E-2,0]
["HHV efficiency (%)",null,69.5,67.900000000000006,75.400000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,69.5,67.900000000000006,75.400000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,69.5,67.900000000000006,75.400000000000006]
["Overall PM emissions (g/hr)",0.62,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.62,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.62]
["PM 1-hr filter pull (g/hr)",1.73,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.73,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.73]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no mention of minimum setting being lowest possible",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no mention of minimum setting being lowest possible",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"clarification included on pg 153 of updated report."]
["All run data","Not reported",null,null,null,null,null,null,"missing pages 21-143 of the test report",null,null,"All run data","Not reported",null,null,null,null,null,null,"missing pages 21-143 of the test report",null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"lignetics premium hardwood",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"lignetics premium hardwood",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"lignetics premium hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Pellet bag label",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Pellet bag label",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Pellet bag label"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2015-05-12",null,null,null,null,null,null,"received 4/15/2015",null,null,"Test dates","2015-05-12",null,null,null,null,null,null,"received 4/15/2015",null,null,"Test dates","2015-05-12",null,null,null,null,null,null,"received 4/15/2015"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon",null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2015-04-15",null,null,null,null,null,null,null,null,null,"date lab received the unit","2015-04-15"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2015-04-30",null,null,null,null,null,null,null,null,null,"date first day of conditioning","2015-04-30"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2015-05-12",null,null,null,null,null,null,null,null,null,"date first day of testing","2015-05-12"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","no"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported",null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives",null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives",null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I22",null,null,"number of hours at correct conditioning conditions",0,null,null,null,null,null,null,"All 50 hours of conditioning were above medium burn rate reported in test (0.8kg/hr or 1.76lb/hr). Avg burn rate for condition was approximately 4lb/hr"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42",null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,7,3.56,2.99,1.07,1,0.18,null,null,null,null,null,7,3.56,2.99,1.07,1,0.18]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","yes"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated",null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is included in the report some are outside the 6 month requriement.",null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is included in the report some are outside the 6 month requriement."]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-05-01","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2016-05-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-05-01",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-05-01"]

{"sheet":"HHH-Accentra 52i-TC","index":3,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,null,null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman"]
["Model","Accentra 52i- TC",null,null,null,null,null,null,null,null,null,"Model","Accentra 52i- TC"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"0+SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":2},"Orange flags",null,5,"Yellow flags",null,5,null,null,null,"Red flags",{"$f":"0+SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":2},"Orange flags",null,5,"Yellow flags",null,5]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"peformed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"peformed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"unable to locate certification within report, only authurized by OMNI Staff.",null,null,"Report certified","Not reported",null,null,null,null,null,null,"unable to locate certification within report, only authurized by OMNI Staff."]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1200000000000001,null,"PM Highest 1-hr (g/hr)",null,null,3.23,null,null,null,null,"Overall PM emissions (g/hr)",1.1200000000000001,null,"PM Highest 1-hr (g/hr)",null,null,3.23]
["Overall HHV efficiency (%)",76.099999999999994,null,null,null,null,null,null,81.3,null,null,"Overall HHV efficiency (%)",76.099999999999994,null,null,null,null,null,null,81.3]
["Overall heat output (Btu/hr)",39724,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",39724]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":15.096},null,"Overall CO (g/min)",null,null,0.25159999999999999,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":15.096},null,"Overall CO (g/min)",null,null,0.25159999999999999]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Missing time and weight for all fuel added. Lab states unit was received on 1/4/2017, however conditioning was  conducted at lab between 12/6-8/2016",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Missing time and weight for all fuel added. Lab states unit was received on 1/4/2017, however conditioning was  conducted at lab between 12/6-8/2016"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data pg. 125, no specific dates of testing only a range. There is no way to determine if conditioning was conducted at medium burn rate due to lack of conditioning information.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data pg. 125, no specific dates of testing only a range. There is no way to determine if conditioning was conducted at medium burn rate due to lack of conditioning information."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.71,1.1499999999999999,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.71,1.1499999999999999,0.6]
["Heat output (Btu/hr)",null,39724,16666,7418,null,null,null,50300,null,null,"Heat output (Btu/hr)",null,39724,16666,7418,null,null,null,50300]
["CO (g/min)",null,"NR","NR","NR",null,null,null,null,null,null,"CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,79,78.5,66.3,null,null,null,null,null,null,"HHV efficiency (%)",null,79,78.5,66.3]
["Overall PM emissions (g/hr)",1.1200000000000001,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.1200000000000001]
["PM 1-hr filter pull (g/hr)",3.23,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.23]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"there is no mention of lowest setting possible",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"there is no mention of lowest setting possible"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Lignetics hardwood",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Lignetics hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2017-01-10",null,null,null,null,null,null,null,null,null,"Test dates","2017-01-10"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2017-01-04"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","12/6-12/8/2016"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2017-01-10"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","not reported"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"refer to I22"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"refer to I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,7,"feed 40%",3.1,0.4,1,0.25]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is included in the report some of the certifications are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2017-02-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2022-02-01"]

{"sheet":"HHH-Allure 50","index":4,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[105,12,105,18],[106,12,106,18],[98,12,98,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[62,12,62,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[36,13,36,15],[36,16,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,13,35,15],[35,16,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,null,null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman"]
["Model","Allure 50",null,null,null,null,null,null,null,null,null,"Model","Allure 50"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Disapproved"]
["Red flags",2,"Orange flags",null,7,"Yellow flags",null,4,null,null,null,"Red flags",2,"Orange flags",null,7,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"found only authorized signatories",null,null,"Report certified","Not reported",null,null,null,null,null,null,"found only authorized signatories"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.48,null,"PM Highest 1-hr (g/hr)",null,null,3.7,null,null,null,null,"Overall PM emissions (g/hr)",1.48,null,"PM Highest 1-hr (g/hr)",null,null,3.7]
["Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,0.79900000000000004,null,null,"Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,0.79900000000000004]
["Overall heat output (Btu/hr)",39105,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",39105]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1818},null,"Overall CO (g/min)",null,null,30.3,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":1818},null,"Overall CO (g/min)",null,null,30.3]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"conditioning data page 120, reported for 9/1 but testing run on 9/2 - when did 50 hours of aging occur?",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"conditioning data page 120, reported for 9/1 but testing run on 9/2 - when did 50 hours of aging occur?"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"missing fuel add, weights and times data",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"missing fuel add, weights and times data"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,"Run 1 not cosidered valid",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,"Run 1 not cosidered valid"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2,null,null,null,"Run #",null,2,2,2,1,1,1,"lab determined run 1 was invalid. After results came back higher than expected lab found that there was damage to equipment. Lab repaired and retested"]
["Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low"]
["Burn rate (kg/hr)",null,2.88,1.32,0.94,2.84,1.26,0.72,null,null,null,"Burn rate (kg/hr)",null,2.88,1.32,0.94,2.84,1.26,0.72]
["Heat output (Btu/hr)",null,32231,18481,12730,39105,17711,9001,52600,null,null,"Heat output (Btu/hr)",null,32231,18481,12730,39105,17711,9001,52600]
["CO (g/min)",null,"NR","NR","NR","NR","NR","NR",null,null,null,"CO (g/min)",null,"NR","NR","NR","NR","NR","NR"]
["HHV efficiency (%)",null,60.4,75.900000000000006,73.599999999999994,74.400000000000006,75.599999999999994,"NR",null,null,null,"HHV efficiency (%)",null,60.4,75.900000000000006,73.599999999999994,74.400000000000006,75.599999999999994,"NR"]
["Overall PM emissions (g/hr)",1.48,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",null,1.48,null,null,2.83]
["PM 1-hr filter pull (g/hr)",3.7,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",null,3.7,null,null,7.23,null,null,"run 2 PM found on pg 122 only"]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no mention of the lowest setting, although control temp set to 1 & 25% feed rate, no way to know actual lowest setting possible",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no mention of the lowest setting, although control temp set to 1 & 25% feed rate, no way to know actual lowest setting possible"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Lignetics hardwood",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Lignetics hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","9/2/15-9/10/15",null,null,null,null,null,null,null,null,null,"Test dates","9/2/15-9/10/15"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2015-08-27"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2015-09-10"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","not reported"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,"see cell I22"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,7,"100% feed ",2.5,0.41,1,0.25]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,"email sent to EPA about lab's invalidation of run 1. "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"although callibration data is included some certifications are outside the 6 month window"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-03-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-03-01"]

{"sheet":"US Stove 6041","index":5,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","6041, 6041I, and SP6000",null,null,null,null,null,null,null,null,null,"Model","6041, 6041I, and SP6000"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",0,"Orange flags",null,7,"Yellow flags",null,4,null,null,null,"Red flags",0,"Orange flags",null,7,"Yellow flags",null,4]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,"only tested with wood. Multi fuel unit required by the method to test with all fuels. ",null,null,"Test method","ASTM 2779",null,null,null,null,null,null,"only tested with wood. Multi fuel unit required by the method to test with all fuels. "]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"performed at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"performed at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","PFS-TECO",null,null,null,null,null,null,"signed by Sebastian Button",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,"signed by Sebastian Button"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.28,null,"PM Highest 1-hr (g/hr)",null,null,0.33,null,"advertised as multi-fuel unit but not tested with other fuels.",null,null,"Overall PM emissions (g/hr)",1.28,null,"PM Highest 1-hr (g/hr)",null,null,0.33,null,"advertised as multi-fuel unit but not tested with other fuels."]
["Overall HHV efficiency (%)",57.6,null,null,null,null,null,null,57,null,null,"Overall HHV efficiency (%)",57.6,null,null,null,null,null,null,57]
["Overall heat output (Btu/hr)",21811,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",21811]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":27.6},null,"Overall CO (g/min)",null,null,0.46,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":27.6},null,"Overall CO (g/min)",null,null,0.46]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab received unit 6/3/2019 testing began 7/17/2019",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Lab received unit 6/3/2019 testing began 7/17/2019"]
["Conditioning data","Reported",null,null,null,null,null,null,null,null,null,"Conditioning data","Reported"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.67,0.79,0.75,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.67,0.79,0.75]
["Heat output (Btu/hr)",null,21811,8311,7540,null,null,null,52300,null,null,"Heat output (Btu/hr)",null,21811,8311,7540,null,null,null,52300]
["CO (g/min)",null,0.57999999999999996,0.48,0.42,null,null,null,null,null,null,"CO (g/min)",null,0.57999999999999996,0.48,0.42]
["HHV efficiency (%)",null,67.400000000000006,54.2,52.1,null,null,null,null,null,null,"HHV efficiency (%)",null,67.400000000000006,54.2,52.1]
["Overall PM emissions (g/hr)",1.28,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.28]
["PM 1-hr filter pull (g/hr)",0.33,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.33]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",4,null,null,null,null,null,null,null,null,null,"Train precision (%)",4]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"both med and low test segment ran at same setting \"#1\"",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"both med and low test segment ran at same setting \"#1\""]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Pre-to-Logs pellet",null,null,"Pellet species/type","Not reported",null,null,null,null,null,null,"Pre-to-Logs pellet"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Other - specify →",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Other - specify →"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Not included",null,null,null,null,null,null,null,null,null,"Replacement parts","Not included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2019-07-26",null,null,null,null,null,null,null,null,null,"Test dates","2019-07-26"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-06-03"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported ",null,null,null,null,null,null,"conditioning data does not have any dates"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-07-17"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",1,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is reported certifications are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-09-18","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-09-18"]

{"sheet":"AES Baby","index":6,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","American Energy Systems (AES)"]
["Model","Magnum Baby Countryside"]
["Prelim review recomm.","Disapproved"]
["Red flags",12,"Orange flags",null,8,"Yellow flags",null,10]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,"only tested with wood. Multi fuel unit required by the method to test with all fuels. "]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"manufacturer modified operating instruction mid-test."]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.98599999999999999,null,"PM Highest 1-hr (g/hr)",null,null,0.97,null,0.69]
["Overall HHV efficiency (%)",72.599999999999994,null,null,null,null,null,null,0.83]
["Overall heat output (Btu/hr)",25519]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":406.8},null,"Overall CO (g/min)",null,null,6.78]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported",null,null,null,null,null,null,"shown in table of contents but not included in posted report"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"states lab did testing on 3/2-4/15 but also states that they did not receive it until 4/10/2015. How were all AES units aged on the same days?"]
["Conditioning data","Not reported",null,null,null,null,null,null,"preburn 3/2-4/2015 (same days as LR)  but not tested until"]
["Lab technician notes","Not reported",null,null,null,null,null,null,"4/21/2015 why was the delay so long."]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,"Mentions anomaly in run 1"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,2,2,2]
["Run Category",null,"Other","High","Medium","Low",null,null,"states it can burn corn but does not "]
["Burn rate (kg/hr)",null,1.63,1.9,1,0.75,null,null,"appear to have tested with that fuel."]
["Heat output (Btu/hr)",null,"NR",25519,13039,10330,null,null,32000]
["CO (g/min)",null,"NR",11.13,10.39,3.02,null,null,"could not maintain sample flow rate so aborted test run 1."]
["HHV efficiency (%)",null,"NR",71.2,69.599999999999994,73.3]
["Overall PM emissions (g/hr)",0.98599999999999999]
["PM 1-hr filter pull (g/hr)",0.97]
["Filter data","Not reported"]
["Train precision (%)",0.83]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"See Run 2 note, air flap was not completely closed. settings are reported in run summary."]
["All run data","Not reported",null,null,null,null,null,null,"no individual run data included in posted report"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Default values"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,"no manual included in posted test report"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"unble to locate information"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,"unble to locate information"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"did not include run 1"]
["All run data submitted","Not reported",null,null,null,null,null,null,"not included in posted report"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,"no data to support summary or R1 data"]
["Test dates","4/21/15 - 4/22/15",null,null,null,null,null,null,"received 4/10/2015"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","No"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same"]
["Test location","Lab"]
["date lab received the unit"]
["date first day of conditioning"]
["date first day of testing"]
["first hour PM emissions reported for all runs"]
["first hour PM emissions reported in grams per hour"]
["first hour PM emissions zero or negative"]
["first hour PM emissions measured with front and back filter"]
["Zero CO emission reported"]
["Any incomplete runs"]
["Pre-ignition data reported"]
["filter changes during test run"]
["filter plugged during test run"]
["What type of filter used"]
["Negative probe weight >5% of PM"]
["Negative probe value"]
["Negative room air values"]
["Ambient background filter data"]
["Proportional sampling"]
["Leak check - pre-test leak check  reported"]
["Leak check - any filter change"]
["Leak check - post leak check reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements"]
["number of conditioning hours reported in summary"]
["number of conditioning hours with data"]
["number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met"]
["high test settings match high in OM"]
["Total number of runs"]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate."]
["Calibration data"]
["Milestone Date","2022-12-06"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"AES 3500P ","index":7,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","American Energy Systems (AES)"]
["Model","3500P, 35001, and 3502"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,8,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,"only tested with wood. Multi fuel unit required by the method to test with all fuels. "]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.0069999999999999,null,"PM Highest 1-hr (g/hr)",null,null,0.89]
["Overall HHV efficiency (%)",66.5,null,null,null,null,null,null,0.71299999999999997]
["Overall heat output (Btu/hr)",20607]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":811.8},null,"Overall CO (g/min)",null,null,13.53]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"preburn 3/2-4/2015 (same days as LR)  but not tested until 4/17/2015 why was the delay so long?"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none but wasn't specifically stated"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.59,0.67,0.42]
["Heat output (Btu/hr)",null,20607,7901,4917,null,null,null,56000]
["CO (g/min)",null,15.64,11.47,13.66]
["HHV efficiency (%)",null,68.7,62.8,62.2]
["Overall PM emissions (g/hr)",1.0069999999999999]
["PM 1-hr filter pull (g/hr)",0.89]
["Filter data","Not reported"]
["Train precision (%)",9.65]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Summary data indicates air shutter not fully closed for low fire setting."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood 5.1 db moisture no additional pellet data provided"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,"Manual not included in posted report"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-04-20"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be Determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"AES Little Rascal","index":8,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","American Energy Systems (AES)"]
["Model","Little Rascal"]
["Prelim review recomm.","Disapproved"]
["Red flags",12,"Orange flags",null,7,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1319999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.07]
["Overall HHV efficiency (%)",71.3]
["Overall heat output (Btu/hr)",24028]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":868.2},null,"Overall CO (g/min)",null,null,14.47]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"preburn 3/2-4/2015 (same days as LR)  but not tested until"]
["Conditioning data","Not reported",null,null,null,null,null,null,"4/23/2015 why was the delay so long."]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none but not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.86,1,0.72]
["Heat output (Btu/hr)",null,24028,12376,10247,null,null,null,40000]
["CO (g/min)",null,25.51,21.18,4.96]
["HHV efficiency (%)",null,68.7,66,75.3]
["Overall PM emissions (g/hr)",1.1319999999999999]
["PM 1-hr filter pull (g/hr)",1.07]
["Filter data","Not reported"]
["Train precision (%)",1.1000000000000001]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air settings reported p 6 but no information if fan was used or fan settings."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood, moisture 5.56% db"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,"Manual not included in posted report"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"unable to located"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,"unable to located"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-04-23"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,"Owners manual not in report and no longer available on website",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Intertek in Middleton",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-04-10",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-03-02",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-04-23",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,"no run data provided",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"Leak check listed in procedures but no data",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles diagramed pg 10",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"see cell i42",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"level 5",".5\"","Level 2",".25\"","Level 1","closed",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,"Owners manual not in report and no longer available on website",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-06-16","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-06-16"]

{"sheet":"APR 100","index":9,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","APR Industries Ltd."]
["Model","Kozi 100 Free Standing and Insert and KSH 120"]
["Prelim review recomm.","Disapproved"]
["Red flags",14,"Orange flags",null,10,"Yellow flags",null,5]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.60899999999999999,null,"PM Highest 1-hr (g/hr)",null,null,"NR",null,"no 1 hr filter pull completed"]
["Overall HHV efficiency (%)",78.599999999999994]
["Overall heat output (Btu/hr)",30596]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":3.6179999999999999},null,"Overall CO (g/min)",null,null,6.0299999999999999E-2]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received on 2/2/2015. Preburn conducted 2/23-2/25/2015"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none but not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.27,0.9,0.53]
["Heat output (Btu/hr)",null,30596,13390,8420,null,null,null,40000]
["CO (g/min)",null,0.26500000000000001,4.02E-2,0]
["HHV efficiency (%)",null,71.400000000000006,78.900000000000006,48.5]
["Overall PM emissions (g/hr)",0.60899999999999999]
["PM 1-hr filter pull (g/hr)","NR"]
["Filter data","Not reported"]
["Train precision (%)",0.86]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"summary data states air shutter wasn't fully closed. "]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,"mentions contacting dealer for parts"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-02-26",null,null,null,null,null,null,"received 2/2/15, aging 2/23-25/15"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"APR Baywin","index":10,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","APR Industries Ltd."]
["Model","BayWin Free Standing and Insert"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,8,"Yellow flags",null,7]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Testing discussed with client during test violation of rule requirements."]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.56200000000000006,null,"PM Highest 1-hr (g/hr)",null,null,"NR",null,"R1 and R2 no 1 hr filter pull data reported"]
["Overall HHV efficiency (%)",78.2,null,null,null,null,null,null,"conducted a one hour test a year later. "]
["Overall heat output (Btu/hr)",27818]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":3.1919999999999997},null,"Overall CO (g/min)",null,null,5.3199999999999997E-2]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 2/2/2015 testing took place 2/23-25/2015, the same dates as the APR Kozy 100"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Partially reported",null,null,null,null,null,null,"run one was stopped due to plugged filter"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,null,null,null,"No R1 data reported"]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.06,0.79,0.47]
["Heat output (Btu/hr)",null,27818,11844,7441,null,null,null,40000]
["CO (g/min)",null,13.65,1.77,0.13]
["HHV efficiency (%)",null,71.599999999999994,79.099999999999994,83.3]
["Overall PM emissions (g/hr)",0.56200000000000006]
["PM 1-hr filter pull (g/hr)",1.66]
["Filter data","Not reported"]
["Train precision (%)",2.17]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Setting data reported, air flap not fully closed for low setting."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,"mentions contacting dealer for parts"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"missing data from run #3 conducted to obtain 1hr filter pull 1 year after original testing"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor"]
["Test dates","2/27/15, 3/2/15 & 6/21/2016",null,null,null,null,null,null,"6/21/16 test just for 1hr filter pull"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be Determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly",null,null,null,null,null,null,null,"Did not complete a filter change on run 1 with 21 minutes left in the test, indicative of high emissions. ",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"APR Previa","index":11,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","APR Industries Ltd."]
["Model","Previa"]
["Prelim review recomm.","Disapproved"]
["Red flags",12,"Orange flags",null,10,"Yellow flags",null,{"$f":"COUNTIF(B9:H12,\"=Not reported\")+COUNTIF(B30:B35,\"=Partially reported\")+COUNTIF(B49:B61,\"Insufficient data\")+COUNTIF(B63:B67,\"Partially reported\")+COUNTIF(B63:B67,\"Partially reported minor\")++COUNTIF(B68:B71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}}]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.02,null,"PM Highest 1-hr (g/hr)",null,null,4.82]
["Overall HHV efficiency (%)",76.099999999999994]
["Overall heat output (Btu/hr)",27113]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":7.62},null,"Overall CO (g/min)",null,null,0.127]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received 2/2/2015 and testing began It is noted that condition took place on 9/02/2015 by intertek staff, and the unit was setup for testing on 9/8/2015. Only 10 hours of conditioning completed & at \"high-to-medium\" burn rates"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"could have been none but not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.08,0.83,0.52]
["Heat output (Btu/hr)",null,27113,11858,8077,null,null,null,40000]
["CO (g/min)",null,0.24,0.13500000000000001,9.2999999999999999E-2]
["HHV efficiency (%)",null,69,75.7,81.8]
["Overall PM emissions (g/hr)",1.02]
["PM 1-hr filter pull (g/hr)",4.82]
["Filter data","Not reported"]
["Train precision (%)",20.12]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Summary run information states air shutter was not fully closed during low burn testing."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,"manual mentions contacting dealer for replacement parts"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report containted only 15 pages"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-09-08"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"EvenTemp Eclipse","index":12,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Even Temp, Inc."]
["Model","Eclipse"]
["Prelim review recomm.","Disapproved"]
["Red flags",12,"Orange flags",null,11,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"testing at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.5620000000000001,null,"PM Highest 1-hr (g/hr)",null,null,0.37]
["Overall HHV efficiency (%)",67.3,null,null,null,null,null,null,0.78]
["Overall heat output (Btu/hr)",35989]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1170},null,"Overall CO (g/min)",null,null,19.5]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Preburns done the same day as the Ashby? Unit received by lab 2/5/2015, 50+ hours of conditioning done on 2/10-12/2015"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.86,1.9410000000000001,1.24]
["Heat output (Btu/hr)",null,35989,22726,13723,null,null,null,40000]
["CO (g/min)",null,51.19,25.08,7.32]
["HHV efficiency (%)",null,70.5,66.7,62]
["Overall PM emissions (g/hr)",1.5620000000000001]
["PM 1-hr filter pull (g/hr)",0.37]
["Filter data","Not reported",null,null,null,null,null,null,"not included in posted test"]
["Train precision (%)",9.56]
["Negative weights","Cannot be determined",null,null,null,null,null,null,"not included in posted test"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Air Shutter was not fully closed during low load testing."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2015-02-23"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-02-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-02-10",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-02-23",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 9 shows mixing baffles",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",".25\"","lvl 3","5/64\"","lvl 1","3/16\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-10-16","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-10-16"]

{"sheet":"EvenTemp Ashby","index":13,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Even Temp, Inc."]
["Model","Ashby - P"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,9,"Yellow flags",null,3]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,"only tested with wood. Multi fuel unit required by the method to test with all fuels. "]
["Test Lab","Intertek",null,null,null,null,null,null,"testing at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.98099999999999998,null,"PM Highest 1-hr (g/hr)",null,null,"NR"]
["Overall HHV efficiency (%)",65.8]
["Overall heat output (Btu/hr)",31713]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":7.8000000000000007},null,"Overall CO (g/min)",null,null,0.13]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 2/5/2015. Manufacturer completed aging, manufacturer conduction another 50 hours of aging from 2/10-12/2015. Why did lab need to conduct an additional three days of pre-burns?"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.31,0.9,0.54]
["Heat output (Btu/hr)",null,31713,10550,5682,null,null,null,40000]
["CO (g/min)",null,"NR",0,0,null,null,null,"report states \"*CO measurement was recorded at around 0%; therefore, the CO emissions could not be accurately calculated.\""]
["HHV efficiency (%)",null,72.7,62.1,55.3]
["Overall PM emissions (g/hr)",0.98099999999999998]
["PM 1-hr filter pull (g/hr)","NR"]
["Filter data","Not reported"]
["Train precision (%)",4.53]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"1 hr filter pull listed as NA"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2015-02-17"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"EvenTemp Prescott EXP","index":14,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Even Temp, Inc."]
["Model","Prescott EXP"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,10,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"testing at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.53200000000000003,null,"PM Highest 1-hr (g/hr)",null,null,2.29]
["Overall HHV efficiency (%)",70.3]
["Overall heat output (Btu/hr)",30089]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":"Not reported"},null,"Overall CO (g/min)",null,null,"Not reported"]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 2/5/2015, same day as APR stoves, report states manufacturer did the pre-burn but it also states that lab conducted 50 hours of testing over 3 days (2/10-12/2015), why was this needed?"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.15,1.2,0.55000000000000004]
["Heat output (Btu/hr)",null,30089,15751,6293,null,null,null,40000]
["CO (g/min)",null,0.77,0,0]
["HHV efficiency (%)",null,74.3,69.8,61.2]
["Overall PM emissions (g/hr)",0.53200000000000003]
["PM 1-hr filter pull (g/hr)",2.29]
["Filter data","Not reported"]
["Train precision (%)",11.13]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Shutter was 1/16\" from closed"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report only 15 pages"]
["Owner manual complete","All reported"]
["Test dates","2015-02-17"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-02-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-02-16",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-02-19",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 10 shows mixing baffle",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5","5/32\"","lvl 2","3/32\"","lvl 1","1/16\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-08-10","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-08-10"]

{"sheet":"EvenTemp Hastings","index":15,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Even Temp, Inc."]
["Model","Hastings"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,9,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"testing at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1339999999999999,null,"PM Highest 1-hr (g/hr)",null,null,3.7]
["Overall HHV efficiency (%)",66.400000000000006]
["Overall heat output (Btu/hr)",37455]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":11.31},null,"Overall CO (g/min)",null,null,0.1885]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 2/5/2015, same day as APR stoves, report states manufacturer did the pre-burn but it also states that lab conducted 50 hours of testing over 3 days (2/16-18/2015), why was this needed?"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically mentioned"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.06,1.18,0.66]
["Heat output (Btu/hr)",null,37455,14698,7232,null,null,null,40000]
["CO (g/min)",null,22.82,10.23,8.1999999999999993]
["HHV efficiency (%)",null,70.8,66,58.2]
["Overall PM emissions (g/hr)",1.1339999999999999]
["PM 1-hr filter pull (g/hr)",3.7]
["Filter data","Not reported",null,null,null,null,null,null,"not included in posted report"]
["Train precision (%)",3.66]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Air Shutter was not fully closed during low load testing."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report only 15 pages"]
["Owner manual complete","All reported"]
["Test dates","2015-02-20"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-02-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-02-16",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-02-20",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 10 shows mixing baffle",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no",null,null,null,null,null,null,"see cell i42",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5","5/16\"","lvl2","3/16\"","lvl 1","1/8\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"E",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-10-16","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-10-16"]

{"sheet":"HHT Santa FE-C","index":16,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31"]
["Model","Santa Fe-C, Santa Fe I-C, Castile-C, Castile I-C",null,null,null,null,null,null,null,null,null,"Model","Santa Fe-C, Santa Fe I-C, Castile-C, Castile I-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,2,"Yellow flags",null,7,null,null,null,"Red flags",1,"Orange flags",null,2,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"did not report test location",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"did not report test location"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authurized signatories only (Ken Morgan & Bruce Davis)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authurized signatories only (Ken Morgan & Bruce Davis)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.0980000000000001,null,"PM Highest 1-hr (g/hr)",null,null,1.597,null,null,null,null,"Overall PM emissions (g/hr)",1.0980000000000001,null,"PM Highest 1-hr (g/hr)",null,null,1.597]
["Overall HHV efficiency (%)",66.099999999999994,null,null,null,null,null,null,0.70399999999999996,null,null,"Overall HHV efficiency (%)",66.099999999999994,null,null,null,null,null,null,0.70399999999999996]
["Overall heat output (Btu/hr)",9097,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",9097]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":10.200000000000001},null,"Overall CO (g/min)",null,null,0.17,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":10.200000000000001},null,"Overall CO (g/min)",null,null,0.17]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Mentions manufacuter's instructions stating preburn was to be conducted at maximum setting but no specific mention of who conducted the preburn",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Mentions manufacuter's instructions stating preburn was to be conducted at maximum setting but no specific mention of who conducted the preburn"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Preburn data located on pg 16 of report does not show scale data or specific dates. Fuel added is shown in lbs but data shows 300+ added every hour.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Preburn data located on pg 16 of report does not show scale data or specific dates. Fuel added is shown in lbs but data shows 300+ added every hour."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.5309999999999999,0.59499999999999997,0.46800000000000003,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.5309999999999999,0.59499999999999997,0.46800000000000003]
["Heat output (Btu/hr)",null,22440,7299,5831,null,null,null,30600,null,null,"Heat output (Btu/hr)",null,22440,7299,5831,null,null,null,30600]
["CO (g/min)",null,0.03,0.17,0.21,null,null,null,null,null,null,"CO (g/min)",null,0.03,0.17,0.21]
["HHV efficiency (%)",null,73.3,61.3,62.3,null,null,null,null,null,null,"HHV efficiency (%)",null,73.3,61.3,62.3]
["Overall PM emissions (g/hr)",1.0980000000000001,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.0980000000000001]
["PM 1-hr filter pull (g/hr)",1.597,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.597]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report notes that they were instructed to test at minimum heat setting with control board switch set to 6. \"The manufacturer’s instructions specified operating the preburn and high burn segments atmaximum heat setting, the “FRAP” (feed rate adjustment plate) fully open, and the controlboard trim switch set to 7. The medium burn segment was operated at heat setting low, FRAPset to fully open, and the control board switch set to 7. The low burn segment at minimum heatsetting, FRAP set to full closed, and the control board switch set to 6.\"",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report notes that they were instructed to test at minimum heat setting with control board switch set to 6. \"The manufacturer’s instructions specified operating the preburn and high burn segments atmaximum heat setting, the “FRAP” (feed rate adjustment plate) fully open, and the controlboard trim switch set to 7. The medium burn segment was operated at heat setting low, FRAPset to fully open, and the control board switch set to 7. The low burn segment at minimum heatsetting, FRAP set to full closed, and the control board switch set to 6.\""]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-log brand",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-log brand"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","from an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","from an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"notes that certain fuels shouldn't be burned, but not in one location in manual",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"notes that certain fuels shouldn't be burned, but not in one location in manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-12-17",null,null,null,null,null,null,null,null,null,"Test dates","2018-12-17"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 2/13/2019",null,null,"60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 2/13/2019"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported",null,null,null,null,null,null,"see I23"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-17"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",7,"Medium",7,"Min",6]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-03-05","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-03-05"]

{"sheet":"HHT PP60-B","index":17,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC ",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC ",null,null,null,null,null,null,"2021-03-31"]
["Model","Pel-Pro PP60-B and Pleasant Hearth PH35PS-B",null,null,null,null,null,null,null,null,null,"Model","Pel-Pro PP60-B and Pleasant Hearth PH35PS-B"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,3,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,3,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing location not identified",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing location not identified"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"Authorized signatories (Bruce Davis & Aaron Kravitz)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Authorized signatories (Bruce Davis & Aaron Kravitz)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.74,null,"PM Highest 1-hr (g/hr)",null,null,0.27700000000000002,null,"0.34 g/hr",null,null,"Overall PM emissions (g/hr)",0.74,null,"PM Highest 1-hr (g/hr)",null,null,0.27700000000000002,null,"0.34 g/hr"]
["Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,0.85,null,null,"Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,0.85]
["Overall heat output (Btu/hr)",11314,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11314]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":13.2},null,"Overall CO (g/min)",null,null,0.22,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":13.2},null,"Overall CO (g/min)",null,null,0.22]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Notes manufacturers instruction for preburn to be conducted at maximum setting. But no specific information of who conducted",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Notes manufacturers instruction for preburn to be conducted at maximum setting. But no specific information of who conducted"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Preburn data located on pg 20, changes show only .1 (no units) change every 1-2 hours. Unable to determine burn rate of conditioning",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Preburn data located on pg 20, changes show only .1 (no units) change every 1-2 hours. Unable to determine burn rate of conditioning"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.65,0.72299999999999998,0.48199999999999998,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.65,0.72299999999999998,0.48199999999999998]
["Heat output (Btu/hr)",null,26020,10665,6815,null,null,null,35000,null,null,"Heat output (Btu/hr)",null,26020,10665,6815,null,null,null,35000]
["CO (g/min)",null,"NR","NR","NR",null,null,null,null,null,null,"CO (g/min)",null,0.02,0.1,0.36]
["HHV efficiency (%)",null,78.400000000000006,73.7,70.7,null,null,null,null,null,null,"HHV efficiency (%)",null,78.400000000000006,73.7,70.7]
["Overall PM emissions (g/hr)",0.74,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.74]
["PM 1-hr filter pull (g/hr)",0.27700000000000002,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.27700000000000002]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"The low burn segment at minimum heat setting (power level 1), and the trim switch set to -4. Photos show low setting was not set at lowest setting. ",null,null,"Lowest burn rate tested","No",null,null,null,null,null,null,"The low burn segment at minimum heat setting (power level 1), and the trim switch set to -4. Photos show low setting was not set at lowest setting. "]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-logs",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-logs"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.25,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.25]
["Source of the pellet specification","Pellet bag lable",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Pellet bag lable"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to located in manual",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to located in manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2019-01-22",null,null,null,null,null,null,null,null,null,"Test dates","2019-01-22"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Not reported"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2019-01-01"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-01-22"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"only stack temps reported"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot Be Determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"level 5","4 trim","level 2",-3,"Level 1 ",-4]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-04-25","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-04-25"]

{"sheet":"HHT PP70","index":18,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC  ",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC  ",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC  ",null,null,null,null,null,null,"2021-03-31"]
["Model","Pelpro PP70",null,null,null,null,null,null,null,null,null,"Model","Pelpro PP70",null,null,null,null,null,null,null,null,null,"Model","Pelpro PP70"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",7,"Orange flags",null,8,"Yellow flags",null,5,null,null,null,"Red flags",7,"Orange flags",null,8,"Yellow flags",null,5,null,null,null,"Red flags",7,"Orange flags",null,8,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"TESTED AT OMNI FACILITY",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"TESTED AT OMNI FACILITY",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"TESTED AT OMNI FACILITY"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer states that the certifier was Omni",null,null,"Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Ken Morgan)",null,null,"Report certified","Omni",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Ken Morgan)",null,null,"Report certified","Omni",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.96,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.96,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.96]
["Overall HHV efficiency (%)",82.8,null,null,null,null,null,null,0.88500000000000001,null,null,"Overall HHV efficiency (%)",82.8,null,null,null,null,null,null,0.88500000000000001,null,null,"Overall HHV efficiency (%)",82.8,null,null,null,null,null,null,0.88500000000000001]
["Overall heat output (Btu/hr)",14961,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14961,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14961]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":3.948},null,"Overall CO (g/min)",null,null,6.5799999999999997E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":3.948},null,"Overall CO (g/min)",null,null,6.5799999999999997E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":3.948},null,"Overall CO (g/min)",null,null,6.5799999999999997E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,"pg. 14",null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,"pg. 14",null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,"pg. 14"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/22/2018, 49 hours conditioning took place on 3/1/2018. Omni staff signature on aging, indicates lab did aging. ",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/22/2018, 49 hours conditioning took place on 3/1/2018. Omni staff signature on aging, indicates lab did aging. ",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/22/2018, 49 hours conditioning took place on 3/1/2018. Omni staff signature on aging, indicates lab did aging. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Only 40 hours of condition done with a medium burn rate .79kg/hr (+/-.5kg)",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Only 40 hours of condition done with a medium burn rate .79kg/hr (+/-.5kg)",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Only 40 hours of condition done with a medium burn rate .79kg/hr (+/-.5kg)"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"statement provided in modified report",null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,"statement provided in modified report",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"statement provided in modified report",null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.1800000000000002,0.79,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.1800000000000002,0.79,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.1800000000000002,0.79,0.6]
["Heat output (Btu/hr)",null,35278,12425,9603,null,null,null,42500,null,null,"Heat output (Btu/hr)",null,35278,12425,9603,null,null,null,42500,null,null,"Heat output (Btu/hr)",null,35278,12425,9603,null,null,null,42500]
["CO (g/min)",null,4.6800000000000001E-2,3.8300000000000001E-2,9.0700000000000003E-2,null,null,null,null,null,null,"CO (g/min)",null,4.6800000000000001E-2,3.8300000000000001E-2,9.0700000000000003E-2,null,null,null,null,null,null,"CO (g/min)",null,4.6800000000000001E-2,3.8300000000000001E-2,9.0700000000000003E-2]
["HHV efficiency (%)",null,82.9,80.5,82.2,null,null,null,null,null,null,"HHV efficiency (%)",null,82.9,80.5,82.2,null,null,null,null,null,null,"HHV efficiency (%)",null,82.9,80.5,82.2]
["Overall PM emissions (g/hr)",0.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.49]
["PM 1-hr filter pull (g/hr)",0.96,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.96,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.96]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states that train precision is not report however they have included gram per kg comparison to page 22 of the modified report.",null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,"ADEC has confirmed with EPA that train precision calculatons and percentage are required, ADEC will not re-calculate unprovided equations to determine compliance. ",null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,"ADEC has confirmed with EPA that train precision calculatons and percentage are required, ADEC will not re-calculate unprovided equations to determine compliance. "]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Manufacturer's instructions state,\"Dial should be set to 1 and the trim pot should be set to 0.\" However, photos of settings show a low setting that wasn't used. also need information on fan settings. ",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,"manufacturer refers reviewer to page 13 of the manual which contains fuel tips.",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"No specific reference of what not to burn in the device provided.",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"No specific reference of what not to burn in the device provided."]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-03-28",null,null,null,null,null,null,null,null,null,"Test dates","2018-03-28",null,null,null,null,null,null,null,null,null,"Test dates","2018-03-28"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"manufacturer states this is not required in report however, is availible upon request.",null,null,"30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,"manufacturer states this is not required in report however, is availible upon request.",null,null,"60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same","partially",null,null,null,null,null,null,"no mention of trim in OM"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-03-22"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-03-01"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-03-28"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",40]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Setting 10","trim to 4","setting 3","trim -1","setting 1","trim 0"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","yes"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although Calibrations are reported some seem to be outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-07-25","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-07-25"]

{"sheet":"HHT PPC90","index":19,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC ",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC ",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC ",null,null,null,null,null,null,"2021-03-31"]
["Model","PelPro PPC90, PelPro TSC90, and Pleasant Hearth PHC90",null,null,null,null,null,null,null,null,null,"Model","PelPro PPC90, PelPro TSC90, and Pleasant Hearth PHC90",null,null,null,null,null,null,null,null,null,"Model","PelPro PPC90, PelPro TSC90, and Pleasant Hearth PHC90"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,6,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,6,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,6,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing at Omni facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis, ALex Tiegs & Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis, ALex Tiegs & Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis, ALex Tiegs & Sebastian Button)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1100000000000001,null,"PM Highest 1-hr (g/hr)",null,null,3.87,null,null,null,null,"Overall PM emissions (g/hr)",1.1100000000000001,null,"PM Highest 1-hr (g/hr)",null,null,3.87,null,null,null,null,"Overall PM emissions (g/hr)",1.1100000000000001,null,"PM Highest 1-hr (g/hr)",null,null,3.87]
["Overall HHV efficiency (%)",82.3,null,null,null,null,null,null,0.88,null,null,"Overall HHV efficiency (%)",82.3,null,null,null,null,null,null,0.88,null,null,"Overall HHV efficiency (%)",82.3,null,null,null,null,null,null,0.88]
["Overall heat output (Btu/hr)",16781,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16781,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16781]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":25.68},null,"Overall CO (g/min)",null,null,0.42799999999999999,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":25.68},null,"Overall CO (g/min)",null,null,0.42799999999999999,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":25.68},null,"Overall CO (g/min)",null,null,0.42799999999999999]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 4/19/2016, no mention of who completed conditioning",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 4/19/2016, no mention of who completed conditioning",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 4/19/2016, no mention of who completed conditioning"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete conditioning data pg 146 and 147, weight data from one day only.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete conditioning data pg 146 and 147, weight data from one day only.",null,null,"Conditioning data","Reported"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"not specifically mentioned that the run was appropriate, however, report does state run was acceptable per ASTM...",null,null,"Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"not specifically mentioned that the run was appropriate, however, report does state run was acceptable per ASTM...",null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,"added to pg 6"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"not specifically mentioned that the run was valid, however, report does state run was acceptable per ASTM...",null,null,"Doc. of run validity","Partially reported",null,null,null,null,null,null,"not specifically mentioned that the run was valid, however, report does state run was acceptable per ASTM...",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,"added to pg 6"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.59,1.1399999999999999,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.59,1.1399999999999999,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.59,1.1399999999999999,0.6]
["Heat output (Btu/hr)",null,39482,17186,8456,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,39482,17186,8456,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,39482,17186,8456,null,null,null,50000]
["CO (g/min)",null,1.1399999999999999,4.4999999999999998E-2,0.495,null,null,null,null,null,null,"CO (g/min)",null,1.1399999999999999,4.4999999999999998E-2,0.495,null,null,null,null,null,null,"CO (g/min)",null,1.1399999999999999,4.4999999999999998E-2,0.495]
["HHV efficiency (%)",null,83.33,82.13,76.489999999999995,null,null,null,null,null,null,"HHV efficiency (%)",null,83.33,82.13,76.489999999999995,null,null,null,null,null,null,"HHV efficiency (%)",null,83.33,82.13,76.489999999999995]
["Overall PM emissions (g/hr)",1.1100000000000001,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.1100000000000001,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.1100000000000001]
["PM 1-hr filter pull (g/hr)",3.87,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.87,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.87]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total, explanation found on pg 6"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"setting of power level is noted as 1 time at -4",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"setting of power level is noted as 1 time at -4",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"setting of power level is noted as 1 trim at -4"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.21,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.21,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.21]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to locate in manual",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to locate in manual",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to locate in manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2016-04-20",null,null,null,null,null,null,null,null,null,"Test dates","2016-04-20",null,null,null,null,null,null,null,null,null,"Test dates","2016-04-20"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same","partially ",null,null,null,null,null,null,"no mention of trim setting",null,null,"check owners manual and highest setting in test are they the same","partially ",null,null,null,null,null,null,"no mention of trim setting"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon",null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-04-19",null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-04-19"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported",null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2016-04-20",null,null,null,null,null,null,null,null,null,"date first day of testing","2016-04-20"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported",null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives",null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives",null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change","no",null,null,null,null,null,null,null,null,null,"Leak check - any filter change","no"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"refer to cell I22",null,null,"number of hours at correct conditioning conditions",0,null,null,null,null,null,null,"All 50 hours of condition had a burn rate above the documented medium burn rate from the test run (2.51 lb/hr or 1.14 kg/hr). Conditioning burnrate averaged at approximately 4lb/hr"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"refer to cell I42",null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"refer to cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"level 5","trim 5","?","?","level 1","trim -4",null,null,null,null,null,"level 5","trim 4",2,"trim 0","level 1","trim -4"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","yes"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","not reported",null,null,null,null,null,null,"no mention of trim setting",null,null,"high test settings match high in OM","not reported",null,null,null,null,null,null,"no mention of trim setting"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated",null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some are outside the 6 month requirement",null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-05-09","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2016-05-09","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-05-09",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-05-09"]

{"sheet":"HHT PP130","index":20,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Pelpro",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Pelpro",null,null,null,null,null,null,"2021-03-31"]
["Model","PP130-B",null,null,null,null,null,null,null,null,null,"Model","PP130-B"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",5,"Orange flags",null,6,"Yellow flags",null,5,null,null,null,"Red flags",5,"Orange flags",null,6,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.53,null,"PM Highest 1-hr (g/hr)",null,null,0.96,null,null,null,null,"Overall PM emissions (g/hr)",0.53,null,"PM Highest 1-hr (g/hr)",null,null,0.96]
["Overall HHV efficiency (%)",81.900000000000006,null,null,null,null,null,null,0.875,null,null,"Overall HHV efficiency (%)",81.900000000000006,null,null,null,null,null,null,0.875]
["Overall heat output (Btu/hr)",16968,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16968]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":9.6},null,"Overall CO (g/min)",null,null,0.16,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":9.6},null,"Overall CO (g/min)",null,null,0.16]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 3/22/2018. No mention of who completed conditioning.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 3/22/2018. No mention of who completed conditioning."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data incomplete, dates and fuel addition data not reported. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data incomplete, dates and fuel addition data not reported. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"The proportionality results and sample train agreement for the test run was acceptable.",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"The proportionality results and sample train agreement for the test run was acceptable."]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"none specifically mentioned",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"none specifically mentioned"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.5299999999999998,1.03,0.6,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.5299999999999998,1.03,0.6]
["Heat output (Btu/hr)",null,40637,15929,9605,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,40637,15929,9605,null,null,null,50000]
["CO (g/min)",null,3.8300000000000001E-2,0.15,0.215,null,null,null,null,null,null,"CO (g/min)",null,3.8300000000000001E-2,0.15,0.215]
["HHV efficiency (%)",null,82.6,79.599999999999994,82.3,null,null,null,null,null,null,"HHV efficiency (%)",null,82.6,79.599999999999994,82.3]
["Overall PM emissions (g/hr)",0.53,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.53]
["PM 1-hr filter pull (g/hr)",0.96,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.96]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"minimum segment was tested at lo heat setting with 0 trim and 1 power level",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"minimum segment was tested at lo heat setting with 0 trim and 1 power level"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"Lignetics",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Lignetics"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.34,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.34]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to locate in manual",null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,"unable to locate in manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-03-26",null,null,null,null,null,null,null,null,null,"Test dates","2018-03-26"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-03-22"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2021-03-26"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-07-19","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-07-19"]

{"sheet":"HHT Classic Bay 1200 iC","index":21,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31"]
["Model","Classic Bay 1200 i-C",null,null,null,null,null,null,null,null,null,"Model","Classic Bay 1200 i-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,3,"Yellow flags",null,7,null,null,null,"Red flags",3,"Orange flags",null,3,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"did not report test location",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"did not report test location"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Alex Tiegs)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Alex Tiegs)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.78200000000000003,null,"PM Highest 1-hr (g/hr)",null,null,0.98699999999999999,null,null,null,null,"Overall PM emissions (g/hr)",0.78200000000000003,null,"PM Highest 1-hr (g/hr)",null,null,0.98699999999999999]
["Overall HHV efficiency (%)",63.6,null,null,null,null,null,null,0.67600000000000005,null,null,"Overall HHV efficiency (%)",63.6,null,null,null,null,null,null,0.67600000000000005]
["Overall heat output (Btu/hr)",14239,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14239]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":8.4},null,"Overall CO (g/min)",null,null,0.14000000000000001,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":8.4},null,"Overall CO (g/min)",null,null,0.14000000000000001]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Report mentions preburn specifications from manufacturer to run preburn at maximum setting. but not who performed the pretest",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Report mentions preburn specifications from manufacturer to run preburn at maximum setting. but not who performed the pretest"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"conditioning data is incomplete and did not report dates on data nor is there scale data. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"conditioning data is incomplete and did not report dates on data nor is there scale data. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.4239999999999999,8.72E-2,0.85099999999999998,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4239999999999999,8.72E-2,0.85099999999999998]
["Heat output (Btu/hr)",null,33925,10421,10182,null,null,null,48500,null,null,"Heat output (Btu/hr)",null,33925,10421,10182,null,null,null,48500]
["CO (g/min)",null,0.06,0.1,0.2,null,null,null,null,null,null,"CO (g/min)",null,0.06,0.1,0.2]
["HHV efficiency (%)",null,69.900000000000006,59.7,59.8,null,null,null,null,null,null,"HHV efficiency (%)",null,69.900000000000006,59.7,59.8]
["Overall PM emissions (g/hr)",0.78200000000000003,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.78200000000000003]
["PM 1-hr filter pull (g/hr)",0.98699999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.98699999999999999]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"-.9 reported on rear filter, subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"-.9 reported on rear filter, subtracted from total"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"The low burn segment at\r\nminimum heat setting, FRAP set to full closed, and the control board switch set to 1.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"The low burn segment at\r\nminimum heat setting, FRAP set to full closed, and the control board switch set to 1."]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-logs",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"pres-to-logs"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.25,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.25]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn items listed in separate locations throughout manual",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn items listed in separate locations throughout manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-12-18",null,null,null,null,null,null,null,null,null,"Test dates","2018-12-18"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-08-18"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-18"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",2,"Medium",2,"Min",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-03-05","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-03-05"]

{"sheet":"HHT Classic Bay 1200C","index":22,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31"]
["Model","Classic Bay 1200 -C ",null,null,null,null,null,null,null,null,null,"Model","Classic Bay 1200 -C "]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,4,"Yellow flags",null,7,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null," authorized signatories (Bruce Davis & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null," authorized signatories (Bruce Davis & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.0009999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.2969999999999999,null,null,null,null,"Overall PM emissions (g/hr)",1.0009999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.2969999999999999]
["Overall HHV efficiency (%)",72.7,null,null,null,null,null,null,0.77800000000000002,null,null,"Overall HHV efficiency (%)",72.7,null,null,null,null,null,null,0.77800000000000002]
["Overall heat output (Btu/hr)",15454,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",15454]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":0},null,"Overall CO (g/min)",null,null,0,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":0},null,"Overall CO (g/min)",null,null,0]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No information about when unit was received by lab or who conducted preburn.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No information about when unit was received by lab or who conducted preburn."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"conditioning data not accurate for weights added and doesn't include specific dates of tesitng, ranges from 8/28 to 10/11/2018",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"conditioning data not accurate for weights added and doesn't include specific dates of tesitng, ranges from 8/28 to 10/11/2018"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.13,1,0.82499999999999996,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.13,1,0.82499999999999996]
["Heat output (Btu/hr)",null,30851,13552,11074,null,null,null,41200,null,null,"Heat output (Btu/hr)",null,30851,13552,11074,null,null,null,41200]
["CO (g/min)",null,0.03,0,0,null,null,null,null,null,null,"CO (g/min)",null,0.03,0,0]
["HHV efficiency (%)",null,75,70.099999999999994,69.599999999999994,null,null,null,null,null,null,"HHV efficiency (%)",null,75,70.099999999999994,69.599999999999994]
["Overall PM emissions (g/hr)",1.0009999999999999,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.0009999999999999]
["PM 1-hr filter pull (g/hr)",1.2969999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.2969999999999999]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","yes",null,null,null,null,null,null,null,null,null,"Negative weights","yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,".2 on rear filter subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,".2 on rear filter subtracted from total"]
["Lowest burn rate tested","Yes",null,null,null,null,null,null,"stated in manufacturer's instructions",null,null,"Lowest burn rate tested","Yes",null,null,null,null,null,null,"stated in manufacturer's instructions"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"lignetics",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"lignetics"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.25,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.25]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials listed throughout the manual",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials listed throughout the manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-10-30",null,null,null,null,null,null,null,null,null,"Test dates","2018-10-30"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/27/2018 - 10/11/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-18"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Maximum",2,"Medium",1,"Minimum",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some of the calibration certificates are outside of the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-03-05","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-03-05"]

{"sheet":"HHT PS35-C","index":23,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Heatilator EcoChoice",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Heatilator EcoChoice",null,null,null,null,null,null,"2021-03-31"]
["Model","PS35-C, ECO Choice PS35-C, Quadra-Fire PS35-C",null,null,null,null,null,null,null,null,null,"Model","PS35-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",5,"Orange flags",null,3,"Yellow flags",null,9,null,null,null,"Red flags",5,"Orange flags",null,3,"Yellow flags",null,9]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Bruce Davis & Ken Morgan",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Bruce Davis & Ken Morgan"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.02,null,"PM Highest 1-hr (g/hr)",null,null,2.04,null,"missing 1-hr filter data from R1",null,null,"Overall PM emissions (g/hr)",1.02,null,"PM Highest 1-hr (g/hr)",null,null,2.04,null,"missing 1-hr filter data from R1"]
["Overall HHV efficiency (%)",68.8,null,null,null,null,null,null,0.78,null,null,"Overall HHV efficiency (%)",68.8,null,null,null,null,null,null,0.78]
["Overall heat output (Btu/hr)",13667,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13667]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":9},null,"Overall CO (g/min)",null,null,0.15,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":9},null,"Overall CO (g/min)",null,null,0.15]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"no mention of who completed preburn, only that manufacturer specified operating at maximum heat setting.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"no mention of who completed preburn, only that manufacturer specified operating at maximum heat setting."]
["Conditioning data","Not reported",null,null,null,null,null,null,"no conditioning data included in report, date of preburn is same date as R1. Preburn reportedly only lasted 78 min however only data for 68 is reported.",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"no conditioning data included in report, date of preburn is same date as R1. Preburn reportedly only lasted 78 min however only data for 68 is reported."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,"Report  states \"The fire went out during run 1 (per the definitions of ASTM E2779), so the test run was aborted.\r\nThe FRAP position was determined as the cause, so a second test run was performed.",null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,"Report  states \"The fire went out during run 1 (per the definitions of ASTM E2779), so the test run was aborted.\nThe FRAP position was determined as the cause, so a second test run was performed."]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,1,1,1,"I can find no cite in 2779 for fire going out",null,null,"Run #",null,2,2,2,1,1,1,"I can find no cite in 2779 for fire going out"]
["Run Category",null,"High","Medium","Low","High","Medium","Low","Run 1 performance requires clarification",null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low","Run 1 performance requires clarification"]
["Burn rate (kg/hr)",null,2.2320000000000002,1.04,0.67100000000000004,"NR","NR","NR","where is 1 hr filter data for R1 - 121 mg?",null,null,"Burn rate (kg/hr)",null,2.2320000000000002,1.04,0.67100000000000004,"NR","NR","NR","where is 1 hr filter data for R1 - 121 mg?"]
["Heat output (Btu/hr)",null,29680,12938,8649,"NR","NR","NR",34000,null,null,"Heat output (Btu/hr)",null,29680,12938,8649,"NR","NR","NR",34000]
["CO (g/min)",null,0.04,0.15,0.17,"NR","NR","NR",null,null,null,"CO (g/min)",null,0.04,0.15,0.17,"NR","NR","NR"]
["HHV efficiency (%)",null,70.8,66.2,68.599999999999994,"NR","NR","NR",null,null,null,"HHV efficiency (%)",null,70.8,66.2,68.599999999999994,"NR","NR","NR"]
["Overall PM emissions (g/hr)",1.02,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.02]
["PM 1-hr filter pull (g/hr)",2.04,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.04]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,"all filter catches for run 1 were reported negative, after subtracting filter weights ",null,null,"Negative weights","Yes",null,null,null,null,null,null,"all filter catches for run 1 were reported negative, after subtracting filter weights "]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No"]
["Lowest burn rate tested","No",null,null,null,null,null,null," Identical settings were used for the High and Medium segments, and the trim and heat setting were the same for the Low segment, but the FRAP position was altered to 3/8” open. ",null,null,"Lowest burn rate tested","No",null,null,null,null,null,null," Identical settings were used for the High and Medium segments, and the trim and heat setting were the same for the Low segment, but the FRAP position was altered to 3/8” open. "]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","Not reported",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","Not reported"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials are throughout the manual",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials are throughout the manual"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"run 1 data not included",null,null,"Summary tables complete","Partially reported",null,null,null,null,null,null,"run 1 data not included"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2/27 & 2/28/18",null,null,null,null,null,null,null,null,null,"Test dates","2/27 & 2/28/18"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Not reported"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-02-27"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","no"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","not reported"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","not reported"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","yes"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with deviation issues",null,null,null,null,null,null,"pgs 17, 20, 21 of report shows deviation outside the allowable - showing ten minute averages higher that 230"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"high",3,"Medium",2,"low",2]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,"email sent to EPA about run averaging on 1/7/22"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is reported some certifications are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date","2020-02-13",null,null,null,null,null,null,null,null,null,"Compliance Date","2020-02-13","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-02-13"]

{"sheet":"HHT P43-C","index":24,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Pelpro",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Pelpro",null,null,null,null,null,null,"2021-03-31"]
["Model","P43-C",null,null,null,null,null,null,null,null,null,"Model","P43-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,3,"Yellow flags",null,5,null,null,null,"Red flags",2,"Orange flags",null,3,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.94599999999999995,null,"PM Highest 1-hr (g/hr)",null,null,1.603,null,null,null,null,"Overall PM emissions (g/hr)",0.94599999999999995,null,"PM Highest 1-hr (g/hr)",null,null,1.603]
["Overall HHV efficiency (%)",77.900000000000006,null,null,null,null,null,null,0.83499999999999996,null,null,"Overall HHV efficiency (%)",77.900000000000006,null,null,null,null,null,null,0.83499999999999996]
["Overall heat output (Btu/hr)",18430,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",18430]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":19.2},null,"Overall CO (g/min)",null,null,0.32,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":19.2},null,"Overall CO (g/min)",null,null,0.32]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"It is not noted when unit was received by lab nor who conducted the conditioning.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"It is not noted when unit was received by lab nor who conducted the conditioning."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Data reported does not include dates of aging (states january 2018) nor does it provide data when fuel was added. It also lacks scale readings for change in weight.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Data reported does not include dates of aging (states january 2018) nor does it provide data when fuel was added. It also lacks scale readings for change in weight."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.3319999999999999,0.96799999999999997,1.107,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.3319999999999999,0.96799999999999997,1.107]
["Heat output (Btu/hr)",null,30879,14412,16606,null,null,null,43500,null,null,"Heat output (Btu/hr)",null,30879,14412,16606,null,null,null,43500]
["CO (g/min)",null,0.11,0.18,0.48,null,null,null,null,null,null,"CO (g/min)",null,0.11,0.18,0.48]
["HHV efficiency (%)",null,71.099999999999994,79.900000000000006,80.5,null,null,null,null,null,null,"HHV efficiency (%)",null,71.099999999999994,79.900000000000006,80.5]
["Overall PM emissions (g/hr)",0.94599999999999995,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.94599999999999995]
["PM 1-hr filter pull (g/hr)",1.603,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.603]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"-.1  rear filter of both train 1 & 2",null,null,"Negs handled appropriately","No",null,null,null,null,null,null," -.1  rear filter of both train 1 & 2"]
["Lowest burn rate tested","Yes",null,null,null,null,null,null,"the low burn segment at the minimum heat dial setting (fixed stop). These settings were\r\nused for the test run, as specified. No home user could achieve a lower burn rate than that\r\ntested via manipulation of any of these settings",null,null,"Lowest burn rate tested","Yes",null,null,null,null,null,null,"the low burn segment at the minimum heat dial setting (fixed stop). These settings were\nused for the test run, as specified. No home user could achieve a lower burn rate than that\ntested via manipulation of any of these settings"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.47,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.47]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-10-29",null,null,null,null,null,null,null,null,null,"Test dates","2018-10-29"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-10-29"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-02-11","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-02-11"]

{"sheet":"HHT CAB50-C","index":25,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Heatilator EcoChoice",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Heatilator EcoChoice",null,null,null,null,null,null,"2021-03-31"]
["Model","ECO CAB50-C and ECO PS50-C",null,null,null,null,null,null,null,null,null,"Model","ECO CAB50-C and ECO PS50-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,4,"Yellow flags",null,8,null,null,null,"Red flags",1,"Orange flags",null,4,"Yellow flags",null,8]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Alex Tiegs)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Alex Tiegs)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.0009999999999999,null,"PM Highest 1-hr (g/hr)",null,null,3.11,null,null,null,null,"Overall PM emissions (g/hr)",1.0009999999999999,null,"PM Highest 1-hr (g/hr)",null,null,3.11]
["Overall HHV efficiency (%)",65.099999999999994,null,null,null,null,null,null,0.78,null,null,"Overall HHV efficiency (%)",65.099999999999994,null,null,null,null,null,null,0.78]
["Overall heat output (Btu/hr)",14825,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14825]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":13.8},null,"Overall CO (g/min)",null,null,0.23,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":13.8},null,"Overall CO (g/min)",null,null,0.23]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who completed the preburn or conditioning. Only that preburn to be conducted at maximum heat setting.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who completed the preburn or conditioning. Only that preburn to be conducted at maximum heat setting."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Aging data incomplete per requirements - need dates and details when fuel was added. Data only has the year 2018 reported",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Aging data incomplete per requirements - need dates and details when fuel was added. Data only has the year 2018 reported"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.65,1.26,0.7,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.65,1.26,0.7]
["Heat output (Btu/hr)",null,36591,14982,7488,null,null,null,43000,null,null,"Heat output (Btu/hr)",null,36591,14982,7488,null,null,null,43000]
["CO (g/min)",null,8.5999999999999993E-2,0.16500000000000001,0.311,null,null,null,null,null,null,"CO (g/min)",null,8.5999999999999993E-2,0.16500000000000001,0.311]
["HHV efficiency (%)",null,73.400000000000006,63.1,57,null,null,null,null,null,null,"HHV efficiency (%)",null,73.400000000000006,63.1,57]
["Overall PM emissions (g/hr)",1.0009999999999999,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.0009999999999999]
["PM 1-hr filter pull (g/hr)",3.11,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.11]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"The low burn segment at minimum heat setting, FRAP set to\r\nfull closed, and the control board switch set to 2. ",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"The low burn segment at minimum heat setting, FRAP set to\nfull closed, and the control board switch set to 2. "]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.33,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.33]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials listed throughout the manual but no specific improper fuel warning",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn materials listed throughout the manual but no specific improper fuel warning"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-11-19",null,null,null,null,null,null,null,null,null,"Test dates","2018-11-19"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Not reported"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-11-19"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,3,"max",2,"med",2,"low"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is reported some certifications are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-04-24","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-04-24"]

{"sheet":"HHT P61-C","index":26,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31"]
["Model","P61-C",null,null,null,null,null,null,null,null,null,"Model","P61-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,2,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,2,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU,  IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU,  IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Aaron Kravits & Alex Tiegs",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Aaron Kravits & Alex Tiegs"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.48,null,"PM Highest 1-hr (g/hr)",null,null,3.68,null,null,null,null,"Overall PM emissions (g/hr)",1.48,null,"PM Highest 1-hr (g/hr)",null,null,3.68]
["Overall HHV efficiency (%)",79.3,null,null,null,null,null,null,0.85,null,null,"Overall HHV efficiency (%)",79.3,null,null,null,null,null,null,0.85]
["Overall heat output (Btu/hr)",23080,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",23080]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":10.799999999999999},null,"Overall CO (g/min)",null,null,0.18,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":10.799999999999999},null,"Overall CO (g/min)",null,null,0.18]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,3.2589999999999999,1.323,1.1479999999999999,null,null,null,null,null,null,"Burn rate (kg/hr)",null,3.2589999999999999,1.323,1.1479999999999999]
["Heat output (Btu/hr)",null,46831,19804,17085,null,null,null,60700,null,null,"Heat output (Btu/hr)",null,46831,19804,17085,null,null,null,60700]
["CO (g/min)",null,0.68,7.0000000000000007E-2,0.09,null,null,null,null,null,null,"CO (g/min)",null,0.68,7.0000000000000007E-2,0.09]
["HHV efficiency (%)",null,77.099999999999994,80.3,79.900000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,77.099999999999994,80.3,79.900000000000006]
["Overall PM emissions (g/hr)",1.48,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.48]
["PM 1-hr filter pull (g/hr)",3.68,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.68]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"-1.5 on rear filter of train 2 subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null," -1.5 on rear filter of train 2 subtracted from total"]
["Lowest burn rate tested","Yes",null,null,null,null,null,null,"low burn segment at the minimum heat dial setting (fixed stop). These settings were\r\nused for the test run, as specified. No home user could achieve a lower burn rate than that\r\ntested via manipulation of any of these settings.",null,null,"Lowest burn rate tested","Yes",null,null,null,null,null,null,"low burn segment at the minimum heat dial setting (fixed stop). These settings were\nused for the test run, as specified. No home user could achieve a lower burn rate than that\ntested via manipulation of any of these settings."]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.37,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.37]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-12-10",null,null,null,null,null,null,null,null,null,"Test dates","2018-12-10"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Not reported"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-11-15"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-10"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","yes",null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",52.5,6,20,"Min",17.5]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some of the calibration certificates are outside of the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-03-05","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-03-05"]

{"sheet":"HHT P68-C","index":27,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31"]
["Model","P68-C",null,null,null,null,null,null,null,null,null,"Model","P68-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,3,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,3,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU,  IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU,  IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"location of testing not detailed in the report"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Aaron Kravits & Alex Tiegs",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories Aaron Kravits & Alex Tiegs"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.38,null,"PM Highest 1-hr (g/hr)",null,null,3.07,null,null,null,null,"Overall PM emissions (g/hr)",1.38,null,"PM Highest 1-hr (g/hr)",null,null,3.07]
["Overall HHV efficiency (%)",79,null,null,null,null,null,null,0.85,null,null,"Overall HHV efficiency (%)",79,null,null,null,null,null,null,0.85]
["Overall heat output (Btu/hr)",24800,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",24800]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":12},null,"Overall CO (g/min)",null,null,0.2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":12},null,"Overall CO (g/min)",null,null,0.2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,3.597,1.524,1.073,null,null,null,null,null,null,"Burn rate (kg/hr)",null,3.597,1.524,1.073]
["Heat output (Btu/hr)",null,53074,23111,15878,null,null,null,67600,null,null,"Heat output (Btu/hr)",null,53074,23111,15878,null,null,null,67600]
["CO (g/min)",null,0.85,0.09,7.0000000000000007E-2,null,null,null,null,null,null,"CO (g/min)",null,0.85,0.09,7.0000000000000007E-2]
["HHV efficiency (%)",null,78.5,80.7,78.7,null,null,null,null,null,null,"HHV efficiency (%)",null,78.5,80.7,78.7]
["Overall PM emissions (g/hr)",1.38,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.38]
["PM 1-hr filter pull (g/hr)",3.07,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.07]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"rear filter weights for both train 1 & 2 were not take post test",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"rear filter weights for both train 1 & 2 were not take post test and rear filter tare weights were subtracted from the total catch"]
["Lowest burn rate tested","Yes",null,null,null,null,null,null,"low burn segment at the\r\nminimum heat dial setting (fixed stop). These settings were used for the test run, as specified.\r\nNo home user could achieve a lower burn rate than that tested via manipulation of any of these\r\nsettings.",null,null,"Lowest burn rate tested","Yes",null,null,null,null,null,null,"low burn segment at the minimum heat dial setting (fixed stop). These settings were used for the test run, as specified. No home user could achieve a lower burn rate than that tested via manipulation of any of these settings."]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.6,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.6]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-01-14",null,null,null,null,null,null,"report was done 1/23/2019?",null,null,"Test dates","2018-01-14",null,null,null,null,null,null,"report was done 1/23/2019?"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Not reported"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-12-19"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-01-14"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","yes",null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"max",47.5,"max",17.5,"min ",125]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some of the calibration certificates are outside of the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-03-26","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-03-26"]

{"sheet":"HHT Absolute 43-C","index":28,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31"]
["Model","Absolute 43-C",null,null,null,null,null,null,null,null,null,"Model","Absolute 43-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",4,"Orange flags",null,6,"Yellow flags",null,4,null,null,null,"Red flags",4,"Orange flags",null,6,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz, Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz, Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.99,null,"PM Highest 1-hr (g/hr)",null,null,1.44,null,null,null,null,"Overall PM emissions (g/hr)",0.99,null,"PM Highest 1-hr (g/hr)",null,null,1.44]
["Overall HHV efficiency (%)",77,null,null,null,null,null,null,0.82299999999999995,null,null,"Overall HHV efficiency (%)",77,null,null,null,null,null,null,0.82299999999999995]
["Overall heat output (Btu/hr)",20876,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",20876]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":6},null,"Overall CO (g/min)",null,null,0.1,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":6},null,"Overall CO (g/min)",null,null,0.1]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"reported in report but not in included in statement summary",null,null,"Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"reported in report but not in included in statement summary"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.2999999999999998,1,0.74,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.2999999999999998,1,0.74]
["Heat output (Btu/hr)",null,44183,19132,14141,null,null,null,44200,null,null,"Heat output (Btu/hr)",null,44183,19132,14141,null,null,null,44200]
["CO (g/min)",null,0.22,0.08,7.0000000000000007E-2,null,null,null,null,null,null,"CO (g/min)",null,0.22,0.08,7.0000000000000007E-2]
["HHV efficiency (%)",null,79.2,76.5,74.900000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,79.2,76.5,74.900000000000006]
["Overall PM emissions (g/hr)",0.99,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.99]
["PM 1-hr filter pull (g/hr)",1.44,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.44]
["Filter data","Reported",null,null,null,null,null,null,"redacted filter weight information without explaination.",null,null,"Filter data","Reported",null,null,null,null,null,null,"redacted filter weight information without explaination."]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"burn setting 1 (states minimum)",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"burn setting 1 (states minimum)"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Blend",null,null,null,null,null,null,null,null,null,"Pellet species/type","Blend"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.47,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.47]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-02-20",null,null,null,null,null,null,null,null,null,"Test dates","2018-02-20"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-02-19"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-02-20"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"See cell I22"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"See cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,7,"Feed 83%",4,"Feed 37%",1,0.25]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","not reported"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some of the calibrations are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-02-11","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-02-13"]

{"sheet":"HHT Absolute 63","index":29,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,13,35,15],[35,16,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31"]
["Model","Absolute 63",null,null,null,null,null,null,null,null,null,"Model","Absolute 63"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",4,"Orange flags",null,8,"Yellow flags",null,5,null,null,null,"Red flags",4,"Orange flags",null,8,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz, Alex Tiegs & Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz, Alex Tiegs & Sebastian Button)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.43,null,"PM Highest 1-hr (g/hr)",null,null,3.04,null,"avg from run 1&2",null,null,"Overall PM emissions (g/hr)",1.43,null,"PM Highest 1-hr (g/hr)",null,null,3.04,null,"avg from run 1&2"]
["Overall HHV efficiency (%)",77.7,null,null,null,null,null,null,0.83199999999999996,null,null,"Overall HHV efficiency (%)",77.7,null,null,null,null,null,null,0.83199999999999996]
["Overall heat output (Btu/hr)",19524,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",19524]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":85.8},null,"Overall CO (g/min)",null,null,1.43,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":85.8},null,"Overall CO (g/min)",null,null,1.43]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 1/27/2016",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 1/27/2016"]
["Conditioning data","Not reported",null,null,null,null,null,null,"unable to locate in report",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"unable to locate in report"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Partially reported",null,null,null,null,null,null,"not specifically called out as anomolies but mentions run 1 being invalid due to stove settings being inproperly set",null,null,"Doc. of run anomolies","Partially reported",null,null,null,null,null,null,"not specifically called out as anomolies but mentions run 1 being invalid due to stove settings being inproperly set"]
["Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"noted in report but not addressed in narrative",null,null,"Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"noted in report but not addressed in narrative"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,2,2,2,3,3,3]
["Run Category",null,"H","M","L",null,null,null,null,null,null,"Run Category",null,"H","M","L","H","M","L"]
["Burn rate (kg/hr)",null,3.59,1.4,1.4,null,null,null,"reported zeros for g/hr R1,2,3, need ind run",null,null,"Burn rate (kg/hr)",null,3.59,1.4,1.4,3.05,1.43,0.76,"reported zeros for g/hr R1,2,3, need ind run"]
["Heat output (Btu/hr)",null,45599,25216,21356,null,null,null,61800,null,null,"Heat output (Btu/hr)",null,45599,25216,21356,56416,26532,14030,61800]
["CO (g/min)",null,700.8,11.5,15.6,null,null,null,null,null,null,"CO (g/min)",null,700.8,11.5,15.6,136.69999999999999,1.3,0,"three runs completed. First run, fan stayed on for the entire run. Lab declared invalid. Ran second test, didn't like result. Ran third test. Averaged results of run 2 and 3. "]
["HHV efficiency (%)",null,68.61,81.64,82.71,null,null,null,null,null,null,"HHV efficiency (%)",null,68.61,81.64,82.71,77.430000000000007,80.34,69.48]
["Overall PM emissions (g/hr)",1.43,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",null,1.43,null,null,2.31]
["PM 1-hr filter pull (g/hr)",3.04,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.04]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,"rear filter on both trains 1&2 had negatives in both runs 1 &3",null,null,"Negative weights","Yes",null,null,null,null,null,null,"rear filter on both trains 1&2 had negatives in both runs 1 &3"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtacted from total pm catch",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtacted from total pm catch"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"temp control 1, feed rate 25%, blower 100%",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"temp control 1, feed rate 25%, blower 100%"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"no analysis",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"no analysis"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2/8-2/11/2016",null,null,null,null,null,null,null,null,null,"Test dates","2/8-2/11/2016"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested in one day","Cannot Be Determined"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-01-27"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2015-02-11"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary","Not reported"]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"refer to cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","not reported"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",3]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,"Uncertain about run averaging email to EPA 1/7/22"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported, some are outside of the 6 month window. Pg. 36 shows a calibration done on 3/4/16 where the mass set arrived out of tolerance. "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-05-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-05-01"]

{"sheet":"HHT Mt. Vernon E2-C","index":30,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Quadra fire",null,null,null,null,null,null,"2021-03-31"]
["Model","Quadra Fire Mount Vernon E2-C, Quadra Fire Mount Vernon E2-C Insert, Trekker, Trekker Insert",null,null,null,null,null,null,null,null,null,"Model","Quadra Fire Mount Vernon E2-C, Quadra Fire Mount Vernon E2-C Insert, Trekker, Trekker Insert"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"0+SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":7},"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",{"$f":"0+SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":7},"Orange flags",null,5,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, NR, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, NR, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing at Omni lab",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing at Omni lab"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz & Alex Tiegs)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz & Alex Tiegs)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.74,null,"PM Highest 1-hr (g/hr)",null,null,0.57999999999999996,null,null,null,null,"Overall PM emissions (g/hr)",0.74,null,"PM Highest 1-hr (g/hr)",null,null,0.57999999999999996]
["Overall HHV efficiency (%)",77.900000000000006,null,null,null,null,null,null,0.83199999999999996,null,null,"Overall HHV efficiency (%)",77.900000000000006,null,null,null,null,null,null,0.83199999999999996]
["Overall heat output (Btu/hr)",19419,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",19419]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":9},null,"Overall CO (g/min)",null,null,0.15,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":9},null,"Overall CO (g/min)",null,null,0.15]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"No mention of who conducted preburn or conditioning. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete, conditioning data does not include specific dates of aging, only provides a date range. It also lacks scale weight change."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"in report but not addressed in narrative",null,null,"Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"in report but not addressed in narrative"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.31,1.26,0.85,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.31,1.26,0.85]
["Heat output (Btu/hr)",null,39428,1913,12682,null,null,null,51000,null,null,"Heat output (Btu/hr)",null,39428,1913,12682,null,null,null,51000]
["CO (g/min)",null,0.06,7.0000000000000007E-2,0.22,null,null,null,null,null,null,"CO (g/min)",null,0.06,7.0000000000000007E-2,0.22]
["HHV efficiency (%)",null,77.7,78.5,77.3,null,null,null,null,null,null,"HHV efficiency (%)",null,77.7,78.5,77.3]
["Overall PM emissions (g/hr)",0.74,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.74]
["PM 1-hr filter pull (g/hr)",0.57999999999999996,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.57999999999999996]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"negative in rear filter catch of both trains ",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"negative in rear filter catch of both trains "]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"dial setting 1, trim setting +1",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"dial setting 1, trim setting +1"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.21,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.21]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"several do not burn warnings throughout manual not able to locate a specific improper fuel warning",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"several do not burn warnings throughout manual not able to locate a specific improper fuel warning"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2017-05-19",null,null,null,null,null,null,null,null,null,"Test dates","2017-05-19"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2017-05-17"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported ",null,null,null,null,null,null,"See I23"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2017-05-19"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low ",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate."]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-04-13","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-04-13"]

{"sheet":"HHT XXV-TC","index":31,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman"]
["Model","XXV-TC"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,"Supplemental information received from manufacturer has not been reviewed due to higher priorities"]
["Red flags",5,"Orange flags",null,3,"Yellow flags",null,4]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: ES1, MD, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni lab"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"AUTHORIZED SIGNATORIES (Aaron Kravitz, Alex Tiegs & Sebastian Button)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.75,null,"PM Highest 1-hr (g/hr)",null,null,7.94]
["Overall HHV efficiency (%)",72.510000000000005,null,null,null,null,null,null,0.72499999999999998]
["Overall heat output (Btu/hr)",14758]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":34.08},null,"Overall CO (g/min)",null,null,0.56799999999999995]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 3/17/2016. No mention of who conducted conditioning or preburn"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete conditioning data page 109, conflicting dates, no weights for fuel. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.59,1.0900000000000001,0.6]
["Heat output (Btu/hr)",null,35283,14827,7096,null,null,null,48000]
["CO (g/min)",null,3.476,0,0]
["HHV efficiency (%)",null,73.58,73.62,64.28]
["Overall PM emissions (g/hr)",1.75]
["PM 1-hr filter pull (g/hr)",7.94]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,"negative on rear filter of train 1"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"temp control 1, feed rate 25%, blower off"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Blend"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","All reported"]
["Test dates","2016-03-22"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2016-04-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2021-04-01"]

{"sheet":"HHT P35i-C","index":32,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Harman",null,null,null,null,null,null,"2021-03-31"]
["Model","P35i-C",null,null,null,null,null,null,null,null,null,"Model","P35i-C"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,5,"Yellow flags",null,4,null,null,null,"Red flags",3,"Orange flags",null,5,"Yellow flags",null,4]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"conducted at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"conducted at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,null,null,null,"Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,1.56,null,null,null,null,"Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,1.56]
["Overall HHV efficiency (%)",68.2,null,null,null,null,null,null,0.74199999999999999,null,null,"Overall HHV efficiency (%)",68.2,null,null,null,null,null,null,0.74199999999999999]
["Overall heat output (Btu/hr)",15533,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",15533]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"not specifically mentioned, although it seems it may have abeen lab",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"not specifically mentioned, although it seems it may have abeen lab"]
["Conditioning data","Not reported",null,null,null,null,null,null,"Located on pg 27 of report. 60 Minutes of preburn conducted. No conditioning data or information included in report.",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"Located on pg 27 of report. 60 Minutes of preburn conducted. No conditioning data or information included in report."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2,null,null,null,"Run #",null,1,1,1,2,2,2]
["Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low"]
["Burn rate (kg/hr)",null,2.04,1.27,0.83,2.12,1,0.86,null,null,null,"Burn rate (kg/hr)",null,2.04,1.27,0.83,2.12,1,0.86]
["Heat output (Btu/hr)",null,29215,16665,10206,30614,12587,10546,38400,null,null,"Heat output (Btu/hr)",null,29215,16665,10206,30614,12587,10546,38400]
["CO (g/min)",null,0.08,0.09,0.09,0.16,0.06,0.04,null,null,null,"CO (g/min)",null,0.08,0.09,0.09,0.16,0.06,0.04]
["HHV efficiency (%)",null,74.900000000000006,68.400000000000006,63.9,75.400000000000006,65.900000000000006,63.9,null,null,null,"HHV efficiency (%)",null,74.900000000000006,68.400000000000006,63.9,75.400000000000006,65.900000000000006,63.9]
["Overall PM emissions (g/hr)",1.46,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.46]
["PM 1-hr filter pull (g/hr)",1.56,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.56]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"temp setting 1, feed limit 1.9",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"temp setting 1, feed limit 1.9"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Douglas Fir",null,null,null,null,null,null,"Olympus pellets",null,null,"Pellet species/type","Douglas Fir",null,null,null,null,null,null,"Olympus pellets"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,0.18,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,0.18]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","11/13-11/14/2019",null,null,null,null,null,null,null,null,null,"Test dates","11/13-11/14/2019"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-11-11"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not reported"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-11-13"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data","not reported"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,"See cell I33"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,7,5.22,3,2,1,1.9]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","not reported"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,"two runs completed but Run 1 did not meet medium burn rate requirementso it was invalidated. "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although reported some of the calibration certificates are outside of the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2020-02-13","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-02-13"]

{"sheet":"HHT PH50PS-B","index":33,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Hearth and Home Technologies, LLC dba Pleasant Hearth",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","Hearth and Home Technologies, LLC dba Pleasant Hearth",null,null,null,null,null,null,"2021-03-31"]
["Model","PH50PS-B, PH50CABPS-B",null,null,null,null,null,null,null,null,null,"Model","PH50PS-B, PH50CABPS-B"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Disapproved"]
["Red flags",9,"Orange flags",null,11,"Yellow flags",null,3,null,null,null,"Red flags",9,"Orange flags",null,11,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR,  NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR,  NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,null,null,null,"Test Lab","PFS-TECO"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"affidavid (Sebastian Button)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"affidavid (Sebastian Button)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.18,null,"PM Highest 1-hr (g/hr)",null,null,1.08,null,null,null,null,"Overall PM emissions (g/hr)",1.18,null,"PM Highest 1-hr (g/hr)",null,null,1.08]
["Overall HHV efficiency (%)",75.900000000000006,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",75.900000000000006]
["Overall heat output (Btu/hr)",13599,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13599]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":"Not reported"},null,"Overall CO (g/min)",null,null,"Not reported",null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":"Not reported"},null,"Overall CO (g/min)",null,null,"Not reported"]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Not reported"]
["Raw data sheets","Not reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Not reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received 3/25/2019. Report does not state who conducted the conditioning or the preburn.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received 3/25/2019. Report does not state who conducted the conditioning or the preburn."]
["Conditioning data","Not reported",null,null,null,null,null,null,"NO preburn or conditioning data included in report.",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"NO preburn or conditioning data included in report."]
["Lab technician notes","Not reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.21,0.92,0.51,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.21,0.92,0.51]
["Heat output (Btu/hr)",null,34132,13102,6871,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,34132,13102,6871,null,null,null,50000]
["CO (g/min)",null,0.08,0.21,0.6,null,null,null,null,null,null,"CO (g/min)",null,0.08,0.21,0.6]
["HHV efficiency (%)",null,79.900000000000006,74.2,69.7,null,null,null,null,null,null,"HHV efficiency (%)",null,79.900000000000006,74.2,69.7]
["Overall PM emissions (g/hr)","Not reported",null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)","Not reported"]
["PM 1-hr filter pull (g/hr)",1.08,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.08]
["Filter data","Not reported",null,null,null,null,null,null,null,null,null,"Filter data","Not reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Cannot be determined",null,null,null,null,null,null,"Not included in posted report",null,null,"Negative weights","Cannot be determined",null,null,null,null,null,null,"Not included in posted report"]
["Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,"Not included in posted report",null,null,"Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,"Not included in posted report"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,null,null,null,"Pellet species/type","Not reported"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,"Manual not inlcuded in posted report, unable to locate manual on website.",null,null,"Stack height",null,null,null,null,null,null,null,"Manual not inlcuded in posted report, unable to locate manual on website."]
["Location recommendation",null,null,null,null,null,null,null,null,null,null,"Location recommendation"]
["Guidance on proper draft",null,null,null,null,null,null,null,null,null,null,"Guidance on proper draft"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.",null,null,null,null,null,null,null,null,null,null,"Fuel selection recomm."]
["Improper fuels warnings",null,null,null,null,null,null,null,null,null,null,"Improper fuels warnings"]
["Fire starting procedures",null,null,null,null,null,null,null,null,null,null,"Fire starting procedures"]
["Proper use of air controls",null,null,null,null,null,null,null,null,null,null,"Proper use of air controls"]
["Proper operation low",null,null,null,null,null,null,null,null,null,null,"Proper operation low"]
["Ash removal procedures",null,null,null,null,null,null,null,null,null,null,"Ash removal procedures"]
["Replacement parts",null,null,null,null,null,null,null,null,null,null,"Replacement parts"]
["Federal warning (C or NC)",null,null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)"]
["Warranty rights",null,null,null,null,null,null,null,null,null,null,"Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","Not reported",null,null,null,null,null,null,null,null,null,"All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"only 18 pages in posted report",null,null,"Test report complete","Partially reported major",null,null,null,null,null,null,"only 18 pages in posted report"]
["Owner manual complete","Not reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","Not reported"]
["Test dates","2019-03-28",null,null,null,null,null,null,null,null,null,"Test dates","2019-03-28"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-03-25"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2019-03-28"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-03-28"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filter chnaged on sample A at one hourafter test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","not reported"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","not reported"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","not reported"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","not reported"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data","Not reported"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","not reported",null,null,null,null,null,null,"Appenidix containing the equipment calibration records not provided"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-05-15","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-05-15"]

{"sheet":"Castle Serenity","index":34,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","ARDISAM, Inc.",null,null,null,null,null,null,null,null,null,"Manufacturer","ARDISAM, Inc."]
["Model","Serenity Castle",null,null,null,null,null,null,null,null,null,"Model","Serenity Castle"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",5,"Orange flags",null,4,"Yellow flags",null,4,null,null,null,"Red flags",5,"Orange flags",null,4,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,null,null,null,"Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.119,null,"PM Highest 1-hr (g/hr)",null,null,1.29,null,null,null,null,"Overall PM emissions (g/hr)",1.119,null,"PM Highest 1-hr (g/hr)",null,null,1.29]
["Overall HHV efficiency (%)",69.8,null,null,null,null,null,null,0.69799999999999995,null,null,"Overall HHV efficiency (%)",69.8,null,null,null,null,null,null,0.69799999999999995]
["Overall heat output (Btu/hr)",13831,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13831]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":5.37},null,"Overall CO (g/min)",null,null,8.9499999999999996E-2,null,"g/min not reported in report",null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":5.37},null,"Overall CO (g/min)",null,null,8.9499999999999996E-2,null,"g/min not reported in report"]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Test report not clear about where conditioning completed. . Report also states that manufacturer aged the unit while it was at Intertek facility but report also states unit received by lab on 12/7/2015, report states manufacturer conducted 10 hours of preburn at high to medium burn rates from 11/10-12/2015",null,null,"Conditioning completed by","Manufacturer"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"indicates only 10 hours of preburn, 3030 minutes of conditioning data is reported on pg 80 of report, but does not include scale weight changes. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"3030 minutes of conditioning data is reported on pg 157 of report, but does not include scale weight changes. Compliance with medium burnrate requirement unable to be determined. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.7,1.17,0.75,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.7,1.17,0.75]
["Heat output (Btu/hr)",null,22266,15319,9575,null,null,null,22266,null,null,"Heat output (Btu/hr)",null,22266,15319,9575,null,null,null,22266]
["CO (g/min)",null,"NR","NR","NR",null,null,null,null,null,null,"CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,69.5,69.400000000000006,67.3,null,null,null,null,null,null,"HHV efficiency (%)",null,69.5,69.400000000000006,67.3]
["Overall PM emissions (g/hr)",1.119,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.119]
["PM 1-hr filter pull (g/hr)",1.29,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.29]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",10.73,null,null,null,null,null,null,null,null,null,"Train precision (%)",10.73]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","Not reported",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Other - specify →",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Other - specify →"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2015-12-07",null,null,null,null,null,null,null,null,null,"Test dates","2015-12-07"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be Determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be Determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,"Voltages for blower not stated in report",null,null,"check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,"Voltages for blower not stated in report"]
["Test location","Lab",null,null,null,null,null,null,"Middleton Wi",null,null,"Test location","Lab",null,null,null,null,null,null,"Middleton Wi"]
["date lab received the unit","2015-12-07",null,null,null,null,null,null,null,null,null,"date lab received the unit","2015-12-07"]
["date first day of conditioning","2015-11-10",null,null,null,null,null,null,null,null,null,"date first day of conditioning","2015-11-10"]
["date first day of testing","2015-12-07",null,null,null,null,null,null,null,null,null,"date first day of testing","2015-12-07"]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","not reported"]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used","other",null,null,null,null,null,null,"Gelman Aa/e 61631 47mm",null,null,"What type of filter used","other",null,null,null,null,null,null,"Gelman Aa/e 61631 47mm"]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negative values"]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,"Negative probe value","no negative values"]
["Negative room air values","no negative values",null,null,null,null,null,null,null,null,null,"Negative room air values","no negative values"]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,"Proportional sampling","not reported"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,"Leak check - any filter change","not reported"]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"mixing baffles shown on pg 10",null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"mixing baffles shown on pg 10"]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"see i23",null,null,"number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"see i23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,"lvl 5",null,"lvl 3",null,"lvl 1",null,null,null,null,null,null,"lvl 5",null,"lvl 3",null,"lvl 1"]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,"medium burn conditions met","not reported"]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,"high test settings match high in OM","not reported"]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,"run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate."]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-12-22","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2015-12-22","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2021-12-22",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-12-22"]

{"sheet":"Englander CAB80","index":35,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","England Stove Works Inc"]
["Model","25CAB80, 55-SHPCAB80, 55-TRPCAB80, 55-SHPCAB80S, 55-RPCAB80S",null,null,null,null,null,null,"4/18/18 similar models added"]
["Prelim review recomm.","Disapproved"]
["Red flags",10,"Orange flags",null,8,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: NR, IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"Tested at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1299999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.36]
["Overall HHV efficiency (%)",64.099999999999994]
["Overall heat output (Btu/hr)",13985,null,null,null,null,null,null,48000]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.74},null,"Overall CO (g/min)",null,null,2.9000000000000001E-2]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported",null,null,null,null,null,null,"unable to locate in report"]
["Burn rate calculations","Not reported",null,null,null,null,null,null,"unable to locate in report"]
["Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null," 2/19/2018 - only 10 hours of aging"]
["Conditioning data","Not reported",null,null,null,null,null,null,"unable to locate in report"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.63,1.1399999999999999,1.01]
["Heat output (Btu/hr)",null,20959,13310,11641,null,null,null,48000]
["CO (g/min)",null,2.9000000000000001E-2,3.5000000000000003E-2,2.5999999999999999E-2]
["HHV efficiency (%)",null,68.3,61.8,61.1]
["Overall PM emissions (g/hr)",1.1299999999999999]
["PM 1-hr filter pull (g/hr)",1.36]
["Filter data","Not reported"]
["Train precision (%)","Not reported"]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"No blower speed information"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marth pellets"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","All reported"]
["Test dates","2018-03-01"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2018-02-21",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2018-02-19",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2018-03-01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown on pg 7",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"see cell i42",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl m9",null,"lvl m2",null,"lvl m1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"How was run  1 valid, it did not meet medium burn rate requirements. ",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2018-06-18","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2023-06-18"]

{"sheet":"Englander CB120","index":36,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","England Stove Works Inc"]
["Model","25-CB120, 55-SHPCB120, 55-TRPCB120",null,null,null,null,null,null,"6/3/16 similar models added"]
["Prelim review recomm.","Disapproved"]
["Red flags",9,"Orange flags",null,6,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"conducted at intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.37,null,"PM Highest 1-hr (g/hr)",null,null,1.07]
["Overall HHV efficiency (%)",75.900000000000006]
["Overall heat output (Btu/hr)",13886]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":16.200000000000003},null,"Overall CO (g/min)",null,null,0.27]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received on 4/12/2016, only 10 hours of aging 4/4-6/2016"]
["Conditioning data","Not reported",null,null,null,null,null,null,"unable to find in report"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.72,0.88,0.78]
["Heat output (Btu/hr)",null,23466,11501,11993]
["CO (g/min)",null,0.3135,0.5383,9.0670000000000001E-2]
["HHV efficiency (%)",null,72.5,69.400000000000006,81.2]
["Overall PM emissions (g/hr)",1.37]
["PM 1-hr filter pull (g/hr)",1.07]
["Filter data","Reported"]
["Train precision (%)",4.26]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"marth pellets"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2016-04-19"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton,WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2016-04-12",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2016-04-04",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2016-04-19",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown on pg 11",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"Blower setting not mentioned in report and is adjustable according ot owners manual",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",null,"lvl 2",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2016-04-26","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2021-04-26"]

{"sheet":"Englander 25-CB PAH","index":37,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","England Stove Works Inc",null,null,null,null,null,null,null,null,null,"Manufacturer","England Stove Works Inc"]
["Model","25-CBPAH, 55-SHPCBPAH, 55-TRCBPAH",null,null,null,null,null,null," 55-SHPAH or 55-TRPAH also listed on manufacturers website but not in report, no updates to report. Possibly old report as EPA has listed a 25-CBPAH w/.76 g/hr emissions",null,null,"Model","25-CBPAH, 55-SHPCBPAH, 55-TRCBPAH",null,null,null,null,null,null," 55-SHPAH or 55-TRPAH also listed on manufacturers website but not in report, no updates to report. Possibly old report as EPA has listed a 25-CBPAH w/.76 g/hr emissions"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",4,"Orange flags",null,3,"Yellow flags",null,0,null,null,null,"Red flags",4,"Orange flags",null,3,"Yellow flags",null,0]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek facility",null,null,"Test Lab","Intertek",null,null,null,null,null,null,"performed at Intertek facility"]
["Third-party certifier","Intertek",null,null,null,null,null,null,null,null,null,"Third-party certifier","Intertek"]
["Report certified","Intertek",null,null,null,null,null,null,null,null,null,"Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.76300000000000001,null,"PM Highest 1-hr (g/hr)",null,null,1.9,null,null,null,null,"Overall PM emissions (g/hr)",0.76300000000000001,null,"PM Highest 1-hr (g/hr)",null,null,1.9]
["Overall HHV efficiency (%)",77.599999999999994,null,null,null,null,null,null,0.78,null,null,"Overall HHV efficiency (%)",77.599999999999994,null,null,null,null,null,null,0.78]
["Overall heat output (Btu/hr)",13,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":25740},null,"Overall CO (g/min)",null,null,429,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":25740},null,"Overall CO (g/min)",null,null,429]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"only 10 hours of aging",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"only 10 hours of aging"]
["Conditioning data","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning data","Not reported"]
["Lab technician notes","Not reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"H","M","L",null,null,null,null,null,null,"Run Category",null,"H","M","L"]
["Burn rate (kg/hr)",null,1.69,0.82,0.72,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.69,0.82,0.72]
["Heat output (Btu/hr)",null,10173,15709,20943,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,10173,15709,20943,null,null,null,48000]
["CO (g/min)",null,7.5999999999999998E-2,3.5999999999999997E-2,2.5999999999999999E-2,null,null,null,null,null,null,"CO (g/min)",null,7.5999999999999998E-2,3.5999999999999997E-2,2.5999999999999999E-2]
["HHV efficiency (%)",null,68.400000000000006,79.3,81.2,null,null,null,null,null,null,"HHV efficiency (%)",null,68.400000000000006,79.3,81.2]
["Overall PM emissions (g/hr)",0.76300000000000001,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.76300000000000001]
["PM 1-hr filter pull (g/hr)",1.9,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.9]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",0.91,null,null,null,null,null,null,null,null,null,"Train precision (%)",0.91]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","5/27-5/28/09",null,null,null,null,null,null,null,null,null,"Test dates","5/27-5/28/09"]
["30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes",null,null,null,null,null,null,"propsoed 5/14/2018",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,"propsoed 5/14/2018"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-05-10"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-05-07"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-05-14"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","not reported"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 Binder Free 47mm diameter"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","not reported"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","not reported"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","not reported"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","not reported"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Does not meet specification",null,null,null,null,null,null,"Shows mixing baffle in diagram pg 7 and noted in summary in pg 5"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",10]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data","-"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","-"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"see cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-09-24","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-09-24"]

{"sheet":"Englanders 25-CBEP","index":38,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","England Stove Works Inc"]
["Model","25-CBEP, 55-SHPCBEP, 55-TRPCBEP"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",8,"Orange flags",null,6,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: NR, IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"tested at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.03,null,"PM Highest 1-hr (g/hr)",null,null,1.25]
["Overall HHV efficiency (%)",63,null,null,null,null,null,null,0.63]
["Overall heat output (Btu/hr)",10194]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.02},null,"Overall CO (g/min)",null,null,1.7000000000000001E-2]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Partially reported",null,null,null,null,null,null,"Only six boxes of hole sheet filled in"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"unit recieved at testing facility 11/5/18"]
["Conditioning data","Not reported",null,null,null,null,null,null,"only 10 hours of aging reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.39,0.97,0.61]
["Heat output (Btu/hr)",null,15318,10535,7918,null,null,null,48000]
["CO (g/min)",null,0.10299999999999999,5.1999999999999998E-2,3.4000000000000002E-2]
["HHV efficiency (%)",null,58.6,57.5,69.3]
["Overall PM emissions (g/hr)",1.03]
["PM 1-hr filter pull (g/hr)",1.25]
["Filter data","Reported"]
["Train precision (%)",5.39]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"set to \"minimum feed rate level 1"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"marth pellets"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","All reported"]
["Test dates","2018-11-05"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2018-11-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2018-11-02",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2018-11-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 47mm",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 7 shows mixing baffles",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"m9",null,"m3",null,"m1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2019-03-13","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2024-03-13"]

{"sheet":"Englander 25-PDVC","index":39,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","England Stove Works Inc"]
["Model","25-PDVC, 25-PDVCH, 55-SHP10, 55-SHP10L, and 55-TRP10"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",6,"Orange flags",null,9,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"conducted at Intertek facility"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.43,null,"PM Highest 1-hr (g/hr)",null,null,"NR",null,"plugged filter 4 hours into run 1"]
["Overall HHV efficiency (%)",68.400000000000006]
["Overall heat output (Btu/hr)",14463]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":0},null,"Overall CO (g/min)",null,null,0]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Partially reported",null,null,null,null,null,null,"no data for run 1"]
["Burn rate calculations","Partially reported",null,null,null,null,null,null,"no data for run 1"]
["Raw data sheets","Partially reported",null,null,null,null,null,null,"only 6 boxes filled out on form and no raw data for run 1"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"only 10 hours of aging"]
["Conditioning data","Not reported"]
["Lab technician notes","Reported",null,null,null,null,null,null,"no data for run 1"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,1,1,1,"Run 1 filter plugged four hours in"]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.84,1.05,0.93,"NR","NR","NR"]
["Heat output (Btu/hr)",null,26179,12691,11220,"NR","NR","NR",48000]
["CO (g/min)",null,0,0,0,"NR","NR","NR"]
["HHV efficiency (%)",null,75.5,64.2,63.9,"NR","NR","NR"]
["Overall PM emissions (g/hr)",1.43]
["PM 1-hr filter pull (g/hr)",1.1359999999999999,null,null,null,null,null,null,"PM one hour only for run 2"]
["Filter data","Reported"]
["Train precision (%)",1.1200000000000001]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Level 1 was used for minimum feed rate"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Marthwood Pellets"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"does not include run 1"]
["All run data submitted","Partially reported",null,null,null,null,null,null,"does not include run 1"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2019-03-18"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2019-03-14",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2019-03-12",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2019-03-18",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free 47mm",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 7 shows mixing baffles",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 9",null,"lvl 3",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"medium burn rate is not less than 50% of max. burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2019-07-19","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2024-07-19"]

{"sheet":"Englander 25-SSP","index":40,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","England Stove Works Inc"]
["Model","25-SSP01,25-SSP01S,55-SHSSP01,55SHSSP01S, 55-TRSSP01, and 55TRSSP01S"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",8,"Orange flags",null,8,"Yellow flags",null,4]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"appears to be an outdated test"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.56399999999999995,null,"PM Highest 1-hr (g/hr)",null,null,"NR"]
["Overall HHV efficiency (%)",78.7]
["Overall heat output (Btu/hr)",15997]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":46.949999999999996},null,"Overall CO (g/min)",null,null,0.78249999999999997]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Not reported"]
["Conditioning data","Not reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.48,0.9,0.69]
["Heat output (Btu/hr)",null,36144,13079,10781]
["CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,77.099999999999994,77.3,78.3]
["Overall PM emissions (g/hr)",0.56399999999999995]
["PM 1-hr filter pull (g/hr)","NR"]
["Filter data","Reported"]
["Train precision (%)",6.52]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"burn setting level 1"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"no 1hr filter pull data"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2014-11-26"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Enviro M55","index":41,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Sherwood Industries Ltd dba Enviro",null,null,null,null,null,null,null,null,null,"Manufacturer","Sherwood Industries Ltd dba Enviro"]
["Model","M55 FS, M55C-FPI and Regency Greenfire – GC60, GCI60",null,null,null,null,null,null,null,null,null,"Model","M55 FS, M55C-FPI and Regency Greenfire – GC60, GCI60"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,4,"Yellow flags",null,8,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,8]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,null,null,null,"Test Lab","OMNI"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Aaron Kravitz)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Bruce Davis & Aaron Kravitz)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.82,null,"PM Highest 1-hr (g/hr)",null,null,1.1299999999999999,null,null,null,null,"Overall PM emissions (g/hr)",1.82,null,"PM Highest 1-hr (g/hr)",null,null,1.1299999999999999]
["Overall HHV efficiency (%)",60.4,null,null,null,null,null,null,0.60299999999999998,null,null,"Overall HHV efficiency (%)",60.4,null,null,null,null,null,null,0.60299999999999998]
["Overall heat output (Btu/hr)",8954,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",8954]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":18},null,"Overall CO (g/min)",null,null,0.3,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":18},null,"Overall CO (g/min)",null,null,0.3]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 3/9/2018, no mention of who conducted preburn or conditioning.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received on 3/9/2018, no mention of who conducted preburn or conditioning."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data does not include scale weight change or when fuel additions take place. Only date range (2/15-27/2018) no specific test dates included in conditioning data.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data does not include scale weight change or when fuel additions take place. Only date range (2/15-27/2018) no specific test dates included in conditioning data."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2,null,null,null,"Run #",null,1,1,1,2,2,2]
["Run Category",null,"High","Medium","Low","high ","med","low",null,null,null,"Run Category",null,"High","Medium","Low","high ","med","low","Two runs, first invalid due to proportionality issues. "]
["Burn rate (kg/hr)",null,1.69,0.71,0.4,1.86,0.74,0.43,null,null,null,"Burn rate (kg/hr)",null,1.69,0.71,0.4,1.86,0.74,0.43]
["Heat output (Btu/hr)",null,20388,6895,2895,23542,8406,4383,35700,null,null,"Heat output (Btu/hr)",null,20388,6895,2895,23542,8406,4383,35700]
["CO (g/min)",null,"NR","NR","NR",0.12,0.2,0.44,null,null,null,"CO (g/min)",null,"NR","NR","NR",0.12,0.2,0.44]
["HHV efficiency (%)",null,62.8,50.2,37.299999999999997,65.8,69.400000000000006,52.7,null,null,null,"HHV efficiency (%)",null,62.8,50.2,37.299999999999997,65.8,69.400000000000006,52.7]
["Overall PM emissions (g/hr)",1.82,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.82]
["PM 1-hr filter pull (g/hr)",1.1299999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.1299999999999999]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total pm catch",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total pm catch"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"set  to heat ouput setting 1 (min)",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"set  to heat ouput setting 1 (min)"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Blend",null,null,null,null,null,null,null,null,null,"Pellet species/type","Blend"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"small do not burn section",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"small do not burn section"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"did not include run 1",null,null,"Summary tables complete","Partially reported",null,null,null,null,null,null,"did not include run 1"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","3/12-3/14/2018",null,null,null,null,null,null,null,null,null,"Test dates","3/12-3/14/2018"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested in one day","Cannot Be Determined"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-03-09"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-02-15"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-03-12"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with deviation issues",null,null,null,null,null,null,"pgs 23 and 39 report shows deviation outside the allowable - showing ten minute averages of less than 90"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"See I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",5,"Medium",2,"Min",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,"run 1 invalidated due to proportionality issues. "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-11-30","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-11-30"]

{"sheet":"Enviro Mini P3","index":42,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Sherwood Industries Ltd dba Enviro",null,null,null,null,null,null,null,null,null,"Manufacturer","Sherwood Industries Ltd dba Enviro"]
["Model","Mini, P3 and Regency Greenfire – GF40",null,null,null,null,null,null,null,null,null,"Model","Mini, P3 and Regency Greenfire – GF40"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",4,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",4,"Orange flags",null,5,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,null,null,null,"Test Lab","OMNI"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.48,null,"PM Highest 1-hr (g/hr)",null,null,0.76,null,null,null,null,"Overall PM emissions (g/hr)",0.48,null,"PM Highest 1-hr (g/hr)",null,null,0.76]
["Overall HHV efficiency (%)",66.2,null,null,null,null,null,null,0.66200000000000003,null,null,"Overall HHV efficiency (%)",66.2,null,null,null,null,null,null,0.66200000000000003]
["Overall heat output (Btu/hr)",9330,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",9330]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":4.8},null,"Overall CO (g/min)",null,null,0.08,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":4.8},null,"Overall CO (g/min)",null,null,0.08]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 2/5/2018, no mention of who conducted conditioning or preburn.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 2/5/2018, no mention of who conducted conditioning or preburn."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data missing scale weight changes, and dates only state Jan 2018. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data missing scale weight changes, and dates only state Jan 2018. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative",null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative"]
["Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative",null,null,"Doc. of run burn rates","Partially reported",null,null,null,null,null,null,"not specifically addressed in run summary or other narrative"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.43,0.69,0.51,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.43,0.69,0.51]
["Heat output (Btu/hr)",null,19996,8097,6447,null,null,null,27700,null,null,"Heat output (Btu/hr)",null,19996,8097,6447,null,null,null,27700]
["CO (g/min)",null,0.03,0.1,0.08,null,null,null,null,null,null,"CO (g/min)",null,0.03,0.1,0.08]
["HHV efficiency (%)",null,72,60.4,65.5,null,null,null,null,null,null,"HHV efficiency (%)",null,72,60.4,65.5]
["Overall PM emissions (g/hr)",0.48,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.48]
["PM 1-hr filter pull (g/hr)",0.76,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.76]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"set to heat ouput setting 1(min)",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"set to heat ouput setting 1(min)"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn warnings throughout manual no specific improper fuel warning",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn warnings throughout manual no specific improper fuel warning"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-02-12",null,null,null,null,null,null,"unit recieved 2/5/18",null,null,"Test dates","2018-02-12",null,null,null,null,null,null,"unit recieved 2/5/18"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-02-05"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","January, 2018",null,null,null,null,null,null,"see I23"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-02-12"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",5,"Medium",2,"Min",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-11-30","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-11-30"]

{"sheet":"Enviro Meridian & GF55","index":43,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Sherwood Industries Ltd dba Enviro"]
["Model","Meridian-1, FPI, Cast Iron, GF55, GF155"]
["Prelim review recomm.","Disapproved"]
["Red flags",7,"Orange flags",null,4,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.89,null,"PM Highest 1-hr (g/hr)",null,null,0.81]
["Overall HHV efficiency (%)",69.7,null,null,null,null,null,null,0.69699999999999995]
["Overall heat output (Btu/hr)",11968]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 1/10/2018, no mention of who conducted conditioning or preburn."]
["Conditioning data","Not reported",null,null,null,null,null,null,"106 minutes of preburn on pg 15 of report, unable to located conditioning data in report."]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.75,0.85,0.62]
["Heat output (Btu/hr)",null,23765,10411,8894,null,null,null,33800]
["CO (g/min)",null,0.06,7.0000000000000007E-2,0.06]
["HHV efficiency (%)",null,70.2,63.5,74]
["Overall PM emissions (g/hr)",0.89]
["PM 1-hr filter pull (g/hr)",0.81]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"heat output set to 1 (min)"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn warnings throughout manual no specific improper fuel warning"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,"missing efficiency and burn rate calcs"]
["Owner manual complete","Partially reported minor"]
["Test dates","2018-01-11"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Enviro MAXX-1","index":44,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Sherwood Industries Ltd dba Enviro"]
["Model","MAXX-1"]
["Prelim review recomm.","Disapproved"]
["Red flags",5,"Orange flags",null,5,"Yellow flags",null,7]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: ES1, MD, IDU, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.865,null,"PM Highest 1-hr (g/hr)",null,null,7.7389999999999999]
["Overall HHV efficiency (%)",77.400000000000006,null,null,null,null,null,null,0.77400000000000002]
["Overall heat output (Btu/hr)",20861]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":68.399999999999991},null,"Overall CO (g/min)",null,null,1.1399999999999999]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 4/12/2018, no mention of who conducted preburn or conditioning."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Incomplete conditioning data lacks fuel addition as well as scale weight change. Unable to determine if conditioning was done at medium burn rate."]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2]
["Run Category",null,"High","Medium","Low","High","Medium","Low"]
["Burn rate (kg/hr)",null,"NR","NR","NR",3.26,1.2529999999999999,0.85199999999999998]
["Heat output (Btu/hr)",null,"NR","NR","NR",50627,19030,12190,63300]
["CO (g/min)",null,"NR","NR","NR",2.1800000000000002,0.87,0.96]
["HHV efficiency (%)",null,"NR","NR","NR",79.900000000000006,78,73.5]
["Overall PM emissions (g/hr)",1.865]
["PM 1-hr filter pull (g/hr)",7.7389999999999999]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total catch"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"heat output settign level 1 (min)"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"not specifically a improper fuel warning, but a do not burn list"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"run 1 not included"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2018-04-16"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","No"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly",null,null,null,null,null,null,null,"email sent to EPA unsure if test run 1 aborted for proper reasons.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"HRSW Chatham","index":45,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Sherwood Industries Ltd dba Hudson River Stove Works"]
["Model","EF2-1, Chatham-1, Davenport-1, and Kinderhook-1"]
["Prelim review recomm.","Disapproved"]
["Red flags",8,"Orange flags",null,8,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null," authorized signatories (Bruce Davis, Sebastian Button & Alex Tiegs)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.44,null,"PM Highest 1-hr (g/hr)",null,null,3.61]
["Overall HHV efficiency (%)",76.7,null,null,null,null,null,null,0.85]
["Overall heat output (Btu/hr)",14033]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":444},null,"Overall CO (g/min)",null,null,7.4]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Not reported"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.21,0.95,0.61]
["Heat output (Btu/hr)",null,32134,12655,8852,null,null,null,50000]
["CO (g/min)",null,22,8.4,2.2999999999999998]
["HHV efficiency (%)",null,78.7,71.8,"78..9"]
["Overall PM emissions (g/hr)",1.44]
["PM 1-hr filter pull (g/hr)",3.61]
["Filter data","Not reported"]
["Train precision (%)","Not reported"]
["Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"heat level 1, feed trim 1, combustion trim 2, air slide closed"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data"]
["Federal warning (C or NC)","Not Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported",null,null,null,null,null,null,"posted report only 10 pages"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"not data only summaries"]
["Owner manual complete","Partially reported minor"]
["Test dates","2016-07-15"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"SMG HP21","index":46,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","SMG Hearth & Home dba Comfortbilt"]
["Model","HP21"]
["Prelim review recomm.","Disapproved"]
["Red flags",11,"Orange flags",null,8,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: NR, IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.2649999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.87]
["Overall HHV efficiency (%)",78.8,null,null,null,null,null,null,0.83]
["Overall heat output (Btu/hr)",20630]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":8.2800000000000011},null,"Overall CO (g/min)",null,null,0.13800000000000001,null,"reported g/hr only"]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Partially reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received 6/4/2015, conditing is stated to have been conducted by both manufacuturer and lab."]
["Conditioning data","Not reported",null,null,null,null,null,null,"Report did not include preburn or conditioning data."]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,"All data sheets show as RUN 3?"]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,15.65,9.69,4.62]
["Heat output (Btu/hr)",null,33458,19540,14820,null,null,null,44000]
["CO (g/min)",null,"NR","NR","NR",null,null," ","co reported in g/hr - H=15.65, M=9.69, L=4.62"]
["HHV efficiency (%)",null,77.400000000000006,77.099999999999994,78.8]
["Overall PM emissions (g/hr)",1.2649999999999999]
["PM 1-hr filter pull (g/hr)",1.87]
["Filter data","Reported"]
["Train precision (%)",0.86]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Feed rate and exhaust setting not reported"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","All reported"]
["Test dates","2015-06-17"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot Be Determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-06-04",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-06-05",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-06-17",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","not reported",null,null,null,null,null,null,"Run is labeled as run 3 in documentation but not in summary",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing Baffles shown on pg 11",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",null,"lvl 2",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium was not less than 50% of maximum burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-06-29","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-06-29"]

{"sheet":"SMG HP22","index":47,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","SMG Hearth & Home dba Comfortbilt ",null,null,null,null,null,null,null,null,null,"Manufacturer","SMG Hearth & Home dba Comfortbilt "]
["Model"," ComfortBilt HP22N, HP22, and HP22i Insert",null,null,null,null,null,null,null,null,null,"Model"," ComfortBilt HP22N, HP22, and HP22i Insert"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,null,null,null,"Prelim review recomm."]
["Red flags",11,"Orange flags",null,9,"Yellow flags",null,3,null,null,null,"Red flags",11,"Orange flags",null,9,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination",null,null,null,null,"Date: 2/3/2022",null,null,"Basis: "]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Intertek"]
["Report certified","Not reported",null,null,null,null,null,null,null,null,null,"Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.9,null,"PM Highest 1-hr (g/hr)",null,null,1.87,null,null,null,null,"Overall PM emissions (g/hr)",1.542,null,"PM Highest 1-hr (g/hr)",null,null,0.81200000000000006]
["Overall HHV efficiency (%)",73.2,null,null,null,null,null,null,0.73199999999999998,null,null,"Overall HHV efficiency (%)",73.3,null,null,null,null,null,null,0.73199999999999998]
["Overall heat output (Btu/hr)",21162,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",23654]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":9.84},null,"Overall CO (g/min)",null,null,0.16400000000000001,null,null,null,null,"Overall CO (g/hr)",0,null,"Overall CO (g/min)",null,null,0]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Not reported"]
["Raw data sheets","Not reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Partially reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 5/5/2016, report states manufacturer conducted 10 hours of conditioning, also says Intertek staff conducted breakin period.",null,null,"Conditioning completed by","Lab"]
["Conditioning data","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning data","Not reported"]
["Lab technician notes","Not reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.64,1.66,1.08,null,null,null,null,null,null,"Burn rate (kg/hr)",null,3.09,2.25,1.0900000000000001]
["Heat output (Btu/hr)",null,36449,22579,14503,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,41810,29556,12987]
["CO (g/min)",null,0.245,0.17599999999999999,0.14099999999999999,null,null,null,null,null,null,"CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,73.2,72,71.3,null,null,null,null,null,null,"HHV efficiency (%)",null,75.8,73.7,66.900000000000006]
["Overall PM emissions (g/hr)",1.9,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.542]
["PM 1-hr filter pull (g/hr)",1.87,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.81200000000000006]
["Filter data","Not reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",1.1200000000000001,null,null,null,null,null,null,null,null,null,"Train precision (%)",1.05]
["Negative weights","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"feed rate and exhaust settings not reported"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,null,null,null,"Pellet species/type","Marthwood"]
["Pellet fuel certification","Not reported",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","bag"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Insufficient data",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete"]
["All run data submitted","Not reported",null,null,null,null,null,null,null,null,null,"All run data submitted","Partially reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2016-05-27",null,null,null,null,null,null,null,null,null,"Test dates","2020-04-13"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same","Cannot be determined"]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,"Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit","2016-05-05",null,null,null,null,null,null,null,null,null,"date lab received the unit","2020-03-28"]
["date first day of conditioning","2016-05-19",null,null,null,null,null,null,null,null,null,"date first day of conditioning","2020-04-01"]
["date first day of testing","2016-05-23",null,null,null,null,null,null,null,null,null,"date first day of testing","2020-04-13"]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters",null,null,"What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters"]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negative values"]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,"Negative probe value","no negative values"]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,"Negative room air values","not reported"]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,"Proportional sampling","not reported"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown on pg 7",null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown on pg 7"]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",10]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0]
["number of hours at correct conditioning conditions","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"Feed rate and air settings not reported",null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"see cell X42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,"Lvl 5",null,"Lvl 2",null,"Lvl 1",null,null,null,null,null,null,"lvl 5",null,"lvl 3",null,"lvl 1"]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,"medium burn conditions met","no"]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,"high test settings match high in OM","not reported",null,null,null,null,null,null,"feed rate and exhaust settings not reported"]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium was not less than 50% of maximum burn rate.",null,null,"run averaging done correctly","no",null,null,null,null,null,null,"Medium was not less than 50% of maximum burn rate."]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2017-03-21",null,null,null,null,null,null,null,null,null,"Compliance Date","2020-05-20","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2022-03-21",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-05-20"]

{"sheet":"SMG HP61","index":48,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","SMG Hearth & Home dba Comfortbilt"]
["Model","HP61"]
["Prelim review recomm.","Disapproved"]
["Red flags",12,"Orange flags",null,9,"Yellow flags",null,3]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: NR, IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.2110000000000001,null,"PM Highest 1-hr (g/hr)",null,null,2]
["Overall HHV efficiency (%)",83.4,null,null,null,null,null,null,0.84]
["Overall heat output (Btu/hr)",28224]
["Overall CO (g/hr)",7.38,null,"Overall CO (g/min)",null,null,{"$f":"B17/60","v":0.123},null,"CO reported in g/min "]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Partially reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received on 6/12/2015, report states manufacturer performed 50 hours of conditioning at high to medium burn rates, it also state Intertek conducted breakin period."]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.73,1.69,1.37]
["Heat output (Btu/hr)",null,42246,26424,21425,null,null,null,50000]
["CO (g/min)",null,"NR","NR","NR",null,null,null,"CO reported in g/min H-19.5, M-6.05, L-3.83"]
["HHV efficiency (%)",null,82,82.9,83.1]
["Overall PM emissions (g/hr)",1.2110000000000001]
["PM 1-hr filter pull (g/hr)",2]
["Filter data","Reported"]
["Train precision (%)",0.18]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Insufficient data"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"posted report only included 16 pages"]
["Owner manual complete","All reported"]
["Test dates","2015-06-18"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot Be Determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-06-12",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-06-15",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-06-18",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing Baffles shown on pg 11",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"feed rate and exhaust settings not reported",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",null,"lvl 2",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium was not less than 50% of maximum burn rate.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-06-26","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2020-06-26"]

{"sheet":"Travis Fox Fire","index":49,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31"]
["Model","Fox Fire",null,null,null,null,null,null,null,null,null,"Model","Fox Fire",null,null,null,null,null,null,null,null,null,"Model","Fox Fire"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,3,"Yellow flags",null,8,null,null,null,"Red flags",1,"Orange flags",null,3,"Yellow flags",null,8,null,null,null,"Red flags",1,"Orange flags",null,3,"Yellow flags",null,8]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.89500000000000002,null,"PM Highest 1-hr (g/hr)",null,null,3.4159999999999999,null,null,null,null,"Overall PM emissions (g/hr)",0.89500000000000002,null,"PM Highest 1-hr (g/hr)",null,null,3.4159999999999999,null,null,null,null,"Overall PM emissions (g/hr)",0.89500000000000002,null,"PM Highest 1-hr (g/hr)",null,null,3.4159999999999999]
["Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72,null,null,"Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72,null,null,"Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72]
["Overall heat output (Btu/hr)",16341,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16341,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16341]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.4870000000000001,1.069,0.82899999999999996,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4870000000000001,1.069,0.82899999999999996,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4870000000000001,1.069,0.82899999999999996]
["Heat output (Btu/hr)",null,38263,14214,10443,null,null,null,38263,null,null,"Heat output (Btu/hr)",null,38263,14214,10443,null,null,null,38263,null,null,"Heat output (Btu/hr)",null,38263,14214,10443,null,null,null,38263]
["CO (g/min)",null,0.55000000000000004,0.15,0.14000000000000001,null,null,null,null,null,null,"CO (g/min)",null,0.55000000000000004,0.15,0.14000000000000001,null,null,null,null,null,null,"CO (g/min)",null,0.55000000000000004,0.15,0.14000000000000001]
["HHV efficiency (%)",null,80.400000000000006,69.5,65.8,null,null,null,null,null,null,"HHV efficiency (%)",null,80.400000000000006,69.5,65.8,null,null,null,null,null,null,"HHV efficiency (%)",null,80.400000000000006,69.5,65.8]
["Overall PM emissions (g/hr)",0.89500000000000002,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.89500000000000002,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.89500000000000002]
["PM 1-hr filter pull (g/hr)",3.4159999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.4159999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.4159999999999999]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","Yes",null,null,null,null,null,null,"Train 2 had negative weight on rear filter catch",null,null,"Negative weights","Yes",null,null,null,null,null,null,"Train 2 had negative weight on rear filter catch",null,null,"Negative weights","Yes",null,null,null,null,null,null,"Train 2 had negative weight on rear filter catch"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-08-31",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-31",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-31"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested in one day","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested in one day","Cannot Be Determined"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR",null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported",null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/6/18 - 8/10/18",null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/6/18 - 8/10/18"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-31",null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-31"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported",null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives",null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives",null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","yes"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23",null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23",null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",10,"Medium",3,"Min",1,null,null,null,null,null,"Max",10,"Medium",3,"Min",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","no",null,null,null,null,null,null,"Instructions in report state restrictor set to full in for all runs and OM states that the restrictor may need adjustment for each output level."]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes",null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-11-28","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2018-11-28","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-11-02",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-11-02"]

{"sheet":"Travis Deerfield","index":50,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31"]
["Model","Deerfield",null,null,null,null,null,null,null,null,null,"Model","Deerfield",null,null,null,null,null,null,null,null,null,"Model","Deerfield"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,5,"Yellow flags",null,7,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,7,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.78500000000000003,null,"PM Highest 1-hr (g/hr)",null,null,2.6539999999999999,null,null,null,null,"Overall PM emissions (g/hr)",0.78500000000000003,null,"PM Highest 1-hr (g/hr)",null,null,2.6539999999999999,null,null,null,null,"Overall PM emissions (g/hr)",0.78500000000000003,null,"PM Highest 1-hr (g/hr)",null,null,2.6539999999999999]
["Overall HHV efficiency (%)",73.3,null,null,null,null,null,null,0.73299999999999998,null,null,"Overall HHV efficiency (%)",73.3,null,null,null,null,null,null,0.73299999999999998,null,null,"Overall HHV efficiency (%)",73.3,null,null,null,null,null,null,0.73299999999999998]
["Overall heat output (Btu/hr)",16126,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16126,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16126]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.4430000000000001,1.0249999999999999,0.8,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4430000000000001,1.0249999999999999,0.8,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4430000000000001,1.0249999999999999,0.8]
["Heat output (Btu/hr)",null,37391,13702,10652,null,null,null,35779,null,null,"Heat output (Btu/hr)",null,37391,13702,10652,null,null,null,35779,null,null,"Heat output (Btu/hr)",null,37391,13702,10652,null,null,null,35779]
["CO (g/min)",null,0.43,0.2,0.22,null,null,null,null,null,null,"CO (g/min)",null,0.43,0.2,0.22,null,null,null,null,null,null,"CO (g/min)",null,0.43,0.2,0.22]
["HHV efficiency (%)",null,79.900000000000006,69.8,69.599999999999994,null,null,null,null,null,null,"HHV efficiency (%)",null,79.900000000000006,69.8,69.599999999999994,null,null,null,null,null,null,"HHV efficiency (%)",null,79.900000000000006,69.8,69.599999999999994]
["Overall PM emissions (g/hr)",0.78500000000000003,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.78500000000000003,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.78500000000000003]
["PM 1-hr filter pull (g/hr)",2.6539999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.6539999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.6539999999999999]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain Brand"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-08-30",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-30",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-30"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR",null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported",null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/6/2018 - 8/10/2018",null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/6/2018 - 8/10/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-30",null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-30"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported",null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives",null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives",null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","yes"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23",null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23",null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max",10,"Medium",3,"Min",1,null,null,null,null,null,"Max",10,"Medium",3,"Min",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","no",null,null,null,null,null,null,"Instructions in report state restrictor set to full in for all runs and OM states that the restrictor may need adjustment for each output level."]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes",null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2020-10-14","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2020-10-14","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-10-14",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-10-14"]

{"sheet":"Travis AGP Insert","index":51,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31",null,null,"Manufacturer","Travis Industries, Inc",null,null,null,null,null,null,"2021-05-31"]
["Model","AGP Insert",null,null,null,null,null,null,null,null,null,"Model","AGP Insert",null,null,null,null,null,null,null,null,null,"Model","AGP Insert"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,null,null,null,"Test Lab","OMNI",null,null,null,null,null,null,null,null,null,"Test Lab","OMNI"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.97799999999999998,null,"PM Highest 1-hr (g/hr)",null,null,3.2730000000000001,null,null,null,null,"Overall PM emissions (g/hr)",0.97799999999999998,null,"PM Highest 1-hr (g/hr)",null,null,3.2730000000000001,null,null,null,null,"Overall PM emissions (g/hr)",0.97799999999999998,null,"PM Highest 1-hr (g/hr)",null,null,3.2730000000000001]
["Overall HHV efficiency (%)",75.599999999999994,null,null,null,null,null,null,0.75600000000000001,null,null,"Overall HHV efficiency (%)",75.599999999999994,null,null,null,null,null,null,0.75600000000000001,null,null,"Overall HHV efficiency (%)",75.599999999999994,null,null,null,null,null,null,0.75600000000000001]
["Overall heat output (Btu/hr)",14861,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14861,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14861]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Not reported"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Conditioning data shows fuel added but no change in scale weight to determine if medium burn rate was used."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.181,1.038,0.63400000000000001,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.181,1.038,0.63400000000000001,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.181,1.038,0.63400000000000001]
["Heat output (Btu/hr)",null,33686,15017,8320,null,null,null,34738,null,null,"Heat output (Btu/hr)",null,33686,15017,8320,null,null,null,34738,null,null,"Heat output (Btu/hr)",null,33686,15017,8320,null,null,null,34738]
["CO (g/min)",null,1.03,0.03,0.06,null,null,null,null,null,null,"CO (g/min)",null,1.03,0.03,0.06,null,null,null,null,null,null,"CO (g/min)",null,1.03,0.03,0.06]
["HHV efficiency (%)",null,80.7,75.599999999999994,68.5,null,null,null,null,null,null,"HHV efficiency (%)",null,80.7,75.599999999999994,68.5,null,null,null,null,null,null,"HHV efficiency (%)",null,80.7,75.599999999999994,68.5]
["Overall PM emissions (g/hr)",0.97799999999999998,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.97799999999999998,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.97799999999999998]
["PM 1-hr filter pull (g/hr)",3.2730000000000001,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.2730000000000001,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.2730000000000001]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Not included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-08-28",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-28",null,null,null,null,null,null,null,null,null,"Test dates","2018-08-28"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR",null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported",null,null,null,null,null,null,null,null,null,"date lab received the unit","Not Reported"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/1/2018 - 8/3/2018",null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/1/2018 - 8/3/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-28",null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-28"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no",null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no",null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no",null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported",null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives",null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives",null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives",null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification",null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","yes"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23",null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23",null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Max","Max","Medium","Max","Min","Max",null,null,null,null,null,"Max","Max","Medium","Max","Min","Max"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","yes"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","yes",null,null,null,null,null,null,null,null,null,"high test settings match high in OM","yes"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes",null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-12-13","No EPA Compliance Date",null,null,null,null,null,null,null,null,"Compliance Date","2018-12-13","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-12-30",null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-12-30"]

{"sheet":"Travis AGP PS","index":52,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Travis Industries, Inc"]
["Model","AGP PS"]
["Prelim review recomm.","Disapproved"]
["Red flags",{"$f":"1+SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":3},"Orange flags",null,5,"Yellow flags",null,6]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: ES1, IR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"testing location not specified"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"aurthorized signatories (Aaron Kravitz & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.8,null,"PM Highest 1-hr (g/hr)",null,null,8.1999999999999993]
["Overall HHV efficiency (%)",75.599999999999994,null,null,null,null,null,null,0.75600000000000001]
["Overall heat output (Btu/hr)",15677]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":18.600000000000001},null,"Overall CO (g/min)",null,null,0.31]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Not reported"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided only a range, cannot tell how many hours per day burned. Provides data on when fuel was added but not hourly burn rates so conformance with medium burn rate cannot be determined. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.27,1.1100000000000001,0.67]
["Heat output (Btu/hr)",null,34738,15937,8959,null,null,null,33686]
["CO (g/min)",null,1.21,0.12,0.15]
["HHV efficiency (%)",null,80,74.8,70]
["Overall PM emissions (g/hr)",1.8]
["PM 1-hr filter pull (g/hr)",8.1999999999999993]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"minimum dial setting"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Softwood",null,null,null,null,null,null,"Bear Mountain"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2018-08-29"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"True North 40","index":53,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Pacific Energy Fireplace Products Limited dba True North"]
["Model","TN40"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",10,"Orange flags",null,10,"Yellow flags",null,5]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, IR, NR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Other"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"original reviewer was able to find report on website, saved a 1 pg summary. Link to report location no longer active"]
["Report certified","Not reported",null,null,null,null,null,null,"unable to find full report"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.36,null,"PM Highest 1-hr (g/hr)",null,null,"NR"]
["Overall HHV efficiency (%)",72.150000000000006,null,null,null,null,null,null,0.78900000000000003]
["Overall heat output (Btu/hr)","NR"]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":"Not reported"},null,"Overall CO (g/min)",null,null,"NR"]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Not reported"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,2,3]
["Run Category",null,"Other","Other","Other"]
["Burn rate (kg/hr)",null,1.02,1.02,0.99]
["Heat output (Btu/hr)",null,"NR","NR","NR",null,null,null,40000]
["CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,65.3,71.099999999999994,72.2]
["Overall PM emissions (g/hr)",1.36]
["PM 1-hr filter pull (g/hr)","NR"]
["Filter data","Not reported"]
["Train precision (%)","Not reported"]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"does not include run 1 or 1 hr filter "]
["All run data submitted","Not reported"]
["Test report complete","Not reported",null,null,null,null,null,null,"no test reported posted on website found"]
["Owner manual complete","All reported"]
["Test dates","Cannot Be Determined",null,null,null,null,null,null,"1 page report is all that was found, summaries only"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Cannot Be Determined"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"USSC 4840","index":54,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[6,12,6,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","4840, KP500, AP5000",null,null,null,null,null,null,null,null,null,"Model","4840, KP500, AP5000",null,null,null,null,null,null,null,null,null,"Model","4840, KP500, AP5000"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,1,"Yellow flags",null,1,null,null,null,"Red flags",1,"Orange flags",null,1,"Yellow flags",null,1]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR ",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 10/20/2020",null,null,"Basis: MD, IR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 10/20/2020",null,null,"Basis: MD, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"The manufacturer states that the PFS-TECO is the third party certifier, and provided proof as certificate of conformity on Page 135 ",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"The manufacturer states that the proof of third party certifier is provided as certificate of conformity in the test report on 135",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.37,null,"PM Highest 1-hr (g/hr)",null,null,0.75,null,null,null,null,"Overall PM emissions (g/hr)",1.37,null,"PM Highest 1-hr (g/hr)",null,null,0.75,null,null,null,null,"Overall PM emissions (g/hr)",1.37,null,"PM Highest 1-hr (g/hr)",null,null,0.75]
["Overall HHV efficiency (%)",71.5,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",71.5,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",71.5]
["Overall heat output (Btu/hr)",8141,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",8141,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",8141]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":18.600000000000001},null,"Overall CO (g/min)",null,null,0.31,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":18.600000000000001},null,"Overall CO (g/min)",null,null,0.31,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":18.600000000000001},null,"Overall CO (g/min)",null,null,0.31]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"The manufacturer states that their staff completed the preburn and provides the info on page 5",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/24/2019",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/24/2019"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Manufacturer provides conditioning data on Page 19 of the report - in response manufacturer states that the data supplied meets the requirements of ASTM E2779 section 9.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data is missing scale readings and weight changes, regulations requires fuel addition info & scale weight is needed to confirm burn rate compliance. - Manufacturer supplied alternate conditioning table showing date & time, stack & ambient temps, and wieght of fuel added but still missing weight changes. Burn rate  is not able to be confirmed for compliance with medium burn setting requirements when lacking data for hourly wieght changes.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data is missing scale readings and weight changes, regulations requires fuel addition info & scale weight is needed to confirm burn rate compliance. - Manufacturer supplied alternate conditioning table showing date & time, stack & ambient temps, and wieght of fuel added but still missing weight changes. Burn rate  is not able to be confirmed for compliance with medium burn setting requirements when lacking data for hourly wieght changes."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,0.84,0.55000000000000004,0.53,null,null,null,"The manufacturer states that there is similarity between the low and the medium setting burn rates because the appliance has 5 heat level settings for medium burn rate. They povided a discussion on this on page 9 of the report - in an updated response manufacturer states that they \"attempted to obtain an ATM for this particular model but Mike Toney stated that an ATM was not required\"",null,null,"Burn rate (kg/hr)",null,0.84,0.55000000000000004,0.53,null,null,null,"ASTM 2779 section 9.4.1.2 requires Medium burn to be 50% of high burn rate. TEST METHOD NOT FOLLOWED. Did manufacturer obtain approval from EPA for ATM?",null,null,"Burn rate (kg/hr)",null,0.84,0.55000000000000004,0.53,null,null,null,"ASTM 2779 section 9.4.1.2 requires Medium burn to be 50% of high burn rate. TEST METHOD NOT FOLLOWED. Did manufacturer obtain approval from EPA for ATM?"]
["Heat output (Btu/hr)",null,12161,7571,7164,null,null,null,24000,null,null,"Heat output (Btu/hr)",null,12161,7571,7164,null,null,null,24000,null,null,"Heat output (Btu/hr)",null,12161,7571,7164,null,null,null,24000]
["CO (g/min)",null,0.17,0.35,0.32,null,null,null,null,null,null,"CO (g/min)",null,0.17,0.35,0.32,null,null,null,null,null,null,"CO (g/min)",null,0.17,0.35,0.32]
["HHV efficiency (%)",null,74.900000000000006,70.900000000000006,69.900000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,74.900000000000006,70.900000000000006,69.900000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,74.900000000000006,70.900000000000006,69.900000000000006]
["Overall PM emissions (g/hr)",1.37,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.37,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.37]
["PM 1-hr filter pull (g/hr)",0.75,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.75,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.75]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"The manufacturer states \"Precision as a percentage is not a directly reported value but individual train emissions difference from average (in both g and g/kg) is reported on the test results page for the test run, pages 36\". - Updated report shows train precision % as difference from Avg.",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"The manufacturer states that the lowest burn rate was performed at setting 1",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"The manufacturer states that the Fuel type is Bear Mountain Wood Pellets",null,null,"Pellet species/type","Reported",null,null,null,null,null,null,"Bear Mountain Wood Pellets",null,null,"Pellet species/type","Reported",null,null,null,null,null,null,"Bear Mountain Wood Pellets"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"The manufacturer provides information on items that are not to be burned on page 84",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2019-09-30",null,null,null,null,null,null,"received 7/24",null,null,"Test dates","2019-09-30",null,null,null,null,null,null,"received 7/24",null,null,"Test dates","2019-09-30",null,null,null,null,null,null,"received 7/24"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"Manufacturer provides evidence of the 30-day notification and proposed test date on page 136 of the updated test report",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"The 30-day notifcation, with proposed test date of week of September 30, 2019 confirms that test was conducted on the proposed date",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-07-24"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","8/6/2019 - 8/8/2019"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-09-30"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Train A front filter changed at I hr"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","reported/handled correctly",null,null,null,null,null,null,"-4% observed"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","reported/handled correctly",null,null,null,null,null,null,"-4% observed"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",1,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","no",null,null,null,null,null,null,"Medium was not less than 50% of maximum burn rate."]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,null,null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-12-19","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-12-19"]

{"sheet":"USSC SP24","index":55,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[48,12,48,18],[49,12,49,18],[50,12,50,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[61,12,61,18],[62,12,62,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[38,12,38,18],[39,12,39,18],[47,12,47,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[35,12,35,18],[36,12,36,18],[37,12,37,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell ",null,null,null,null,null,null,"2021-03-31"]
["Model","SP22(i), SP23(i), SP24(i),\nSP2000(i), AP2000(i), SP2700, SP4000,\nSPC4000, APC4000 and 5040(i)",null,null,null,null,null,null,null,null,null,"Model","SP22(i), SP23(i), SP24(i),\nSP2000(i), AP2000(i), SP2700, SP4000,\nSPC4000, APC4000 and 5040(i)",null,null,null,null,null,null,null,null,null,"Model","SP22(i), SP23(i), SP24(i),\nSP2000(i), AP2000(i), SP2700, SP4000,\nSPC4000, APC4000 and 5040(i)"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,6,"Yellow flags",null,4,null,null,null,"Red flags",1,"Orange flags",null,6,"Yellow flags",null,4,null,null,null,"Red flags",1,"Orange flags",null,6,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.75,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.75,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,"PM Highest 1-hr (g/hr)",null,null,0.75]
["Overall HHV efficiency (%)",62.6,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",62.6,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",62.6]
["Overall heat output (Btu/hr)",11234,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11234,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11234]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":4.2},null,"Overall CO (g/min)",null,null,7.0000000000000007E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 7/31/2018, no mention of who conducted preburn or conditioning. - updated report shows USSC conducted conditioning",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/31/2018",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/31/2018"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 19 of report and is missing specific dates, hours of testing on dates, and fuel additions. - updated report incldues fuel additions and date and times of testing.",null,null,"Conditioning data","Reported",null,null,null,null,null,null,null,null,null,"Conditioning data","Reported"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.4500000000000002,0.88,0.47,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4500000000000002,0.88,0.47,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4500000000000002,0.88,0.47]
["Heat output (Btu/hr)",null,32788,9881,4814,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,32788,9881,4814,null,null,null,50000,null,null,"Heat output (Btu/hr)",null,32788,9881,4814,null,null,null,50000]
["CO (g/min)",null,0.17,0.08,0.03,null,null,null,null,null,null,"CO (g/min)",null,0.17,0.08,0.03,null,null,null,null,null,null,"CO (g/min)",null,0.17,0.08,0.03]
["HHV efficiency (%)",null,69.599999999999994,58.8,53.7,null,null,null,null,null,null,"HHV efficiency (%)",null,69.599999999999994,58.8,53.7,null,null,null,null,null,null,"HHV efficiency (%)",null,69.599999999999994,58.8,53.7]
["Overall PM emissions (g/hr)",0.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.49]
["PM 1-hr filter pull (g/hr)",0.75,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.75,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.75]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Train precision calculatons and percentage are required, ADEC will not re-calculate unprovided equations to determine compliance. - updated report includes train precision shown was difference from Avg in %",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"heat setting 1 - Manufacturer states that Heat setting 1 is th lowest possible setting.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Manufactrure provided picture of pellet bag label",null,null,"Pellet species/type","Softwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Softwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-08-21",null,null,null,null,null,null,"aging 6/20, received 7/31",null,null,"Test dates","2018-08-21",null,null,null,null,null,null,"aging 6/20, received 7/31",null,null,"Test dates","2018-08-21",null,null,null,null,null,null,"aging 6/20, received 7/31"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"Manufacturer provided 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"Manufacturer provided 30 day notice",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-07-31"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","6/20/2018 - 6/22/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-08-21"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","reported/handled correctly"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","reported/handled correctly",null,null,null,null,null,null,-3.6999999999999998E-2]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-02-10","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-02-10"]

{"sheet":"USSC SP2047","index":56,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31"]
["Model","SP2047, GW7400",null,null,null,null,null,null,null,null,null,"Model","SP2047, GW7400",null,null,null,null,null,null,null,null,null,"Model","SP2047, GW7400"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,5,"Yellow flags",null,7,null,null,null,"Red flags",2,"Orange flags",null,5,"Yellow flags",null,7,null,null,null,"Red flags",2,"Orange flags",null,5,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Other (ATM)",null,null,null,null,null,null,"ATM - need to review - report indictes it is in",null,null,"Test method","Other (ATM)",null,null,null,null,null,null,"ATM - need to review - report indictes it is in",null,null,"Test method","Other (ATM)",null,null,null,null,null,null,"ATM - need to review - report indictes it is in"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"an appendix of the report but was not included",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"an appendix of the report but was not included",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"an appendix of the report but was not included"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer submittted COC ",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer submittted COC ",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.41,null,"PM Highest 1-hr (g/hr)",null,null,0.22,null,null,null,null,"Overall PM emissions (g/hr)",0.41,null,"PM Highest 1-hr (g/hr)",null,null,0.22,null,null,null,null,"Overall PM emissions (g/hr)",0.41,null,"PM Highest 1-hr (g/hr)",null,null,0.22]
["Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",74.599999999999994,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",74.599999999999994]
["Overall heat output (Btu/hr)",19339,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",19339,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",19339]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":21.599999999999998},null,"Overall CO (g/min)",null,null,0.36,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":21.599999999999998},null,"Overall CO (g/min)",null,null,0.36,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":21.599999999999998},null,"Overall CO (g/min)",null,null,0.36]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 10/19/2018, no mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 10/19/2018, no mention of who conducted preburn or conditioning. ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 10/19/2018, no mention of who conducted preburn or conditioning. "]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 67 of report and missing required data including dates, fuel additions, and weights for aging not reported",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Weight additions are listed and seems to have been overlooked by reviewer. - However it apprears this may have been flagged in regards to the 50 hr at med burn rate requirment. Review requires sufficient data to determine compliance with med burn rate requirement.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Weight additions are listed and seems to have been overlooked by reviewer. - However it apprears this may have been flagged in regards to the 50 hr at med burn rate requirment. Review requires sufficient data to determine compliance with med burn rate requirement."]
["Lab technician notes","Not reported",null,null,null,null,null,null,"Manufacturer refers reviewer to notes on pg 68 of the report",null,null,"Lab technician notes","Not reported",null,null,null,null,null,null,"Pg 68 is a one paragraph summary of use of the ATM and does not constitute lab notes for an entire certification test.",null,null,"Lab technician notes","Not reported",null,null,null,null,null,null,"Pg 68 is a one paragraph summary of use of the ATM and does not constitute lab notes for an entire certification test."]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.5099999999999998,1.21,1.1499999999999999,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.5099999999999998,1.21,1.1499999999999999,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.5099999999999998,1.21,1.1499999999999999]
["Heat output (Btu/hr)",null,33684,16871,16030,null,null,null,null,null,null,"Heat output (Btu/hr)",null,33684,16871,16030,null,null,null,35000,null,null,"Heat output (Btu/hr)",null,33684,16871,16030,null,null,null,35000]
["CO (g/min)",null,0.12,0.25,0.49,null,null,null,null,null,null,"CO (g/min)",null,0.12,0.25,0.49,null,null,null,null,null,null,"CO (g/min)",null,0.12,0.25,0.49]
["HHV efficiency (%)",null,72.3,75,75.2,null,null,null,null,null,null,"HHV efficiency (%)",null,72.3,75,75.2,null,null,null,null,null,null,"HHV efficiency (%)",null,72.3,75,75.2]
["Overall PM emissions (g/hr)",0.41,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.41,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.41]
["PM 1-hr filter pull (g/hr)",0.22,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.22,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.22]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states \"\tTrain precision is called out on page 85 as OK. Doing the math from the data on that same page will show better than 7.5% required.\"",null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,"ADEC has confirmed with EPA that train precision calculatons and percentage are required, ADEC will not re-calculate unprovided equations to determine compliance. ",null,null,"Train precision (%)","Not reported",null,null,null,null,null,null,"ADEC has confirmed with EPA that train precision calculatons and percentage are required, ADEC will not re-calculate unprovided equations to determine compliance. "]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close - Manufacturer states \"If it is set to full closed, that would be the “lowest setting”",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat pellet",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat pellet",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat pellet"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"Manfucturer refers reviewer to page 11 where a do not burn list exists but no specific improper fuel list",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-12-06",null,null,null,null,null,null,"received 10/19/18, why the delay in testing",null,null,"Test dates","2018-12-06",null,null,null,null,null,null,"received 10/19/18, why the delay in testing",null,null,"Test dates","2018-12-06",null,null,null,null,null,null,"received 10/19/18, why the delay in testing"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"manfucturer submitted 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"manfucturer submitted 30 day notice",null,null,"Tested on the proposed date","No",null,null,null,null,null,null,"Tested 4 days earlier",null,null,"Tested on the proposed date","No",null,null,null,null,null,null,"Tested 4 days earlier"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be Determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be Determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be Determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-10-19"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported",null,null,null,null,null,null,"The conditioning data does not have any dates"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-06"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High","Full open","Medium","1/32\" open","Low","Full closed"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-02-27","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-02-27"]

{"sheet":"USSC SP1000","index":57,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[67,1,67,7],[68,1,68,7],[69,1,69,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company dba Breckwell",null,null,null,null,null,null,"2021-03-31"]
["Model","SP1000",null,null,null,null,null,null,null,null,null,"Model","SP1000",null,null,null,null,null,null,null,null,null,"Model","SP1000"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,4,"Yellow flags",null,4,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,4,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IDU, IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,null,null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,null,null,null,"Test Lab","PFS-TECO"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer supplied COC",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer supplied COC",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.49,null,"PM Highest 1-hr (g/hr)",null,null,1.68,null,null,null,null,"Overall PM emissions (g/hr)",1.49,null,"PM Highest 1-hr (g/hr)",null,null,1.68,null,null,null,null,"Overall PM emissions (g/hr)",1.49,null,"PM Highest 1-hr (g/hr)",null,null,1.68]
["Overall HHV efficiency (%)",66.400000000000006,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",66.400000000000006,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",66.400000000000006]
["Overall heat output (Btu/hr)",11805,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11805,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11805]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":15},null,"Overall CO (g/min)",null,null,0.25]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 7/6/2018, no mention of who conducted conditioning or preburn. - Manufacturer stated preburn was conducted by USSC in June before being received at lab in July. ",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/6/2018",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 7/6/2018"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 19 of report and listed only one day of conditioning (6/8/2018) for aging. No data on specific dates or times of conditioning, temps appear to be low burn rates. - Updated report shows 3 days of conditioning (6/6-6/8). ",null,null,"Conditioning data","Reported",null,null,null,null,null,null,"Data  suggests that conditioning used low burn rate conditions rather than medium burn rate. ",null,null,"Conditioning data","Reported",null,null,null,null,null,null,"Data  suggests that conditioning used low burn rate conditions rather than medium burn rate. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.35,0.9,0.53,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.35,0.9,0.53,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.35,0.9,0.53]
["Heat output (Btu/hr)",null,31935,10620,5813,null,null,null,null,null,null,"Heat output (Btu/hr)",null,31935,10620,5813,null,null,null,47000,null,null,"Heat output (Btu/hr)",null,31935,10620,5813,null,null,null,47000]
["CO (g/min)",null,0.19,0.3,0.24,null,null,null,null,null,null,"CO (g/min)",null,0.19,0.3,0.24,null,null,null,null,null,null,"CO (g/min)",null,0.19,0.3,0.24]
["HHV efficiency (%)",null,73,63.66,59.2,null,null,null,null,null,null,"HHV efficiency (%)",null,73,63.66,59.2,null,null,null,null,null,null,"HHV efficiency (%)",null,73,63.66,59.2]
["Overall PM emissions (g/hr)",1.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.49,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.49]
["PM 1-hr filter pull (g/hr)",1.68,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.68,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.68]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states \"Page 28 states the precision was OK. Doing the math with the data on this page confirms this statement.\" - Updated report includes difference from Avg given in %",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes",null,null,null,null,null,null,null,null,null,"Negative weights","Yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from catch total - Manufacture response states \"The lab states the negative weights were dealt with appropriately and any issues would be the decision of EPA-OECA\"",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from catch total - ADEC is awaiting a determination from EPA on this issue",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from catch total - ADEC is awaiting a determination from EPA on this issue"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"heat setting 1, P60 NOTES AIR DAMPER PARTIALLY OPEN. - Manufacturer states \"The appliance can’t be set below 1\"",null,null,"Lowest burn rate tested","No",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","No",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat - corrected by entering \"hardwood\" which can be found on page 13 of the report",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-07-11",null,null,null,null,null,null,null,null,null,"Test dates","2018-07-11",null,null,null,null,null,null,null,null,null,"Test dates","2018-07-11"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"Manufacturer provided 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"Manufacturer provided 30 day notice",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-07-06"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-06-08"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-07-11"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium ",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-10-17","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-10-17"]

{"sheet":"United States Stove-5780 Series","index":58,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","5780, AP5780, VG5780, SP5780, and SP58",null,null,null,null,null,null,null,null,null,"Model","5780, AP5780, VG5780, SP5780, and SP58",null,null,null,null,null,null,null,null,null,"Model","5780, AP5780, VG5780, SP5780, and SP58"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,6,null,null,null,"Red flags",1,"Orange flags",null,5,"Yellow flags",null,6]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer supplied COC from OMNI",null,null,"Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer supplied COC from OMNI",null,null,"Report certified","Omni",null,null,null,null,null,null,null,null,null,"Report certified","Omni"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.3,null,"PM Highest 1-hr (g/hr)",null,null,2.5,null,null,null,null,"Overall PM emissions (g/hr)",1.3,null,"PM Highest 1-hr (g/hr)",null,null,2.5,null,null,null,null,"Overall PM emissions (g/hr)",1.3,null,"PM Highest 1-hr (g/hr)",null,null,2.5]
["Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72,null,null,"Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72,null,null,"Overall HHV efficiency (%)",72,null,null,null,null,null,null,0.72]
["Overall heat output (Btu/hr)",11704,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11704,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11704]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":12.6},null,"Overall CO (g/min)",null,null,0.21]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/6/2017, no mention of who conducted preburn or conditioning. - Manufacturer updated report to state that pre-burn was conducted by PFS",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/6/2017",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 3/6/2017"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 15 of report and missing required data including specific dates and weights for aging not reported - Time and fuel additions addin in updated report pg 18",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"In order to determine compliance ADEC requires scales weights on a 60 minute increment.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"In order to determine compliance ADEC requires scales weights on a 60 minute increment."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.79,0.68,0.64,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.79,0.68,0.64,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.79,0.68,0.64]
["Heat output (Btu/hr)",null,26386,9097,8507,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,26386,9097,8507,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,26386,9097,8507,null,null,null,48000]
["CO (g/min)",null,0.24,0.19,0.21,null,null,null,null,null,null,"CO (g/min)",null,0.24,0.19,0.21,null,null,null,null,null,null,"CO (g/min)",null,0.24,0.19,0.21]
["HHV efficiency (%)",null,76.7,69.400000000000006,69.2,null,null,null,null,null,null,"HHV efficiency (%)",null,76.7,69.400000000000006,69.2,null,null,null,null,null,null,"HHV efficiency (%)",null,76.7,69.400000000000006,69.2]
["Overall PM emissions (g/hr)",1.3,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.3,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.3]
["PM 1-hr filter pull (g/hr)",2.5,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.5,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.5]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer States \"On page 14 of the report, it shows the precision being “acceptable”. On the same page, when you do the math on emission, it is well within the 7.5% requirement.\" - updated report includes train precision and calculations on pg 16.",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"\"For this appliance, the only heat setting that produces a burn rate of lessthan 50% of the maximum burn rate is the low burn rate setting. Therefore, the medium burnrate segment was performed at the same heat setting as the low burn rate segment.\" -- Manufacturer states \"On page 33 of the report, it states that setting 1 was used for the lowest burn rate. Since the setting are only 1-5, 1 being the lowest, the appliance can’t go any lower.\"",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"no details reported",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"no details reported",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"no details reported"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported",null,null,null,null,null,null,"updated report included pellet bag labe on pg. 14 .",null,null,"Source of the pellet specification","Pellet bag label",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Pellet bag label"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"Manfucturer refers reviewer to page 11 where a do not burn list exists but no specific improper fuel list",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2017-04-10",null,null,null,null,null,null,null,null,null,"Test dates","2017-04-10",null,null,null,null,null,null,null,null,null,"Test dates","2017-04-10"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"manufacturer submitted 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"manufacturer submitted 30 day notice showing proposed test dates",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2017-03-06"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2/17/2017 - 2/22/2017"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2017-04-10"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",1,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2017-05-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2022-05-01"]

{"sheet":"United States Stove - 5770","index":59,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","5770, 5770i, VG5770, VG5770i, AP5770, AP5770i, DNMP577, DNMP577(i), 5790, VG5790, AP5790, and DNMP579 ",null,null,null,null,null,null,null,null,null,"Model","5770, 5770i, VG5770, VG5770i, AP5770, AP5770i, DNMP577, DNMP577(i), 5790, VG5790, AP5790, and DNMP579 ",null,null,null,null,null,null,null,null,null,"Model","5770, 5770i, VG5770, VG5770i, AP5770, AP5770i, DNMP577, DNMP577(i), 5790, VG5790, AP5790, and DNMP579 "]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",4,"Orange flags",null,5,"Yellow flags",null,8,null,null,null,"Red flags",4,"Orange flags",null,5,"Yellow flags",null,8,null,null,null,"Red flags",4,"Orange flags",null,5,"Yellow flags",null,8]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer submitted a COC issued by PFS",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer submitted a COC issued by PFS",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.85,null,"PM Highest 1-hr (g/hr)",null,null,1.19,null,null,null,null,"Overall PM emissions (g/hr)",0.85,null,"PM Highest 1-hr (g/hr)",null,null,1.19,null,null,null,null,"Overall PM emissions (g/hr)",0.85,null,"PM Highest 1-hr (g/hr)",null,null,1.19]
["Overall HHV efficiency (%)",70,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",70,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",70]
["Overall heat output (Btu/hr)",11980,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11980,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",11980]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 12/20/2017",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 12/20/2017",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Unit received by lab on 12/20/2017"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 20 of report and missing specific dates and hours of testing. No weight change given for hours when fuel is added. Majority of conditioning hours have a burn rate greater than average medium burn rate of 0.79 kg/hr +/-.5kg ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 20 of report and missing specific dates and hours of testing. No weight change given for hours when fuel is added. Majority of conditioning hours have a burn rate greater than average medium burn rate of 0.79 kg/hr +/-.5kg - Original reviewer stated no change in weight when fuel was added however, it appears this was an oversight.  Though this does not address issue regarding burn rate.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Located on pg 20 of report and missing specific dates and hours of testing. No weight change given for hours when fuel is added. Majority of conditioning hours have a burn rate greater than average medium burn rate of 0.79 kg/hr +/-.5kg - Original reviewer stated no change in weight when fuel was added however, it appears this was an oversight.  Though this does not address issue regarding burn rate."]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,3,3,3,null,null,null,"Run #",null,2,2,2,3,3,3,null,null,null,"Run #",null,2,2,2,3,3,3]
["Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low"]
["Burn rate (kg/hr)",null,1.41,0.92,0.63,1.36,0.66,0.69,null,null,null,"Burn rate (kg/hr)",null,1.41,0.92,0.63,1.36,0.66,0.69,null,null,null,"Burn rate (kg/hr)",null,1.41,0.92,0.63,1.36,0.66,0.69]
["Heat output (Btu/hr)",null,19344,13187,8592,18619,8830,9218,48000,null,null,"Heat output (Btu/hr)",null,19344,13187,8592,18619,8830,9218,48000,null,null,"Heat output (Btu/hr)",null,19344,13187,8592,18619,8830,9218,48000]
["CO (g/min)",null,0.63,0.19,0.24,0.61,0.37,0.38,null,null,null,"CO (g/min)",null,0.63,0.19,0.24,0.61,0.37,0.38,null,null,null,"CO (g/min)",null,0.63,0.19,0.24,0.61,0.37,0.38]
["HHV efficiency (%)",null,71,73.7,70.400000000000006,70.5,69.099999999999994,69.099999999999994,null,null,null,"HHV efficiency (%)",null,71,73.7,70.400000000000006,70.5,69.099999999999994,69.099999999999994,null,null,null,"HHV efficiency (%)",null,71,73.7,70.400000000000006,70.5,69.099999999999994,69.099999999999994]
["Overall PM emissions (g/hr)",0.85,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.85,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.85]
["PM 1-hr filter pull (g/hr)",1.19,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.19,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.19]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states that on page 69 of the report it states that train precision is ok and if you do the math from the data it proves it. - Updated report provided including train precision % difference",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","yes",null,null,null,null,null,null,null,null,null,"Negative weights","yes",null,null,null,null,null,null,null,null,null,"Negative weights","yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Heat setting 1, damper full closed. Manufacturer states that heat setting 1 is the lowest setting possible out of the 1-5 settings on the device.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"air damper set to full close, no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Not reported",null,null,null,null,null,null,"30 minutes of run 1 not reported - Manufacturer has added missing run 1 data to report and submitted to EPA",null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Pres-to-logs (western conifer)",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Pres-to-logs (western conifer)",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Pres-to-logs (western conifer)"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"Manufacturer States that the improper fuels warning is located on page 11 of owners manual, located here is a list of do not burn items.",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"not data for run 1 included",null,null,"Summary tables complete","All reported",null,null,null,null,null,null,"not data for run 1 included - data from run 1 is included in Appendix A of report and outlines that the run was stopped due to equipment malfunction 30 minutes into the run.",null,null,"Summary tables complete","All reported",null,null,null,null,null,null,"not data for run 1 included - data from run 1 is included in Appendix A of report and outlines that the run was stopped due to equipment malfunction 30 minutes into the run."]
["All run data submitted","Partially reported",null,null,null,null,null,null,"the 30 minutes of run 1 not reported",null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2/5-2/8/18",null,null,null,null,null,null,null,null,null,"Test dates","2/5-2/8/18",null,null,null,null,null,null,null,null,null,"Test dates","2/5-2/8/18"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"Manufacturer supplied 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"Manufacturer supplied 30 day notice showing proposed test dates",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2017-12-20"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","1/15/2018 - 1/26/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-02-05"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","yes",null,null,null,null,null,null,"Run 1 aborted about 30 minutes into test because of equipment malfunction"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed  on sample train at one hour for runs 2 and 3"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"See I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",3,null,null,null,null,null,null,"see I83"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","not reported",null,null,null,null,null,null,"Said to be contained in the Appendix C that is not included in the report"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-06-07","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-06-07"]

{"sheet":"United States Stove - 5660E","index":60,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","5660E, AP5660, AP5660L, AP5660PE and DNMP566",null,null,null,null,null,null,null,null,null,"Model","5660E, AP5660, AP5660L, AP5660PE and DNMP566"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",8,"Orange flags",null,3,"Yellow flags",null,7,null,null,null,"Red flags",8,"Orange flags",null,3,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni's facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni's facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz, Jared Sorenson & Ken Morgan)",null,null,"Report certified","Not reported",null,null,null,null,null,null,"authorized signatories (Aaron Kravitz, Jared Sorenson & Ken Morgan)"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.92,null,"PM Highest 1-hr (g/hr)",null,null,2.08,null,null,null,null,"Overall PM emissions (g/hr)",1.92,null,"PM Highest 1-hr (g/hr)",null,null,2.08]
["Overall HHV efficiency (%)",66.5,null,null,null,null,null,null,0.621,null,null,"Overall HHV efficiency (%)",66.5,null,null,null,null,null,null,0.621]
["Overall heat output (Btu/hr)",13316,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13316]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":0},null,"Overall CO (g/min)",null,null,0,null,"CO reported as \"below detection limit\" ",null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":0},null,"Overall CO (g/min)",null,null,0,null,"CO reported as \"below detection limit\" "]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Received by lab on 7/31/2015, no mention of who conducted preburn or conditioning.",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"Received by lab on 7/31/2015, no mention of who conducted preburn or conditioning."]
["Conditioning data","Not reported",null,null,null,null,null,null,"unable to locate in report",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"unable to locate in report"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.0099999999999998,1.1000000000000001,0.91,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.0099999999999998,1.1000000000000001,0.91]
["Heat output (Btu/hr)",null,22574,12848,10334,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,22574,12848,10334,null,null,null,48000]
["CO (g/min)",null,0,0,0,null,null,null,null,null,null,"CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,60.9,63.1,61.6,null,null,null,null,null,null,"HHV efficiency (%)",null,60.9,63.1,61.6]
["Overall PM emissions (g/hr)",1.92,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.92]
["PM 1-hr filter pull (g/hr)",2.08,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.08]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Not reported"]
["Negative weights","yes",null,null,null,null,null,null,null,null,null,"Negative weights","yes"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"heat rate 1, damper 1/4\" from closed",null,null,"Lowest burn rate tested","No",null,null,null,null,null,null,"heat rate 1, damper 1/4\" from closed"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","Pellet bag lable",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","Pellet bag lable"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn list ",null,null,"Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"do not burn list "]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"no actual # for CO",null,null,"Summary tables complete","Partially reported",null,null,null,null,null,null,"no actual # for CO"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2015-08-06",null,null,null,null,null,null,null,null,null,"Test dates","2015-08-06"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2015-07-31"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2015-08-06"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negative values"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negative values"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negative values"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negative values"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary","not reported ",null,null,null,null,null,null,"see I23"]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data","not reported ",null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","no"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","not reported",null,null,null,null,null,null,"Equipment for calibration listed, but no data and dates"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2020-05-28","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2025-05-28"]

{"sheet":"United States Stove - 5710 ","index":61,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","5710, AP5710, VG5710, 5501S, AP5501S, VG5501S",null,null,null,null,null,null,null,null,null,"Model","5710, AP5710, VG5710, 5501S, AP5501S, VG5501S",null,null,null,null,null,null,null,null,null,"Model","5710, AP5710, VG5710, 5501S, AP5501S, VG5501S"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,4,"Yellow flags",null,6,null,null,null,"Red flags",3,"Orange flags",null,4,"Yellow flags",null,6,null,null,null,"Red flags",3,"Orange flags",null,4,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni's facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni's facility",null,null,"Test Lab","OMNI",null,null,null,null,null,null,"performed at Omni's facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"manufacturer submitted COC  ",null,null,"Third-party certifier","OMNI",null,null,null,null,null,null,null,null,null,"Third-party certifier","OMNI"]
["Report certified","Not reported",null,null,null,null,null,null,"manufacturer submitted COC ",null,null,"Report certified","Omni",null,null,null,null,null,null,null,null,null,"Report certified","Omni"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.03,null,"PM Highest 1-hr (g/hr)",null,null,1.1100000000000001,null,null,null,null,"Overall PM emissions (g/hr)",1.03,null,"PM Highest 1-hr (g/hr)",null,null,1.1100000000000001,null,null,null,null,"Overall PM emissions (g/hr)",1.03,null,"PM Highest 1-hr (g/hr)",null,null,1.1100000000000001]
["Overall HHV efficiency (%)",68.53,null,null,null,null,null,null,0.68530000000000002,null,null,"Overall HHV efficiency (%)",68.53,null,null,null,null,null,null,0.68530000000000002,null,null,"Overall HHV efficiency (%)",68.53,null,null,null,null,null,null,0.68530000000000002]
["Overall heat output (Btu/hr)",10766,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",10766,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",10766]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":5.76},null,"Overall CO (g/min)",null,null,9.6000000000000002E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":5.76},null,"Overall CO (g/min)",null,null,9.6000000000000002E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":5.76},null,"Overall CO (g/min)",null,null,9.6000000000000002E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 2/12/2016, no mention of who completed preburn or conditioning. - manufacturer states that \"The Federal Register does not state we need to record who did the preburn, nor does this have to be part of the certification report.\" ",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"ADEC requires this information to confirm compliance with ASTM 2779 section 9.1",null,null,"Conditioning completed by","Not reported",null,null,null,null,null,null,"ADEC requires this information to confirm compliance with ASTM 2779 section 9.1"]
["Conditioning data","Not reported",null,null,null,null,null,null,"Unable to locate in report.- Manufacturer submitted preburn datawith revised report. Time and fuel additions addin in updated report pg 107",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"In order to determine compliance ADEC requires scales weights on a 60 minute increment.",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Updated report does though it includes fuel addition weights it does not include hourly weight changes "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.49,0.73,0.72,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.49,0.73,0.72,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.49,0.73,0.72]
["Heat output (Btu/hr)",null,20076,9279,8606,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,20076,9279,8606,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,20076,9279,8606,null,null,null,48000]
["CO (g/min)",null,0,0,0.19,null,null,null,null,null,null,"CO (g/min)",null,0,0,0.19,null,null,null,null,null,null,"CO (g/min)",null,0,0,0.19]
["HHV efficiency (%)",null,73.03,68.92,64.8,null,null,null,null,null,null,"HHV efficiency (%)",null,73.03,68.92,64.8,null,null,null,null,null,null,"HHV efficiency (%)",null,73.03,68.92,64.8]
["Overall PM emissions (g/hr)",1.03,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.03,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.03]
["PM 1-hr filter pull (g/hr)",1.1100000000000001,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.1100000000000001,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.1100000000000001]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer submitted a statement that \"Ken Morgan at OMNI went back and determined the precision at 5.48% and the limit is 7.5%\" - Train precision and calcualtions added to pg 89 of updated report.",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","yes",null,null,null,null,null,null,"train 1 rear filter (-.4)",null,null,"Negative weights","yes",null,null,null,null,null,null,"train 1 rear filter (-.4)",null,null,"Negative weights","yes",null,null,null,null,null,null,"train 1 rear filter (-.4)"]
["Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"subtracted from total"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"DAMPER REPORTED AS FULLY OPEN - Manufacturer states \"Page 93 of the report clearly states the low burn was on setting 1. The owner’s manual clearly states the settings for this run from 5 to 1 (highest to lowest)\"",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"DAMPER REPORTED AS FULLY OPEN - no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null," The updated report included this statement,  \"the burn setting for both low and medium was  set to position 1, this was required to achieve a burn rate less than 50% of high. To generate a low burn rate lower than the medium, the air damper was fully open. This is the lowest possible  setting allowed by user controls.\""]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"Manufacturer refers reviewer to page 11 of manual for improper fuels list. However it is labeled as do not burn.",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2016-02-23",null,null,null,null,null,null,null,null,null,"Test dates","2016-02-23",null,null,null,null,null,null,null,null,null,"Test dates","2016-02-23"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"Manufacturer states \"30 day notice was submitted, it is not part of the EPA Certification Report\" - updated report includes 30 day notice on pg 109.",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","No",null,null,null,null,null,null,"Propesed date was 2/22/2016",null,null,"Tested on the proposed date","No",null,null,null,null,null,null,"Propesed date was 2/22/2016"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same","Same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, Oregon"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-02-12"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2016-01-27"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2016-02-23"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes",null,null,null,null,null,null,"During max and medium burns"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change","not reported"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Unable to be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"setting 5","dampner open","setting 1 ","dampner closed ","setting 1 ","dampner open"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","yes"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"though calibration data is report some certificates are outside six months with at least one that was calibrated after the test was conducted and found to be out of calibration."]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-02-23","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-02-23"]

{"sheet":"United States Stove - KP60","index":62,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","King KP60, Ashley AP60, Vogelzang VG60",null,null,null,null,null,null,null,null,null,"Model","King KP60, Ashley AP60, Vogelzang VG60",null,null,null,null,null,null,null,null,null,"Model","King KP60, Ashley AP60, Vogelzang VG60"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,4,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,6,null,null,null,"Red flags",2,"Orange flags",null,4,"Yellow flags",null,6]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"performed at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"performed at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"performed at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,2.0099999999999998,null,null,null,null,"Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,2.0099999999999998,null,null,null,null,"Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,2.0099999999999998]
["Overall HHV efficiency (%)",66.2,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",66.2,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",66.2]
["Overall heat output (Btu/hr)",10800,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",10800,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",10800]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":17.399999999999999},null,"Overall CO (g/min)",null,null,0.28999999999999998,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":17.399999999999999},null,"Overall CO (g/min)",null,null,0.28999999999999998,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":17.399999999999999},null,"Overall CO (g/min)",null,null,0.28999999999999998]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"Unit received by lab on 3/21/2018, no mention of who completed preburn or conditioning. - updated report states that USSC did conditioning",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 3/21/2018",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 3/21/2018"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data missing specific dates for aging, also data for hours where fuel was added doesn't show weight changes prior to additions. 22 hours out of 50 do not seem to be at medium burn rate of .77 kg/hr +/-.5kg- updated report included datea and times ",null,null,"Conditioning data","Reported",null,null,null,null,null,null," 22 hours out of 50 do not seem to be at medium burn rate of .77 kg/hr +/-.5kg - ",null,null,"Conditioning data","Reported",null,null,null,null,null,null," 22 hours out of 50 do not seem to be at medium burn rate of .77 kg/hr +/-.5kg - "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.63,0.77,0.7,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.63,0.77,0.7,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.63,0.77,0.7]
["Heat output (Btu/hr)",null,20700,9192,8476,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,20700,9192,8476,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,20700,9192,8476,null,null,null,48000]
["CO (g/min)",null,0.2,0.34,0.27,null,null,null,null,null,null,"CO (g/min)",null,0.2,0.34,0.27,null,null,null,null,null,null,"CO (g/min)",null,0.2,0.34,0.27]
["HHV efficiency (%)",null,68.5,64.2,65.2,null,null,null,null,null,null,"HHV efficiency (%)",null,68.5,64.2,65.2,null,null,null,null,null,null,"HHV efficiency (%)",null,68.5,64.2,65.2]
["Overall PM emissions (g/hr)",1.46,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.46,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.46]
["PM 1-hr filter pull (g/hr)",2.0099999999999998,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.0099999999999998,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",2.0099999999999998]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states \"Train precision is reported on page 28 (24 of 35) of the non-CBI report.\" - The information on the page only states the train precision is OK and below the required 7.5%, equations & calcualtions not provided. - updated report includes train precision as difference from Avg in %",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","Yes",null,null,null,null,null,null,"rear filters on both trains",null,null,"Negative weights","Yes",null,null,null,null,null,null,"rear filters on both trains",null,null,"Negative weights","Yes",null,null,null,null,null,null,"rear filters on both trains"]
["Negs handled appropriately","No",null,null,null,null,null,null,"Subtracted, manufacturer feels that this was addressed by EPA.",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"ADEC is awaiting formal written clarification from the EPA regarding negative filter values.",null,null,"Negs handled appropriately","No",null,null,null,null,null,null,"ADEC is awaiting formal written clarification from the EPA regarding negative filter values."]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Medium and low heat segments are reported as having the same settings - Manufacturer states setting 1 is the lowest setting. However this does not address the medium burn settings being the same.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response. Manufacturer response does not address the medium burn settings being the same.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response. Manufacturer response does not address the medium burn settings being the same."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"Manfuacturer directs reviewer to Page 14 of the manual for the improper fuels - referred to as Do Not Burn ",null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2018-04-23",null,null,null,null,null,null,"recieved @ lab 3/21/18",null,null,"Test dates","2018-04-23",null,null,null,null,null,null,"recieved @ lab 3/21/18",null,null,"Test dates","2018-04-23",null,null,null,null,null,null,"recieved @ lab 3/21/18"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"updated report included 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"4/23-4/27",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-03-21"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","3/20/2018 - 4/19/2018"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-04-23"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",1,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","no",null,null,null,null,null,null,"Calibration data said to be in Appendix C that is not included in the report"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2018-07-18","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2023-07-19"]

{"sheet":"United States Stove - GW1949","index":63,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","GW1949, AP77, SW1117",null,null,null,null,null,null,null,null,null,"Model","GW1949, AP77, SW1117",null,null,null,null,null,null,null,null,null,"Model","GW1949, AP77, SW1117"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,5,"Yellow flags",null,4,null,null,null,"Red flags",3,"Orange flags",null,5,"Yellow flags",null,4,null,null,null,"Red flags",3,"Orange flags",null,5,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer provided COC ",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer provided COC ",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.94,null,"PM Highest 1-hr (g/hr)",null,null,3.37,null,null,null,null,"Overall PM emissions (g/hr)",0.94,null,"PM Highest 1-hr (g/hr)",null,null,3.37,null,null,null,null,"Overall PM emissions (g/hr)",0.94,null,"PM Highest 1-hr (g/hr)",null,null,3.37]
["Overall HHV efficiency (%)",69.3,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",69.3,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",69.3]
["Overall heat output (Btu/hr)",13286,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13286,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13286]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":27.6},null,"Overall CO (g/min)",null,null,0.46,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":27.6},null,"Overall CO (g/min)",null,null,0.46,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":27.6},null,"Overall CO (g/min)",null,null,0.46]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Not reported",null,null,null,null,null,null,"received @ lab 10/30/19, no mention of who conducted preburn (i.e. Lab, Manufacturer) or conditioning (i.e. Lab or Manufacturer). - updated report shows conditioning was conducted by USSC on 10/9-10/11",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Manufacturer"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data missing specific dates for aging, also data for hours where fuel was added doesn't show weight changes prior to additions. 40 hours out of 50 do not seem to be at avg medium burn rate of 1.532 kg/hr +/-.5kg - updated report includes dates and times. ",null,null,"Conditioning data","Reported",null,null,null,null,null,null," 40 hours out of 50 do not seem to be at avg medium burn rate of 1.532 kg/hr +/-.5kg",null,null,"Conditioning data","Reported",null,null,null,null,null,null," 40 hours out of 50 do not seem to be at avg medium burn rate of 1.532 kg/hr +/-.5kg"]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2,null,null,null,"Run #",null,1,1,1,2,2,2,null,null,null,"Run #",null,1,1,1,2,2,2]
["Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low",null,null,null,"Run Category",null,"High","Medium","Low","High","Medium","Low"]
["Burn rate (kg/hr)",null,1.91,1.1200000000000001,0.87,2.74,1.95,0.8,null,null,null,"Burn rate (kg/hr)",null,1.91,1.1200000000000001,0.87,2.74,1.95,0.8,null,null,null,"Burn rate (kg/hr)",null,1.91,1.1200000000000001,0.87,2.74,1.95,0.8]
["Heat output (Btu/hr)",null,23649,12835,10031,38544,26313,9762,48000,null,null,"Heat output (Btu/hr)",null,23649,12835,10031,38544,26313,9762,48000,null,null,"Heat output (Btu/hr)",null,23649,12835,10031,38544,26313,9762,48000]
["CO (g/min)",null,0.09,0.56999999999999995,0.43,2.0299999999999998,0.09,0.17,null,null,null,"CO (g/min)",null,0.09,0.56999999999999995,0.43,2.0299999999999998,0.09,0.17,null,null,null,"CO (g/min)",null,0.09,0.56999999999999995,0.43,2.0299999999999998,0.09,0.17]
["HHV efficiency (%)",null,64.7,59.6,60.1,72.8,70,63.5,null,null,null,"HHV efficiency (%)",null,64.7,59.6,60.1,72.8,70,63.5,null,null,null,"HHV efficiency (%)",null,64.7,59.6,60.1,72.8,70,63.5]
["Overall PM emissions (g/hr)",0.94,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.94,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.94]
["PM 1-hr filter pull (g/hr)",3.37,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.37,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.37]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Manufacturer states \"Page 39 shows that the train precision was ok and this can be confirmed by doing the math on the same page.\" - updated report provides Precision % in difference form average.",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Manufacturer states \"The low burn was achieved by the slide damper being fully open. This is noted in the report in the notes section. With this appliance, the lowest setting is with the slide damper fully open.\"",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"no information provided for fan/air flow settings. This issue has been forwarded to EPA per the decision matrix. ADEC will make a decision following receipt of formal EPA response."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","11/18-11/22/2019",null,null,null,null,null,null,null,null,null,"Test dates","11/18-11/22/2019",null,null,null,null,null,null,null,null,null,"Test dates","11/18-11/22/2019"]
["30 Day notice submitted to EPA","No",null,null,null,null,null,null,"manufacturer provided 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"manufacturer provided 30 day notice",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-10-30"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported",null,null,null,null,null,null,"Calibration data does not have any dates"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-11-18"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High",3,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",2]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","no",null,null,null,null,null,null,"question to EPA on run 1. Run 2 medium burn rate did not meet ASTM 2779 burn rate requirements to be less than 50% of maximum."]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration"]

{"sheet":"United States Stoves - 5520","index":64,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model",5520,null,null,null,null,null,null,null,null,null,"Model",5520]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Disapproved"]
["Red flags",5,"Orange flags",null,5,"Yellow flags",null,8,null,null,null,"Red flags",5,"Orange flags",null,5,"Yellow flags",null,8]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,null,null,null,"Test Lab","PFS-TECO"]
["Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,3.11,null,null,null,null,"Overall PM emissions (g/hr)",1.46,null,"PM Highest 1-hr (g/hr)",null,null,3.11]
["Overall HHV efficiency (%)",68.099999999999994,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",68.099999999999994]
["Overall heat output (Btu/hr)",14252,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14252]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":20.400000000000002},null,"Overall CO (g/min)",null,null,0.34,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":20.400000000000002},null,"Overall CO (g/min)",null,null,0.34]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 2/26/2015, only 10 hours of conditioning done at high to medium burn rates.",null,null,"Conditioning completed by","Manufacturer",null,null,null,null,null,null,"Unit received by lab on 2/26/2015, only 10 hours of conditioning done at high to medium burn rates."]
["Conditioning data","Not reported",null,null,null,null,null,null,"Cannot find any conditioning data. Preburn data found. 74 minutes of Preburn for run 1 located on pg 115 of report. 60 minutes of preburn for run 2 on pg 122. 70 minutes of preburn for run 3 on pg 130. 60 minutes for run 4 on pg 137. ",null,null,"Conditioning data","Not reported",null,null,null,null,null,null,"Cannot find any conditioning data. Preburn data found. 74 minutes of Preburn for run 1 located on pg 115 of report. 60 minutes of preburn for run 2 on pg 122. 70 minutes of preburn for run 3 on pg 130. 60 minutes for run 4 on pg 137. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported",null,null,null,null,null,null,"no mention of run validity",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,"no mention of run validity"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,"no metion of run anomalies",null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,"no metion of run anomalies"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"H","M","L",null,null,null,null,null,null,"Run Category",null,"H","M","L"]
["Burn rate (kg/hr)",null,2.52,0.91,0.72,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.52,0.91,0.72]
["Heat output (Btu/hr)",null,37379,11215,8506,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,37379,11215,8506,null,null,null,48000]
["CO (g/min)",null,0.3,0.41,0.31,null,null,null,null,null,null,"CO (g/min)",null,0.3,0.41,0.31]
["HHV efficiency (%)",null,76.7,64,61,null,null,null,null,null,null,"HHV efficiency (%)",null,76.7,64,61]
["Overall PM emissions (g/hr)",1.46,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.46]
["PM 1-hr filter pull (g/hr)",3.11,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",3.11]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Reported ",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported "]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions heat range of low(1) at 0.9 Ibs/hr feed rate",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions heat range of low(1) at 0.9 Ibs/hr feed rate"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Bear Mountain",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"Bear Mountain"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","from an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","from an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","Partially reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","3/3/15 - 3/4/15",null,null,null,null,null,null,null,null,null,"Test dates","8/29/19 - 8/29/19"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","No",null,null,null,null,null,null,null,null,null,"Tested in one day","No"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2019-08-13"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-08-29"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Run 1 aborted about 30 minutes into test because of equipment malfunction"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",4,"Medium",1,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","yes"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-12-19","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-12-19"]

{"sheet":"United States Stove - KP130","index":65,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,23,106,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[5,23,5,26],[5,27,5,29],[6,23,6,29],[106,12,106,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[105,1,105,7],[106,1,106,7],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31",null,null,"Manufacturer","United States Stove Company",null,null,null,null,null,null,"2021-03-31"]
["Model","KP130, AP130, VG130, 5502M, 5500, 5500M, and 5500XL",null,null,null,null,null,null,null,null,null,"Model","KP130, AP130, VG130, 5502M, 5500, 5500M, and 5500XL",null,null,null,null,null,null,null,null,null,"Model","KP130, AP130, VG130, 5502M, 5500, 5500M, and 5500XL"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"0+SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":0},"Orange flags",null,2,"Yellow flags",null,6,null,null,null,"Red flags",{"$f":"0+SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":0},"Orange flags",null,2,"Yellow flags",null,6,null,null,null,"Red flags",{"$f":"0+SUMPRODUCT((X14=\"NR\")+(X14=\"Not reported\")+(AC14=\"NR\")+(AC14=\"Not reported\")) +COUNTIF(X14,\">2\")+COUNTIF(AC14,\">6\")+COUNTIF(X18:AD28,\"=Not reported\")+SUMPRODUCT((X36=\"NR\")+(X36=\"Not reported\")+(X37=\"NR\")+(X37=\"Not reported\")+(X38=\"Not reported\")+(X41=\"No\")+(X42=\"No\")+(X43=\"Not reported\"))+IFERROR(IF(INDEX(Y32:AD32,1,MATCH(\"High\",Y31:AD31,0))*0.5<INDEX(Y32:AD32,1,MATCH(\"Medium\",Y31:AD31,0)),1,0),0)+IFERROR(IF(INDEX(Y32:AD32,1,MATCH(\"Low\",Y31:AD31,0))<>MIN(Y32:AD32),1,0),0)","v":0},"Orange flags",null,2,"Yellow flags",null,6]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility",null,null,"Test Lab","PFS-TECO",null,null,null,null,null,null,"tested at PFS facility"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Third-party certifier","PFS-TECO",null,null,null,null,null,null,null,null,null,"Third-party certifier","PFS-TECO"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer submitted COC",null,null,"Report certified","PFS-TECO",null,null,null,null,null,null,null,null,null,"Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.27,null,"PM Highest 1-hr (g/hr)",null,null,1.91,null,null,null,null,"Overall PM emissions (g/hr)",1.27,null,"PM Highest 1-hr (g/hr)",null,null,1.91,null,null,null,null,"Overall PM emissions (g/hr)",1.27,null,"PM Highest 1-hr (g/hr)",null,null,1.91]
["Overall HHV efficiency (%)",63.7,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",63.7,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",63.7]
["Overall heat output (Btu/hr)",12905,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",12905,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",12905]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(AC17*60,\"Not reported\")","v":24.599999999999998},null,"Overall CO (g/min)",null,null,0.41]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,null,null,null,"Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"specific dates of aging not provided. 50 hours at medium burn rate confirmed. - manufacturer states \"If you review Section 9.1.4 of ASTM E2779 it states to record the time and weight.\" implying the date is not required - updated report provides dates and time of conditioning.",null,null,"Conditioning data","Reported",null,null,null,null,null,null," Data is provided in 15 minute increments. Need one hour burn rate data to determine conformance with medium burn rate requirements. ",null,null,"Conditioning data","Reported",null,null,null,null,null,null," Data is provided in 15 minute increments. Need one hour burn rate data to determine conformance with medium burn rate requirements. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run appropriateness","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report"]
["Doc. of run validity","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run validity","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report",null,null,"Doc. of run anomolies","Reported",null,null,null,null,null,null,"Reported on Page 8 of the report"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.17,1.06,0.75,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.17,1.06,0.75,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.17,1.06,0.75]
["Heat output (Btu/hr)",null,25701,12083,8932,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,25701,12083,8932,null,null,null,48000,null,null,"Heat output (Btu/hr)",null,25701,12083,8932,null,null,null,48000]
["CO (g/min)",null,0.22,0.49,0.42,null,null,null,null,null,null,"CO (g/min)",null,0.22,0.49,0.42,null,null,null,null,null,null,"CO (g/min)",null,0.22,0.49,0.42]
["HHV efficiency (%)",null,63.8,61.2,64,null,null,null,null,null,null,"HHV efficiency (%)",null,63.8,61.2,64,null,null,null,null,null,null,"HHV efficiency (%)",null,63.8,61.2,64]
["Overall PM emissions (g/hr)",1.27,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.27,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.27]
["PM 1-hr filter pull (g/hr)",1.91,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.91,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.91]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)","Not reported",null,null,null,null,null,null,"Only reported as OK - Manufacturer states \"On page 20 it states ok and the data is on the same page. By doing the math, the precision fell well with the 7.5% range.\" - updated report includes train precision % given in difference from Avg ",null,null,"Train precision (%)","Reported",null,null,null,null,null,null,null,null,null,"Train precision (%)","Reported"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions low burn rate settings: HR-1 but does not mention other controls fan, damper, etc. ",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions low burn rate settings: HR-1 but does not mention other controls fan, damper, etc. ",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions low burn rate settings: HR-1 but does not mention other controls fan, damper, etc. "]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat",null,null,"Pellet species/type","Hardwood",null,null,null,null,null,null,"purHeat"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported",null,null,null,null,null,null,null,null,null,"Owner manual complete","All reported"]
["Test dates","2019-02-04",null,null,null,null,null,null,null,null,null,"Test dates","2019-02-04",null,null,null,null,null,null,null,null,null,"Test dates","2019-02-04"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"manufacturer submitted 30 day notice",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"manufacturer submitted 30 day notice showing proposed dates",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Yes"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Portland, OR"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-12-04"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","Not Reported ",null,null,null,null,null,null,"The conditioning data does not have any dates"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2019-02-04"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","yes",null,null,null,null,null,null,"Front filters changed on sample A at one hour after the test began"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","reported/handled correctly"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","reported/handled correctly",null,null,null,null,null,null,-1.4E-2]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"High ",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"Although calibration data is reported certifications are outside the 6 month requirement"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-05-15"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-05-29"]

{"sheet":"Enerco Group - PSBF66W","index":66,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group, Inc."]
["Model","PSBF66W"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,4,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"Report, on page 2, mentions that this report does not constitute certification of this product nor an opinion or endorsement by this laboratory. "]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.18,null,"PM Highest 1-hr (g/hr)",null,null,0.87]
["Overall HHV efficiency (%)",82.2,null,null,null,null,null,null,0.82199999999999995]
["Overall heat output (Btu/hr)",21022]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.2},null,"Overall CO (g/min)",null,null,0.02]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 11/28/18 through 11/29/18 on med and high burn rate"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. see note in cell above. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.64,0.88,0.48]
["Heat output (Btu/hr)",null,40259,13421,7420,null,null,null,52000]
["CO (g/min)",null,0.11799999999999999,3.9E-2,0.02]
["HHV efficiency (%)",null,80.7,81,82.6]
["Overall PM emissions (g/hr)",1.18]
["PM 1-hr filter pull (g/hr)","Not reported"]
["Filter data","Reported"]
["Train precision (%)",6.3,null,null,null,null,null,null,"Reported as 6.30% deviation"]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"the heater was changed to the minimum feed rate (level 4) with a burn rate of 1.0 kg/h"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Other - specify →"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"reported as do not burn garbage or flammable fluids such as gasoline, naphtha or engine"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2018-12-12"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"LMF B-100","index":67,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","LMF Manufacturing Ltd dba America's Heat"]
["Model","America's Heat B-100"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",7,"Orange flags",null,7,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.7390000000000001,null,"PM Highest 1-hr (g/hr)",null,null,2]
["Overall HHV efficiency (%)",57.8]
["Overall heat output (Btu/hr)",12050]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":17.009999999999998},null,"Overall CO (g/min)",null,null,0.28349999999999997]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Report states 10 hours of greak in at medium to high burn rate. No data provided. "]
["Conditioning data","Not reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.65,1.1499999999999999,0.89]
["Heat output (Btu/hr)",null,18773,12102,9098]
["CO (g/min)",null,7.43,14.02,23.51]
["HHV efficiency (%)",null,60.2,55.9,53.9]
["Overall PM emissions (g/hr)",1.7390000000000001]
["PM 1-hr filter pull (g/hr)",2]
["Filter data","Not reported"]
["Train precision (%)",6.79,null,null,null,null,null,null,"Reported as the dilution tunnel dual train precision on page 7 of the report"]
["Negative weights","Not reported"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","No",null,null,null,null,null,null,"Report mentions that at 12:01 pm, the heater was changed to the minimum feed rate (level #3) with a burn rate of 0.94 kg/hr"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Other - specify →"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,"It is a 15-page test report"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-12-12"]
["30 Day notice submitted to EPA","No"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be Determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-12-09",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-12-14",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-12-15",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 10 shows mixing baffle",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot Be Determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no",null,null,null,null,null,null,"lvl 3 was used",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 7",null,"lvl5",null,"lvl 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output. ",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-12-21"]
["DEC Calculated Certification Expiration","2020-12-21"]

{"sheet":"Ravelli - RV100 Classic","index":68,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Ravelli ",null,null,null,null,null,null,null,null,null,"Manufacturer","Ravelli "]
["Model","RV100 Classic",null,null,null,null,null,null,null,null,null,"Model","RV100 Classic"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,"original recommendation from different report of model of the same name.",null,null,"Prelim review recomm.","Disapproved",null,null,null,null,null,null,"original recommendation from different report of model of the same name."]
["Red flags",1,"Orange flags",null,9,"Yellow flags",null,7,null,null,null,"Red flags",1,"Orange flags",null,9,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IDU, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Polytests Inc.",null,null,null,null,null,null,null,null,null,"Test Lab","Polytests Inc."]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,null,null,null,"Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,0.67,null,null,null,null,"Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,0.67]
["Overall HHV efficiency (%)",80.2,null,null,null,null,null,null,0.875,null,null,"Overall HHV efficiency (%)",80.2,null,null,null,null,null,null,0.875]
["Overall heat output (Btu/hr)",16900,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",16900]
["Overall CO (g/hr)",2.72,null,"Overall CO (g/min)",null,null,4.4999999999999998E-2,null,null,null,null,"Overall CO (g/hr)",2.72,null,"Overall CO (g/min)",null,null,4.4999999999999998E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard.",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness",null,null,"Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity",null,null,"Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,1,null,null,null,null,null,"Run #",null,1,1,1,1]
["Run Category",null,"High","Medium","Low","overall",null,null,null,null,null,"Run Category",null,"High","Medium","Low","overall"]
["Burn rate (kg/hr)",null,2.31,1.1200000000000001,0.68,1.1000000000000001,null,null,null,null,null,"Burn rate (kg/hr)",null,2.31,1.1200000000000001,0.68,1.1000000000000001]
["Heat output (Btu/hr)",null,34500,17400,10750,16900,null,null,44000,null,null,"Heat output (Btu/hr)",null,34500,17400,10750,16900,null,null,44000]
["CO (g/min)",null,5.8999999999999997E-2,6.3E-2,4.9000000000000002E-2,4.4999999999999998E-2,null,null,null,null,null,"CO (g/min)",null,5.8999999999999997E-2,6.3E-2,4.9000000000000002E-2,4.4999999999999998E-2]
["HHV efficiency (%)",null,77.97,80.8,82.1,80.2,null,null,null,null,null,"HHV efficiency (%)",null,77.97,80.8,82.1,80.2]
["Overall PM emissions (g/hr)",0.7,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.7]
["PM 1-hr filter pull (g/hr)",0.67,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.67]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",0.39,null,null,null,null,null,null,"Reported as 0.39% on page 8 as the dilution tunnel dual train precision",null,null,"Train precision (%)",0.39,null,null,null,null,null,null,"Reported as 0.39% on page 8 as the dilution tunnel dual train precision"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"for the last portion of the test the pellet stove is set at power 1 for 3hours of minimum burn rate.",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"for the last portion of the test the pellet stove is set at power 1 for 3hours of minimum burn rate."]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hotzpellets",null,null,null,null,null,null,null,null,null,"Pellet species/type","Hotzpellets"]
["Pellet fuel certification","NR",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","NR"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Not Included",null,null,null,null,null,null,null,null,null,"Stack height","Not Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Included",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Included"]
["Fuel selection recomm.","Insufficient data",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Insufficient data"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Not included",null,null,null,null,null,null,null,null,null,"Replacement parts","Not included"]
["Federal warning (C or NC)","Not Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Not Included"]
["Warranty rights","Not Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Not Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported major"]
["Test dates","2016-05-25",null,null,null,null,null,null,null,null,null,"Test dates","2016-05-25"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"St-jean-sur-Richelieu QC, Canada J3B 7S7"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-05-02"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2016-05-17"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2016-05-25"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes",null,null,null,null,null,null,"see I23"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","not reported"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","no negatives"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","no negatives"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",50]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",0,null,null,null,null,null,null,"see I23"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see I23"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"High",5,"Medium",2,"Low",1]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","no",null,null,null,null,null,null,"Calibration data, including dates not found"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-06-01","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-06-01"]

{"sheet":"Ravelli - RV80","index":69,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Ravelli"]
["Model","Monica 2015, Francesca 2015, RV80 CERAMICA"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,6,"Yellow flags",null,7]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Polytests Inc."]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.57999999999999996,null,"PM Highest 1-hr (g/hr)",null,null,1.36]
["Overall HHV efficiency (%)",77.87,null,null,null,null,null,null,0.82]
["Overall heat output (Btu/hr)",14993]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":22.8},null,"Overall CO (g/min)",null,null,0.38]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.79,1.08,0.71]
["Heat output (Btu/hr)",null,34000,20500,13400,null,null,null,35000]
["CO (g/min)",null,0.44,0.52,0.35]
["HHV efficiency (%)",null,77.180000000000007,77.180000000000007,78.97]
["Overall PM emissions (g/hr)",0.57999999999999996]
["PM 1-hr filter pull (g/hr)",1.36]
["Filter data","Reported"]
["Train precision (%)","Reported ",null,null,null,null,null,null,"Reported on page 8 as the dilution tunnel dual train precision"]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Report mentions that for the last portion of the test the pellet stove is set at power for 3 hours of minimum burn rate"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Not included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2015-06-23"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot Be Determined",null,null,null,null,null,null,"Air/pellet settings not included in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"695-B Gaudette St-jean-sur-Richelieu QC, Canada J3B 7S7",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-03-15",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-06-01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-06-21",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","reported and handled correctly",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",59,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"See Cell I23",null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,5,null,3,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06"]
["Compliance Date","2015-08-30"]
["DEC Calculated Certification Expiration","2020-11-30"]

{"sheet":"Enerco Group - PS130W","index":70,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group, Inc."]
["Model","PS130W"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",2,"Orange flags",null,2,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Not reported"]
["Report certified","Intertek",null,null,null,null,null,null,"Report certified by Charles Meyers"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.5960000000000001,null,"PM Highest 1-hr (g/hr)",null,null,0.92]
["Overall HHV efficiency (%)",75.8,null,null,null,null,null,null,0.75800000000000001]
["Overall heat output (Btu/hr)",18250]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.6199999999999999},null,"Overall CO (g/min)",null,null,2.7E-2]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 11/28/18 through 11/29/18 on med and high burn rate"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,"no mention of run validity"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"no mention of run anomalies"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,2.59,1.22,1]
["Heat output (Btu/hr)",null,34129,13535,16714]
["CO (g/min)",null,0.16,0.08,5.2999999999999999E-2]
["HHV efficiency (%)",null,73.2,75.3,76]
["Overall PM emissions (g/hr)",1.5960000000000001]
["PM 1-hr filter pull (g/hr)",0.92]
["Filter data","Reported"]
["Train precision (%)",8.16,null,null,null,null,null,null,"Reported deviation % under as dilution tunnel dual train precision "]
["Negative weights","No"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"the heater was changed to the minimum feed rate (level 4) with a burn rate of 1.00 kg/hr"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Other - specify →",null,null,null,null,null,null,"Wood pellets used for the testing were manufactured by Marthwood."]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2018-12-10"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2018-11-16",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2018-11-28",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2018-12-10",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman 47mm",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown in diagram on pg 7 and described on pg 6",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","no",null,null,null,null,null,null,"OM shows 4 settings 1-4 4 being minimum",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"Level 1",null,"Level 2",null,"level 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2019-04-25","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2024-04-25"]

{"sheet":"Sierra Products - EasyFire","index":71,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Sierra Product, Inc."]
["Model","EasyFire Pellet Stove, EF3801, EF5001, EF4001"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",3,"Orange flags",null,7,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Other"]
["Third-party certifier","PFS-TECO"]
["Report certified","PFS-TECO",null,null,null,null,null,null,"Report mentions that the test report was reviewed and authorized by Daniel Shoman of PFS Corporation"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.82299999999999995,null,"PM Highest 1-hr (g/hr)",null,null,0.84799999999999998]
["Overall HHV efficiency (%)",63.6,null,null,null,null,null,null,0.78500000000000003]
["Overall heat output (Btu/hr)",11376]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":33.6},null,"Overall CO (g/min)",null,null,0.56000000000000005]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.49,1.07,0.7]
["Heat output (Btu/hr)",null,17732,12233,7943]
["CO (g/min)",null,0.34,0.59,0.69]
["HHV efficiency (%)",null,63.3,61.1,60.7]
["Overall PM emissions (g/hr)",0.82299999999999995]
["PM 1-hr filter pull (g/hr)",0.84799999999999998]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","Yes"]
["Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Not included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Insufficient data",null,null,null,null,null,null,"No mention of specific type of pellet"]
["Improper fuels warnings","Insufficient data",null,null,null,null,null,null,"the report suggests that different brands of pellets should be tried until clean effcient burn is found "]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,"Though it is difficult to find federal warning specifically, different types of warnings are included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported major"]
["Test dates","2016-10-21"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Colviille WA",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2016-09-15",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2016-10-03",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2016-10-21",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","no",null,null,null,null,null,null,"front ",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","not reported",null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing baffles shown on pg 24",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,"unable to locate in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2017-01-24"]
["DEC Calculated Certification Expiration","2022-04-27"]

{"sheet":"Enerco Group - PS60W","index":72,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[106,12,106,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Enerco Group, Inc.",null,null,null,null,null,null,null,null,null,"Manufacturer","Enerco Group, Inc."]
["Model","PS60W",null,null,null,null,null,null,null,null,null,"Model","PS60W"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"0+SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":2},"Orange flags",null,{"$f":"SUMPRODUCT((B15=\"NR\")+(B15=\"Not reported\")+(B16=\"NR\")+(B16=\"Not reported\")+(G17=\"NR\")+(G17=\"Not reported\"))+COUNTIF(B18:H28,\"=Partially reported\")+COUNTIF(B30:B35,\"=Not reported\")+SUMPRODUCT((B39=\"Not reported\")+(B40=\"NR\")+(B40=\"Not reported\")+(B41=\"Cannot be determined\")+(B42=\"Cannot be determined\"))+COUNTIF(B45:B47,\"Not reported\")+COUNTIF(B49:B61,\"Not included\")+COUNTIF(B63:B67,\"Not reported\")+COUNTIF(B63:B67,\"=NR\")+COUNTIF(B63:B67,\"Partially reported major\")+COUNTIF(B68:B71,\"=No\")","v":2},"Yellow flags",null,{"$f":"COUNTIF(B9:H12,\"=Not reported\")+COUNTIF(B30:B35,\"=Partially reported\")+COUNTIF(B49:B61,\"Insufficient data\")+COUNTIF(B63:B67,\"Partially reported\")+COUNTIF(B63:B67,\"Partially reported minor\")++COUNTIF(B68:B71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},null,null,null,"Red flags",{"$f":"0+SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":2},"Orange flags",null,{"$f":"SUMPRODUCT((M15=\"NR\")+(M15=\"Not reported\")+(M16=\"NR\")+(M16=\"Not reported\")+(R17=\"NR\")+(R17=\"Not reported\"))+COUNTIF(M18:S28,\"=Partially reported\")+COUNTIF(M30:M35,\"=Not reported\")+SUMPRODUCT((M39=\"Not reported\")+(M40=\"NR\")+(M40=\"Not reported\")+(M41=\"Cannot be determined\")+(M42=\"Cannot be determined\"))+COUNTIF(M45:M47,\"Not reported\")+COUNTIF(M49:M61,\"Not included\")+COUNTIF(M63:M67,\"Not reported\")+COUNTIF(M63:M67,\"=NR\")+COUNTIF(M63:M67,\"Partially reported major\")+COUNTIF(M68:M71,\"=No\")","v":2},"Yellow flags",null,{"$f":"COUNTIF(M9:S12,\"=Not reported\")+COUNTIF(M30:M35,\"=Partially reported\")+COUNTIF(M49:M61,\"Insufficient data\")+COUNTIF(M63:M67,\"Partially reported\")+COUNTIF(M63:M67,\"Partially reported minor\")++COUNTIF(M68:M71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}}]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,null,null,null,"Third-party certifier","Not reported"]
["Report certified","Not reported",null,null,null,null,null,null,"Report mentions that this report does not constitute certification of this product nor an opinion or endorsement by this laboratory.",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Report mentions that this report does not constitute certification of this product nor an opinion or endorsement by this laboratory."]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.995,null,"PM Highest 1-hr (g/hr)",null,null,0.83699999999999997,null,null,null,null,"Overall PM emissions (g/hr)",0.995,null,"PM Highest 1-hr (g/hr)",null,null,0.83699999999999997]
["Overall HHV efficiency (%)",82.3,null,null,null,null,null,null,0.82299999999999995,null,null,"Overall HHV efficiency (%)",82.3,null,null,null,null,null,null,0.82299999999999995]
["Overall heat output (Btu/hr)",13317,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",13317]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":1.02},null,"Overall CO (g/min)",null,null,1.7000000000000001E-2,null,null,null,null,"Overall CO (g/hr)",{"$f":"IFERROR(R17*60,\"Not reported\")","v":1.02},null,"Overall CO (g/min)",null,null,1.7000000000000001E-2]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 11/28/18 through 11/29/18 on med and high burn rate",null,null,"Conditioning completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 11/28/18 through 11/29/18 on med and high burn rate"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. ",null,null,"Conditioning data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,"no mention of run validity",null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,"no mention of run validity"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,"None specifically mentioned ",null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,"None specifically mentioned "]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Medium","Low",null,null,null,null,null,null,"Run Category",null,"High","Medium","Low"]
["Burn rate (kg/hr)",null,1.73,0.8,0.61,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.73,0.8,0.61]
["Heat output (Btu/hr)",null,26865,12297,9265,null,null,null,34000,null,null,"Heat output (Btu/hr)",null,26865,12297,9265,null,null,null,34000]
["CO (g/min)",null,0.1,0.05,3.3000000000000002E-2,null,null,null,null,null,null,"CO (g/min)",null,0.1,0.05,3.3000000000000002E-2]
["HHV efficiency (%)",null,82.2,81.7,81,null,null,null,null,null,null,"HHV efficiency (%)",null,82.2,81.7,81]
["Overall PM emissions (g/hr)",0.995,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.995]
["PM 1-hr filter pull (g/hr)",0.83699999999999997,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",0.83699999999999997]
["Filter data","Reported",null,null,null,null,null,null,null,null,null,"Filter data","Reported"]
["Train precision (%)",6.93,null,null,null,null,null,null,"Reported as 6.93% deviation",null,null,"Train precision (%)",6.93,null,null,null,null,null,null,"Reported as 6.93% deviation"]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"the heater was changed to the minimum feed rate (level 4) with a burn rate of 0.64 kg/h",null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"the heater was changed to the minimum feed rate (level 4) with a burn rate of 0.64 kg/h"]
["All run data","Reported",null,null,null,null,null,null,null,null,null,"All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Other - specify →",null,null,null,null,null,null,"Marthwood",null,null,"Pellet species/type","Other - specify →",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","PFI",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","PFI"]
["Source of the pellet specification","From an analyzed sample",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low","Included",null,null,null,null,null,null,null,null,null,"Proper operation low","Included"]
["Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts","Included",null,null,null,null,null,null,null,null,null,"Replacement parts","Included"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,null,null,null,"Owner manual complete","Partially reported minor"]
["Test dates","2018-12-11",null,null,null,null,null,null,null,null,null,"Test dates","2018-12-11"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot Be Determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Yes",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same","Cannot be determined"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2018-11-16"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2018-11-28"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2018-12-11"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","not reported"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","no"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","not reported"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters."]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","no negatives"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","no negatives"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","not reported"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change","Meets Specification"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Does not meet specification",null,null,null,null,null,null,"Mixing baffle shown on pg 7"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary","Cannot be determined"]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data","Cannot be determined"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"refer to cell I42"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,"level 1",null,"Level 2",null,"Level 4"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met","not reported"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM","not reported"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"calibration certificates start on pg 96 of report, although included some are outside the 6 month requirement."]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2019-04-25","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2024-04-25"]

{"sheet":"Heat Tech - HTP 26 Bay","index":73,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Heat Tech Industries, LLC."]
["Model","HTP 26 Bay, HTP26 Bay Pedestal/Insert"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,12,"Yellow flags",null,4]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Other"]
["Third-party certifier","Not reported"]
["Report certified","Other",null,null,null,null,null,null,"By Alben T. Myren Jr. of Myren Consulting, Inc. on 1/13/16"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.3845000000000001,null,"PM Highest 1-hr (g/hr)",null,null,0.36]
["Overall HHV efficiency (%)",69.7]
["Overall heat output (Btu/hr)",13081]
["Overall CO (g/hr)",{"$f":"IFERROR(G17*60,\"Not reported\")","v":"Not reported"},null,"Overall CO (g/min)",null,null,"Not reported",null,"No overall data. However, CO data was recorded for both vaiable runs conducted for 60 minute and 360 minutes, respectively "]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1]
["Run Category",null,"Other","High"]
["Burn rate (kg/hr)",null,1,1.8]
["Heat output (Btu/hr)",null,13081,22998,null,null,null,null,40000]
["CO (g/min)",null,0.224,0.1055]
["HHV efficiency (%)",null,69.7,68.099999999999994]
["Overall PM emissions (g/hr)",1.3845000000000001]
["PM 1-hr filter pull (g/hr)",0.36]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","Yes"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,"Lost filter material accounted for in acetone catch"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,"Efficiency, fuel info, and replacement part missing"]
["Test dates","2015-07-30"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot be determined",null,null,null,null,null,null,"The notice, however, mentions that test will start during the period beginning on 7/27/2015"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Heat Tech - HTP 26 Standard","index":74,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Heat Tech Industries, LLC."]
["Model","HTP 26 Standard"]
["Prelim review recomm.","Requires a more thorough review"]
["Red flags",1,"Orange flags",null,11,"Yellow flags",null,5]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Other"]
["Third-party certifier","Not reported"]
["Report certified","Other",null,null,null,null,null,null,"By Alben T. Myren Jr. of Myren Consulting, Inc. on 1/11/16"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.9675,null,"PM Highest 1-hr (g/hr)",null,null,0.27400000000000002]
["Overall HHV efficiency (%)",66.400000000000006]
["Overall heat output (Btu/hr)",10762]
["Overall CO (g/hr)","Not reported",null,"Overall CO (g/min)",null,null,"Not reported",null,"No overall data. However, CO data was recorded for both vaiable runs conducted for 60 minute and 360 minutes, respectively "]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"No mention of run appropriateness"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"No mention of run validity"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1]
["Run Category",null,"H","M","L","FULL RUN"]
["Burn rate (kg/hr)",null,null,null,null,1.8]
["Heat output (Btu/hr)",null,null,null,null,24244,null,null,40000]
["CO (g/min)",null,null,null,null,0.105]
["HHV efficiency (%)",null,null,null,null,68.099999999999994]
["Overall PM emissions (g/hr)",1.9675]
["PM 1-hr filter pull (g/hr)",0.27400000000000002]
["Filter data","Reported"]
["Train precision (%)","Not reported"]
["Negative weights","Yes"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,"Lost filter material accounted for in acetone catch"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","From an analyzed sample"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Not included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor",null,null,null,null,null,null,"Efficiency, fuel info, and replacement parts missing"]
["Test dates","2015-07-28"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Cannot Be Determined",null,null,null,null,null,null,"The notice, however, mentions that test will start during the period beginning on 7/27/2015"]
["Tested in one day","Yes"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Colville WA",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2015-06-20",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2015-07-01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2015-07-28",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","yes with allowable deviations",null,null,null,null,null,null,"Item K on pg 18 (mixing baffles has been X out",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,"unable to locate air settings in report",null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2015-12-26"]
["DEC Calculated Certification Expiration","2020-12-26"]

{"sheet":"LIA Pellet Stove","index":75,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,23,102,29],[103,23,103,29],[104,23,104,29],[105,23,105,29],[106,23,106,29],[95,23,95,29],[96,23,96,29],[97,23,97,29],[98,23,98,29],[99,23,99,29],[100,22,101,22],[100,23,100,24],[100,25,100,26],[100,27,100,28],[86,23,86,29],[87,23,87,29],[88,23,88,29],[89,23,89,29],[90,23,90,29],[91,23,91,29],[92,23,92,29],[93,23,93,29],[94,23,94,29],[77,23,77,29],[78,23,78,29],[79,23,79,29],[80,23,80,29],[81,23,81,29],[82,23,82,29],[83,23,83,29],[84,23,84,29],[85,23,85,29],[68,23,68,29],[69,23,69,29],[70,23,70,29],[71,23,71,29],[72,23,72,29],[73,23,73,29],[74,23,74,29],[75,23,75,29],[76,23,76,29],[59,23,59,29],[60,23,60,29],[61,23,61,29],[62,23,62,29],[63,23,63,29],[64,23,64,29],[65,23,65,29],[66,23,66,29],[67,23,67,29],[50,23,50,29],[51,23,51,29],[52,23,52,29],[53,23,53,29],[54,23,54,29],[55,23,55,29],[56,23,56,29],[57,23,57,29],[58,23,58,29],[42,23,42,29],[43,23,43,29],[44,23,44,29],[44,30,46,30],[45,23,45,29],[46,23,46,29],[47,23,47,29],[48,23,48,29],[49,23,49,29],[27,23,27,29],[28,23,28,29],[35,23,35,29],[36,23,36,29],[37,23,37,29],[38,23,38,29],[39,23,39,29],[40,23,40,29],[41,23,41,29],[18,23,18,29],[19,23,19,29],[20,23,20,29],[21,23,21,29],[22,23,22,29],[23,23,23,29],[24,23,24,29],[25,23,25,29],[26,23,26,29],[13,23,13,24],[13,25,13,27],[13,28,13,29],[14,23,14,29],[15,23,15,29],[16,23,16,24],[16,25,16,27],[16,28,16,29],[17,23,17,29],[5,23,5,26],[5,27,5,29],[6,23,6,29],[7,23,7,29],[8,23,8,29],[9,23,9,29],[10,23,10,29],[11,23,11,29],[12,23,12,29],[102,12,102,18],[103,12,103,18],[104,12,104,18],[105,12,105,18],[106,12,106,18],[95,12,95,18],[96,12,96,18],[97,12,97,18],[98,12,98,18],[99,12,99,18],[100,11,101,11],[100,12,100,13],[100,14,100,15],[100,16,100,17],[86,12,86,18],[87,12,87,18],[88,12,88,18],[89,12,89,18],[90,12,90,18],[91,12,91,18],[92,12,92,18],[93,12,93,18],[94,12,94,18],[77,12,77,18],[78,12,78,18],[79,12,79,18],[80,12,80,18],[81,12,81,18],[82,12,82,18],[83,12,83,18],[84,12,84,18],[85,12,85,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[71,12,71,18],[72,12,72,18],[73,12,73,18],[74,12,74,18],[75,12,75,18],[76,12,76,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[42,12,42,18],[43,12,43,18],[44,12,44,18],[44,19,46,19],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[5,12,5,15],[5,16,5,18],[6,12,6,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[105,1,105,7],[106,1,106,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[102,1,102,7],[103,1,103,7],[104,1,104,7],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,22,0,30],[1,23,1,29],[2,23,2,29],[3,23,3,29],[4,24,4,25],[4,27,4,28],[24,8,27,8],[44,8,46,8],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Gruppo Piazzetta S.P.A.",null,null,null,null,null,null,"Pacific Energy is listed on report but then Gruppo Piazzetta S.P.A. is listed on EPA & Mentioned",null,null,"Manufacturer","Gruppo Piazzetta S.P.A.",null,null,null,null,null,null,"Pacific Energy is listed on report but then Gruppo Piazzetta S.P.A. is listed on EPA & Mentioned",null,null,"Manufacturer","Gruppo Piazzetta S.P.A.",null,null,null,null,null,null,"Pacific Energy is listed on report but then Gruppo Piazzetta S.P.A. is listed on EPA & Mentioned"]
["Model","LIA",null,null,null,null,null,null,null,null,null,"Model","LIA",null,null,null,null,null,null,null,null,null,"Model","LIA"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,"OM not reviewed",null,null,"Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,null,null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":6},"Orange flags",null,{"$f":"SUMPRODUCT((B15=\"NR\")+(B15=\"Not reported\")+(B16=\"NR\")+(B16=\"Not reported\")+(G17=\"NR\")+(G17=\"Not reported\"))+COUNTIF(B18:H28,\"=Partially reported\")+COUNTIF(B30:B35,\"=Not reported\")+SUMPRODUCT((B39=\"Not reported\")+(B40=\"NR\")+(B40=\"Not reported\")+(B41=\"Cannot be determined\")+(B42=\"Cannot be determined\"))+COUNTIF(B45:B47,\"Not reported\")+COUNTIF(B49:B61,\"Not included\")+COUNTIF(B63:B67,\"Not reported\")+COUNTIF(B63:B67,\"=NR\")+COUNTIF(B63:B67,\"Partially reported major\")+COUNTIF(B68:B71,\"=No\")","v":4},"Yellow flags",null,{"$f":"COUNTIF(B9:H12,\"=Not reported\")+COUNTIF(B30:B35,\"=Partially reported\")+COUNTIF(B49:B61,\"Insufficient data\")+COUNTIF(B63:B67,\"Partially reported\")+COUNTIF(B63:B67,\"Partially reported minor\")++COUNTIF(B68:B71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},null,null,null,"Red flags",{"$f":"SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":5},"Orange flags",null,{"$f":"SUMPRODUCT((M15=\"NR\")+(M15=\"Not reported\")+(M16=\"NR\")+(M16=\"Not reported\")+(R17=\"NR\")+(R17=\"Not reported\"))+COUNTIF(M18:S28,\"=Partially reported\")+COUNTIF(M30:M35,\"=Not reported\")+SUMPRODUCT((M39=\"Not reported\")+(M40=\"NR\")+(M40=\"Not reported\")+(M41=\"Cannot be determined\")+(M42=\"Cannot be determined\"))+COUNTIF(M45:M47,\"Not reported\")+COUNTIF(M49:M61,\"Not included\")+COUNTIF(M63:M67,\"Not reported\")+COUNTIF(M63:M67,\"=NR\")+COUNTIF(M63:M67,\"Partially reported major\")+COUNTIF(M68:M71,\"=No\")","v":5},"Yellow flags",null,{"$f":"COUNTIF(M9:S12,\"=Not reported\")+COUNTIF(M30:M35,\"=Partially reported\")+COUNTIF(M49:M61,\"Insufficient data\")+COUNTIF(M63:M67,\"Partially reported\")+COUNTIF(M63:M67,\"Partially reported minor\")++COUNTIF(M68:M71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},null,null,null,"Red flags",{"$f":"SUMPRODUCT((X14=\"NR\")+(X14=\"Not reported\")+(AC14=\"NR\")+(AC14=\"Not reported\")) +COUNTIF(X14,\">2\")+COUNTIF(AC14,\">6\")+COUNTIF(X18:AD28,\"=Not reported\")+SUMPRODUCT((X36=\"NR\")+(X36=\"Not reported\")+(X37=\"NR\")+(X37=\"Not reported\")+(X38=\"Not reported\")+(X41=\"No\")+(X42=\"No\")+(X43=\"Not reported\"))+IFERROR(IF(INDEX(Y32:AD32,1,MATCH(\"High\",Y31:AD31,0))*0.5<INDEX(Y32:AD32,1,MATCH(\"Medium\",Y31:AD31,0)),1,0),0)+IFERROR(IF(INDEX(Y32:AD32,1,MATCH(\"Low\",Y31:AD31,0))<>MIN(Y32:AD32),1,0),0)","v":5},"Orange flags",null,{"$f":"SUMPRODUCT((X15=\"NR\")+(X15=\"Not reported\")+(X16=\"NR\")+(X16=\"Not reported\")+(AC17=\"NR\")+(AC17=\"Not reported\"))+COUNTIF(X18:AD28,\"=Partially reported\")+COUNTIF(X30:X35,\"=Not reported\")+SUMPRODUCT((X39=\"Not reported\")+(X40=\"NR\")+(X40=\"Not reported\")+(X41=\"Cannot be determined\")+(X42=\"Cannot be determined\"))+COUNTIF(X45:X47,\"Not reported\")+COUNTIF(X49:X61,\"Not included\")+COUNTIF(X63:X67,\"Not reported\")+COUNTIF(X63:X67,\"=NR\")+COUNTIF(X63:X67,\"Partially reported major\")+COUNTIF(X68:X71,\"=No\")","v":5},"Yellow flags",null,{"$f":"COUNTIF(X9:AD12,\"=Not reported\")+COUNTIF(X30:X35,\"=Partially reported\")+COUNTIF(X49:X61,\"Insufficient data\")+COUNTIF(X63:X67,\"Partially reported\")+COUNTIF(X63:X67,\"Partially reported minor\")++COUNTIF(X68:X71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}}]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","Approved List - Pending",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer states that this information was provided to EPA in the NSPS Affected Source App Form, that form was supplied. Though it was not in the report",null,null,"Third-party certifier","Intertek",null,null,null,null,null,null,"Manufacturer states that this information was provided to EPA in the NSPS Affected Source App Form, that form was supplied. Though it was not in the report",null,null,"Third-party certifier","Intertek",null,null,null,null,null,null,"Manufacturer states that this information was provided to EPA in the NSPS Affected Source App Form, that form was supplied. Though it was not in the report"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the certified report is located @ https://us.piazzetta.com/en/sc-pellet-stoves/pellet-stove-lia - the only signature on in the report does not include any sort of certifcation statment ",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the certified report is located @ https://us.piazzetta.com/en/sc-pellet-stoves/pellet-stove-lia - the only signature on in the report does not include any sort of certifcation statment ",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the certified report is located @ https://us.piazzetta.com/en/sc-pellet-stoves/pellet-stove-lia - the only signature on in the report does not include any sort of certifcation statment "]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,4.03,null,null,null,null,"Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,4.03,null,null,null,null,"Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,4.03]
["Overall HHV efficiency (%)",84,null,null,null,null,null,null,0.84,null,null,"Overall HHV efficiency (%)",84,null,null,null,null,null,null,0.84,null,null,"Overall HHV efficiency (%)",84,null,null,null,null,null,null,0.84]
["Overall heat output (Btu/hr)",14628,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14628,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",14628]
["Overall CO (g/hr)",1.83,null,null,null,null,{"$f":"(1.83/60)","v":3.0500000000000003E-2},null,"g/min not reported",null,null,"Overall CO (g/hr)",1.83,null,null,null,null,{"$f":"(1.83/60)","v":3.0500000000000003E-2},null,"g/min not reported",null,null,"Overall CO (g/hr)",1.83,null,null,null,null,{"$f":"(1.83/60)","v":3.0500000000000003E-2},null,"g/min not reported"]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,"Manufacturer states that the installation manual's operating instructions are also the manufacturer's instructions.",null,null,"Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,null,null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Efficiency  calculations","Reported",null,null,null,null,null,null,null,null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Burn rate calculations","Reported",null,null,null,null,null,null,null,null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,null,null,null,"Pre-burn completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 6/27/2016 through 6/28/2016 on med & high burn rate",null,null,"Pre-burn completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 6/27/2016 through 6/28/2016 on med & high burn rate"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information. p5. states that only 10 hours of conditioning at high to medium burn rate completed. No other data reported. Appears not meet aginign requirements. ",null,null,"Pre-burn data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. ",null,null,"Pre-burn data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Lab technician notes","Reported",null,null,null,null,null,null,null,null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Manufacturer states that all elements can be found in nonCBI test report. Reviewer found no specific language addressing run appropriateness, run validity, anomolies.",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Med","Low",null,null,null,null,null,null,"Run Category",null,"High","Med","Low",null,null,null,null,null,null,"Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.97,0.92,0.56999999999999995,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.97,0.92,0.56999999999999995,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.97,0.92,0.56999999999999995]
["Heat output (Btu/hr)",null,30927,14568,8996,null,null,null,37258,null,null,"Heat output (Btu/hr)",null,30927,14568,8996,null,null,null,37258,null,null,"Heat output (Btu/hr)",null,30927,14568,8996,null,null,null,37258]
["CO (g/min)",null,1.1299999999999999,0,3.3,null,null,null,"CO FOR MED REPORTED AS 0",null,null,"CO (g/min)",null,1.1299999999999999,0,3.3,null,null,null,"CO FOR MED REPORTED AS 0",null,null,"CO (g/min)",null,1.1299999999999999,0,3.3,null,null,null,"CO FOR MED REPORTED AS 0"]
["HHV efficiency (%)",null,83,83.8,83.1,null,null,null,null,null,null,"HHV efficiency (%)",null,83,83.8,83.1,null,null,null,null,null,null,"HHV efficiency (%)",null,83,83.8,83.1]
["Overall PM emissions (g/hr)",0.7,null,null,null,null,null,null,83,null,null,"Overall PM emissions (g/hr)",0.7,null,null,null,null,null,null,83,null,null,"Overall PM emissions (g/hr)",0.7,null,null,null,null,null,null,83]
["PM 1-hr filter pull (g/hr)",4.03,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",4.03,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",4.03]
["Filter data","Not reported",null,null,null,null,null,null,"Manufacturer states filter and all other data required for a valid certification is in the non CBI test report",null,null,"Filter data","Not reported",null,null,null,null,null,null,"Manufacturer did not provided reviewer with specific location to locate required data elements. ",null,null,"Filter data","Not reported",null,null,null,null,null,null,"Manufacturer did not provided reviewer with specific location to locate required data elements. "]
["Train precision (%)",0.1,null,null,null,null,null,null,null,null,null,"Train precision (%)",0.1,null,null,null,null,null,null,null,null,null,"Train precision (%)",0.1]
["Negative weights","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negative weights","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported",null,null,null,null,null,null,"No filter data was located by reviewer.",null,null,"All run data","Not reported",null,null,null,null,null,null,"No filter data was located by reviewer."]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Other",null,null,null,null,null,null,"Manufacturer clarified that Marthwood pellets were used and it was stated in report",null,null,"Pellet species/type","Other",null,null,null,null,null,null,"Marthwood",null,null,"Pellet species/type","Other",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","N/A",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","N/A",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","N/A"]
["Source of the pellet specification","N/A",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","N/A",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","N/A"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,null,null,null,"Stack height","Included",null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation",null,null,null,null,null,null,null,null,null,null,"Location recommendation","Included",null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft",null,null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included",null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading",null,null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable",null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.",null,null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included",null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings",null,null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included",null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures",null,null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included",null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls",null,null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included",null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low",null,null,null,null,null,null,null,null,null,null,"Proper operation low","Insufficient data",null,null,null,null,null,null,null,null,null,"Proper operation low","Insufficient data"]
["Ash removal procedures",null,null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included",null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts",null,null,null,null,null,null,null,null,null,null,"Replacement parts","Not included",null,null,null,null,null,null,null,null,null,"Replacement parts","Not included"]
["Federal warning (C or NC)",null,null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included",null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights",null,null,null,null,null,null,null,null,null,null,"Warranty rights","Included",null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","All reported"]
["All run data submitted","Partially reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported",null,null,null,null,null,null,null,null,null,"All run data submitted","All reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major"]
["Owner manual complete",null,null,null,null,null,null,null,null,null,null,"Owner manual complete",null,null,null,null,null,null,null,null,null,null,"Owner manual complete"]
["Test dates","2016-07-12",null,null,null,null,null,null,null,null,null,"Test dates","2016-07-12",null,null,null,null,null,null,null,null,null,"Test dates","2016-07-12"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"Manufacturer states that EPA Application was the 30 day notice and supplied that form",null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"Manufacturer provided application and not 30 day notice.",null,null,"30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"Manufacturer provided application and not 30 day notice."]
["Tested on the proposed date","Cannot be determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot be determined",null,null,null,null,null,null,null,null,null,"Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,"check owners manual and highest setting in test are they the same"]
["Test location",null,null,null,null,null,null,null,null,null,null,"Test location",null,null,null,null,null,null,null,null,null,null,"Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit",null,null,null,null,null,null,null,null,null,null,"date lab received the unit","2016-06-23"]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning",null,null,null,null,null,null,null,null,null,null,"date first day of conditioning","2016-06-27"]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing",null,null,null,null,null,null,null,null,null,null,"date first day of testing","2016-07-11"]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,"first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,"Zero CO emission reported","yes"]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs",null,null,null,null,null,null,null,null,null,null,"Any incomplete runs","no"]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,"Pre-ignition data reported","yes"]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run",null,null,null,null,null,null,null,null,null,null,"filter changes during test run","no"]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run",null,null,null,null,null,null,null,null,null,null,"filter plugged during test run","no"]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used",null,null,null,null,null,null,null,null,null,null,"What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters"]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,"Negative probe weight >5% of PM","not reported"]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value",null,null,null,null,null,null,null,null,null,null,"Negative probe value","not reported"]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values",null,null,null,null,null,null,null,null,null,null,"Negative room air values","not reported"]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data",null,null,null,null,null,null,null,null,null,null,"Ambient background filter data","not reported"]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling",null,null,null,null,null,null,null,null,null,null,"Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,"Leak check - pre-test leak check  reported","Meets Specification"]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,"Leak check - any filter change"]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,"Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,"Dilution tunnel schematic meets ASTM 2515 requirements","Does not meet specification",null,null,null,null,null,null,"Mixing baffle shown on pg 10 of report and noted in summary on pg 9"]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours reported in summary",10]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,"number of conditioning hours with data"]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,"number of hours at correct conditioning conditions",null,null,null,null,null,null,null,"see cell I22"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,"used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,"see cell I57"]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,"Air setting data","High",null,"Medium",null,"Low"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"level 4",null,"level 2",null,"level 1"]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met",null,null,null,null,null,null,null,null,null,null,"medium burn conditions met"]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,"high test settings match high in OM"]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",null,null,null,null,null,null,null,null,null,null,"Total number of runs",1,null,null,null,null,null,null,"integrated"]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly",null,null,null,null,null,null,null,null,null,null,"run averaging done correctly","yes"]
["Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data",null,null,null,null,null,null,null,null,null,null,"Calibration data","partially reported",null,null,null,null,null,null,"some outside of the 6 month window"]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements",null,null,"Milestone Date","2022-01-20"]
["Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date",null,null,null,null,null,null,null,null,null,null,"Compliance Date","2016-07-19","No EPA Compliance Date"]
["DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration",null,null,null,null,null,null,null,null,null,null,"DEC Calculated Certification Expiration","2021-07-19"]

{"sheet":"Monia 2.0","index":76,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[62,12,62,18],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[68,12,68,18],[69,12,69,18],[70,12,70,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18],[52,12,52,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[43,12,43,18],[21,12,21,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[24,19,27,19],[25,12,25,18],[26,12,26,18],[27,12,27,18],[28,12,28,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[5,12,5,15],[5,16,5,18],[6,12,6,18],[105,1,105,7],[106,1,106,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[102,1,102,7],[103,1,103,7],[104,1,104,7],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[24,8,27,8],[67,1,67,7],[68,1,68,7],[69,1,69,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Gruppo Piazzetta S.P.A.",null,null,null,null,null,null,null,null,null,"Manufacturer","Gruppo Piazzetta S.P.A."]
["Model","Monia 2.0, Marcella 2.0, Maya 2.0, Monica 2.0",null,null,null,null,null,null,null,null,null,"Model","Monia 2.0, Marcella 2.0, Maya 2.0, Monica 2.0"]
["Prelim review recomm.","Disapproved",null,null,null,null,null,null,"OM not reviewed",null,null,"Prelim review recomm.","Disapproved"]
["Red flags",{"$f":"SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":6},"Orange flags",null,{"$f":"SUMPRODUCT((B15=\"NR\")+(B15=\"Not reported\")+(B16=\"NR\")+(B16=\"Not reported\")+(G17=\"NR\")+(G17=\"Not reported\"))+COUNTIF(B18:H28,\"=Partially reported\")+COUNTIF(B30:B35,\"=Not reported\")+SUMPRODUCT((B39=\"Not reported\")+(B40=\"NR\")+(B40=\"Not reported\")+(B41=\"Cannot be determined\")+(B42=\"Cannot be determined\"))+COUNTIF(B45:B47,\"Not reported\")+COUNTIF(B49:B61,\"Not included\")+COUNTIF(B63:B67,\"Not reported\")+COUNTIF(B63:B67,\"=NR\")+COUNTIF(B63:B67,\"Partially reported major\")+COUNTIF(B68:B71,\"=No\")","v":7},"Yellow flags",null,{"$f":"COUNTIF(B9:H12,\"=Not reported\")+COUNTIF(B30:B35,\"=Partially reported\")+COUNTIF(B49:B61,\"Insufficient data\")+COUNTIF(B63:B67,\"Partially reported\")+COUNTIF(B63:B67,\"Partially reported minor\")++COUNTIF(B68:B71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},"OM not reviewed",null,null,"Red flags",{"$f":"SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":4},"Orange flags",null,{"$f":"SUMPRODUCT((M15=\"NR\")+(M15=\"Not reported\")+(M16=\"NR\")+(M16=\"Not reported\")+(R17=\"NR\")+(R17=\"Not reported\"))+COUNTIF(M18:S28,\"=Partially reported\")+COUNTIF(M30:M35,\"=Not reported\")+SUMPRODUCT((M39=\"Not reported\")+(M40=\"NR\")+(M40=\"Not reported\")+(M41=\"Cannot be determined\")+(M42=\"Cannot be determined\"))+COUNTIF(M45:M47,\"Not reported\")+COUNTIF(M49:M61,\"Not included\")+COUNTIF(M63:M67,\"Not reported\")+COUNTIF(M63:M67,\"=NR\")+COUNTIF(M63:M67,\"Partially reported major\")+COUNTIF(M68:M71,\"=No\")","v":9},"Yellow flags",null,{"$f":"COUNTIF(M9:S12,\"=Not reported\")+COUNTIF(M30:M35,\"=Partially reported\")+COUNTIF(M49:M61,\"Insufficient data\")+COUNTIF(M63:M67,\"Partially reported\")+COUNTIF(M63:M67,\"Partially reported minor\")++COUNTIF(M68:M71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},"OM not reviewed"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR, NR",null,null,"Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: M1, MD, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Though not listed specifically in the report the manufacturer has identified the 3rd party certifier as Intertek",null,null,"Third-party certifier","Intertek",null,null,null,null,null,null,"Though not listed specifically in the report the manufacturer has identified the 3rd party certifier as Intertek"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the report was signed and certified but no certification statement can be identified by reviewer",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the report was signed and certified but no certification statement can be identified by reviewer"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.82,null,"PM Highest 1-hr (g/hr)",null,null,1.1850000000000001,null,"run 1 could have had a higher value but was not reported",null,null,"Overall PM emissions (g/hr)",0.82,null,"PM Highest 1-hr (g/hr)",null,null,1.1850000000000001,null,"run 1 could have had a higher value but was not reported - manufacturer states and supplied notification was sent to EPA regarding the stopped run. The manufacturer states \" EPA approved the report and all the run data sending a Certification Letter\""]
["Overall HHV efficiency (%)",82.4,null,null,null,null,null,null,null,null,null,"Overall HHV efficiency (%)",82.4,null,null,null,null,null,null,0.82399999999999995]
["Overall heat output (Btu/hr)",15215,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",15215]
["Overall CO (g/hr)",0,null,null,null,null,null,null,null,null,null,"Overall CO (g/hr)",0,null,null,null,null,0]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,"Manufacturer states that the installation manual's operating instructions are also the manufacturer's instructions.",null,null,"Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Partially reported",null,null,null,null,null,null,"run 2 only",null,null,"Efficiency  calculations","Partially reported",null,null,null,null,null,null,"run 2 only"]
["Burn rate calculations","Partially reported",null,null,null,null,null,null,"run 2 only",null,null,"Burn rate calculations","Partially reported",null,null,null,null,null,null,"run 2 only"]
["Raw data sheets","Reported",null,null,null,null,null,null,null,null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,null,null,null,"Pre-burn completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 2/14/19 through 2/15/19 on med & high burn rate"]
["Conditioning data","Not reported",null,null,null,null,null,null,"only 10 hours of conditioning completed at high to medium burn rate per p 3. No other data",null,null,"Pre-burn data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Partially reported",null,null,null,null,null,null,"run 2 only",null,null,"Lab technician notes","Partially reported",null,null,null,null,null,null,"run 2 only"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Manufacturer states that all elements can be found in nonCBI test report. Reviewer found no specific language addressing run appropriateness, run validity, anomolies.",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Manufacturer did not provided reviewer with specific location to locate required data elements. "]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Partially reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Partially reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,null,null,null,"run 1 was not reported",null,null,"Run #",null,2,2,2,null,null,null,"run 1 was not reported"]
["Run Category",null,"High","Med","Low",null,null,null,null,null,null,"Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.96,0.93,0.68,null,null,null,null,null,null,"Burn rate (kg/hr)",null,1.96,0.93,0.68]
["Heat output (Btu/hr)",null,30574,14279,10479,null,null,null,null,null,null,"Heat output (Btu/hr)",null,30574,14279,10479,null,null,null,36944]
["CO (g/min)",null,0,0,0,null,null,null,null,null,null,"CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,82.8,81.099999999999994,81.400000000000006,null,null,null,null,null,null,"HHV efficiency (%)",null,82.8,81.099999999999994,81.400000000000006]
["Overall PM emissions (g/hr)",0.82,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",0.82]
["PM 1-hr filter pull (g/hr)",1.1850000000000001,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.1850000000000001]
["Filter data","Not reported",null,null,null,null,null,null,"run 2 reported only",null,null,"Filter data","Not reported",null,null,null,null,null,null,"run 2 reported only"]
["Train precision (%)",4.32,null,null,null,null,null,null,null,null,null,"Train precision (%)",4.32]
["Negative weights","No",null,null,null,null,null,null,null,null,null,"Negative weights","No"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported",null,null,null,null,null,null,"Run 1 data was included however the PM & 1st hour were not ",null,null,"All run data","Not reported",null,null,null,null,null,null,"Run 1 data was included however the PM & 1st hour were not "]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood",null,null,"Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification",null,null,null,null,null,null,null,null,null,null,"Pellet fuel certification"]
["Source of the pellet specification",null,null,null,null,null,null,null,null,null,null,"Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation",null,null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft",null,null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading",null,null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.",null,null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings",null,null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures",null,null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls",null,null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low",null,null,null,null,null,null,null,null,null,null,"Proper operation low","Insufficient data"]
["Ash removal procedures",null,null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts",null,null,null,null,null,null,null,null,null,null,"Replacement parts","Not included"]
["Federal warning (C or NC)",null,null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights",null,null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,"only run 2",null,null,"Summary tables complete","Partially reported",null,null,null,null,null,null,"only run 2"]
["All run data submitted","Partially reported",null,null,null,null,null,null,"left out pm info for run 1",null,null,"All run data submitted","Partially reported",null,null,null,null,null,null,"left out pm info for run 1"]
["Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major"]
["Owner manual complete",null,null,null,null,null,null,null,null,null,null,"Owner manual complete"]
["Test dates","2/20 & 2/21/2019",null,null,null,null,null,null,null,null,null,"Test dates","2/20 & 2/21/2019"]
["30 Day notice submitted to EPA","Cannot be determined",null,null,null,null,null,null,"Submitted by manufacturer but not included in report",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,"Submitted by manufacturer but not included in report"]
["Tested on the proposed date","Cannot be determined",null,null,null,null,null,null,"Run 1 was conducted on proposed date. Run 2 was done on the following day.",null,null,"Tested on the proposed date","Yes",null,null,null,null,null,null,"Run 1 was conducted on proposed date. Run 2 was done on the following day."]
["Tested in one day","No",null,null,null,null,null,null,"2 runs, one on each day",null,null,"Tested in one day","No",null,null,null,null,null,null,"2 runs, one on each day"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same"]
["Test location"]
["date lab received the unit"]
["date first day of conditioning"]
["date first day of testing"]
["first hour PM emissions reported for all runs"]
["first hour PM emissions reported in grams per hour"]
["first hour PM emissions zero or negative"]
["first hour PM emissions measured with front and back filter"]
["Zero CO emission reported"]
["Any incomplete runs"]
["Pre-ignition data reported"]
["filter changes during test run"]
["filter plugged during test run"]
["What type of filter used"]
["Negative probe weight >5% of PM"]
["Negative probe value"]
["Negative room air values"]
["Ambient background filter data"]
["Proportional sampling"]
["Leak check - pre-test leak check  reported"]
["Leak check - any filter change"]
["Leak check - post leak check reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements"]
["number of conditioning hours reported in summary"]
["number of conditioning hours with data"]
["number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met"]
["high test settings match high in OM"]
["Total number of runs"]
["run averaging done correctly"]
["Calibration data"]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Sabrina 2.0","index":77,"n_rows":110,"n_cols":20,"rows_kept":110,"cut":false,"hidden":false,"merged":[[105,1,105,7],[106,1,106,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[102,1,102,7],[103,1,103,7],[104,1,104,7],[89,1,89,7],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[96,1,96,7],[97,1,97,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[65,1,65,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7],[0,11,0,19],[1,12,1,18],[2,12,2,18],[3,12,3,18],[4,13,4,14],[4,16,4,17],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,12,10,18],[11,12,11,18],[12,12,12,18],[13,12,13,13],[13,14,13,16],[13,17,13,18],[5,12,5,15],[5,16,5,18],[7,12,7,18],[8,12,8,18],[9,12,9,18],[6,12,6,18],[17,12,17,18],[18,12,18,18],[19,12,19,18],[20,12,20,18],[21,12,21,18],[14,12,14,18],[15,12,15,18],[16,12,16,13],[16,14,16,16],[16,17,16,18],[27,12,27,18],[28,12,28,18],[35,12,35,18],[36,12,36,18],[37,12,37,18],[22,12,22,18],[23,12,23,18],[24,12,24,18],[25,12,25,18],[26,12,26,18],[52,12,52,18],[43,12,43,18],[44,12,44,18],[45,12,45,18],[46,12,46,18],[47,12,47,18],[38,12,38,18],[39,12,39,18],[40,12,40,18],[41,12,41,18],[42,12,42,18],[24,8,27,8],[68,12,68,18],[69,12,69,18],[70,12,70,18],[24,19,27,19],[63,12,63,18],[64,12,64,18],[65,12,65,18],[66,12,66,18],[67,12,67,18],[58,12,58,18],[59,12,59,18],[60,12,60,18],[61,12,61,18],[62,12,62,18],[53,12,53,18],[54,12,54,18],[55,12,55,18],[56,12,56,18],[57,12,57,18],[48,12,48,18],[49,12,49,18],[50,12,50,18],[51,12,51,18]]}
["Summary of Review",null,null,null,null,null,null,null,null,null,null,"Summary of Review"]
["Manufacturer","Gruppo Piazzetta S.P.A.",null,null,null,null,null,null,null,null,null,"Manufacturer","Gruppo Piazzetta S.P.A."]
["Model","Sabrina 2.0, Sally 2.0, Solange 2.0, Sveva 2.0",null,null,null,null,null,null,null,null,null,"Model","Sabrina 2.0, Sally 2.0, Solange 2.0, Sveva 2.0"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,"OM not reviewed",null,null,"Prelim review recomm.","Requires a more thorough review"]
["Red flags",{"$f":"SUMPRODUCT((B14=\"NR\")+(B14=\"Not reported\")+(G14=\"NR\")+(G14=\"Not reported\")) +COUNTIF(B14,\">2\")+COUNTIF(G14,\">6\")+COUNTIF(B18:H28,\"=Not reported\")+SUMPRODUCT((B36=\"NR\")+(B36=\"Not reported\")+(B37=\"NR\")+(B37=\"Not reported\")+(B38=\"Not reported\")+(B41=\"No\")+(B42=\"No\")+(B43=\"Not reported\"))+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"High\",C31:H31,0))*0.5<INDEX(C32:H32,1,MATCH(\"Medium\",C31:H31,0)),1,0),0)+IFERROR(IF(INDEX(C32:H32,1,MATCH(\"Low\",C31:H31,0))<>MIN(C32:H32),1,0),0)","v":7},"Orange flags",null,6,"Yellow flags",null,{"$f":"COUNTIF(B9:H12,\"=Not reported\")+COUNTIF(B30:B35,\"=Partially reported\")+COUNTIF(B49:B61,\"Insufficient data\")+COUNTIF(B63:B67,\"Partially reported\")+COUNTIF(B63:B67,\"Partially reported minor\")++COUNTIF(B68:B71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},"OM not reviewed",null,null,"Red flags",{"$f":"SUMPRODUCT((M14=\"NR\")+(M14=\"Not reported\")+(R14=\"NR\")+(R14=\"Not reported\")) +COUNTIF(M14,\">2\")+COUNTIF(R14,\">6\")+COUNTIF(M18:S28,\"=Not reported\")+SUMPRODUCT((M36=\"NR\")+(M36=\"Not reported\")+(M37=\"NR\")+(M37=\"Not reported\")+(M38=\"Not reported\")+(M41=\"No\")+(M42=\"No\")+(M43=\"Not reported\"))+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"High\",N31:S31,0))*0.5<INDEX(N32:S32,1,MATCH(\"Medium\",N31:S31,0)),1,0),0)+IFERROR(IF(INDEX(N32:S32,1,MATCH(\"Low\",N31:S31,0))<>MIN(N32:S32),1,0),0)","v":5},"Orange flags",null,6,"Yellow flags",null,{"$f":"COUNTIF(M9:S12,\"=Not reported\")+COUNTIF(M30:M35,\"=Partially reported\")+COUNTIF(M49:M61,\"Insufficient data\")+COUNTIF(M63:M67,\"Partially reported\")+COUNTIF(M63:M67,\"Partially reported minor\")++COUNTIF(M68:M71,\"=Cannot be determined\")+COUNTIF(#REF!,\"=NR\")+COUNTIF(#REF!,\"=Not reported\")","v":{"$error":"#REF!"}},"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR",null,null,"Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List",null,null,null,null,null,null,null,null,null,"AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes",null,null,"Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779",null,null,null,null,null,null,null,null,null,"Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,null,null,null,"Test Lab","Intertek"]
["Third-party certifier","Not reported",null,null,null,null,null,null,"Manufacturer states that this information was provided to EPA in the NSPS Affected Source App Form, that form was supplied.",null,null,"Third-party certifier","Intertek"]
["Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the certified report is located @ https://us.piazzetta.com/en/sc-pellet-stoves/pellet-stove-sabrina-painted-steel-cladding - the only signature on in the 22 page report specifically states \"This report does not constitute certification of this product nor an opinion or endorsement by this laboratory.\"",null,null,"Report certified","Not reported",null,null,null,null,null,null,"Manufacturer states that the certified report is located @ https://us.piazzetta.com/en/sc-pellet-stoves/pellet-stove-sabrina-painted-steel-cladding - the only signature on in the 22 page report specifically states \"This report does not constitute certification of this product nor an opinion or endorsement by this laboratory.\""]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.155,null,"PM Highest 1-hr (g/hr)",null,null,1.9339999999999999,null,null,null,null,"Overall PM emissions (g/hr)",1.155,null,"PM Highest 1-hr (g/hr)",null,null,1.9339999999999999]
["Overall HHV efficiency (%)",81.8,null,null,null,null,null,null,0.81799999999999995,null,null,"Overall HHV efficiency (%)",81.8,null,null,null,null,null,null,0.81799999999999995]
["Overall heat output (Btu/hr)",18491,null,null,null,null,null,null,null,null,null,"Overall heat output (Btu/hr)",18491]
["Overall CO (g/hr)",0,null,null,null,null,0,null,"CO reported as zero",null,null,"Overall CO (g/hr)",0,null,null,null,null,0,null,"CO reported as zero"]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,"Manufacturer states that the installation manual's operating instructions are also the manufacturer's instructions.",null,null,"Manufacturers Instructions to lab","Partially reported"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Efficiency  calculations","Reported"]
["Burn rate calculations","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Burn rate calculations","Reported"]
["Raw data sheets","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,null,null,null,"Pre-burn completed by","Lab",null,null,null,null,null,null,"Report mentions that 10 plus hours of preburning  were conducted on 2/14/19 through 2/15/19 on med & high burn rate"]
["Conditioning data","Not reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information. Summary date indicates only 10  hours of conditioning at the high-medium burn rate was completed. Insufficient data to indicate conditioning completed as the method requires. ",null,null,"Pre-burn data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Reported",null,null,null,null,null,null,"Manufacturer referred reviewer to location of information",null,null,"Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Manufacturer states that all elements can be found in nonCBI test report. Reviewer found no specific language addressing run appropriateness, run validity, anomolies.",null,null,"Doc. of run appropriateness","Not reported",null,null,null,null,null,null,"Manufacturer did not provided reviewer with specific location to locate required data elements. "]
["Doc. of run validity","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported",null,null,null,null,null,null,null,null,null,"Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,null,null,null,"Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes",null,null,"Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,null,null,null,null,null,null,"Run #",null,1,1,1]
["Run Category",null,"High","Med","Low",null,null,null,null,null,null,"Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.4,1.18,0.81,null,null,null,null,null,null,"Burn rate (kg/hr)",null,2.4,1.18,0.81]
["Heat output (Btu/hr)",null,37238,18247,12096,null,null,null,45325,null,null,"Heat output (Btu/hr)",null,37238,18247,12096,null,null,null,45325]
["CO (g/min)",null,0,0,0,null,null,null,null,null,null,"CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,82.2,82.3,79.099999999999994,null,null,null,null,null,null,"HHV efficiency (%)",null,82.2,82.3,79.099999999999994]
["Overall PM emissions (g/hr)",1.155,null,null,null,null,null,null,null,null,null,"Overall PM emissions (g/hr)",1.155]
["PM 1-hr filter pull (g/hr)",1.9339999999999999,null,null,null,null,null,null,null,null,null,"PM 1-hr filter pull (g/hr)",1.9339999999999999]
["Filter data","Not reported",null,null,null,null,null,null,"Manufacturer states filter and all other data required for a valid certification is in the non CBI test report, reviewer is unable to locted the filter data.",null,null,"Filter data","Not reported",null,null,null,null,null,null,"Manufacturer did not provided reviewer with specific location to locate required data elements. "]
["Train precision (%)",1.59,null,null,null,null,null,null,null,null,null,"Train precision (%)",1.59]
["Negative weights","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negative weights","Cannot be determined"]
["Negs handled appropriately","Cannot be determined",null,null,null,null,null,null,null,null,null,"Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,null,null,null,"Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported",null,null,null,null,null,null,null,null,null,"All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes",null,null,"Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Other",null,null,null,null,null,null,"Marthwood",null,null,"Pellet species/type","Other",null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","N/A",null,null,null,null,null,null,null,null,null,"Pellet fuel certification","N/A"]
["Source of the pellet specification","N/A",null,null,null,null,null,null,null,null,null,"Source of the pellet specification","N/A"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes",null,null,"Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,null,null,null,"Stack height","Included"]
["Location recommendation",null,null,null,null,null,null,null,null,null,null,"Location recommendation","Included"]
["Guidance on proper draft",null,null,null,null,null,null,null,null,null,null,"Guidance on proper draft","Included"]
["Fuel loading & reloading",null,null,null,null,null,null,null,null,null,null,"Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.",null,null,null,null,null,null,null,null,null,null,"Fuel selection recomm.","Included"]
["Improper fuels warnings",null,null,null,null,null,null,null,null,null,null,"Improper fuels warnings","Included"]
["Fire starting procedures",null,null,null,null,null,null,null,null,null,null,"Fire starting procedures","Included"]
["Proper use of air controls",null,null,null,null,null,null,null,null,null,null,"Proper use of air controls","Included"]
["Proper operation low",null,null,null,null,null,null,null,null,null,null,"Proper operation low","Insufficient data"]
["Ash removal procedures",null,null,null,null,null,null,null,null,null,null,"Ash removal procedures","Included"]
["Replacement parts",null,null,null,null,null,null,null,null,null,null,"Replacement parts","Not included"]
["Federal warning (C or NC)",null,null,null,null,null,null,null,null,null,null,"Federal warning (C or NC)","Included"]
["Warranty rights",null,null,null,null,null,null,null,null,null,null,"Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes",null,null,"Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported",null,null,null,null,null,null,null,null,null,"Summary tables complete","Partially reported"]
["All run data submitted","Partially reported",null,null,null,null,null,null,null,null,null,"All run data submitted","Partially reported"]
["Test report complete","Partially reported major",null,null,null,null,null,null,null,null,null,"Test report complete","Partially reported major"]
["Owner manual complete",null,null,null,null,null,null,null,null,null,null,"Owner manual complete"]
["Test dates","2019-02-19",null,null,null,null,null,null,null,null,null,"Test dates","2019-02-19"]
["30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,"Manfacturer submitted 30 day notice, though it was not included in the report",null,null,"30 Day notice submitted to EPA","Yes",null,null,null,null,null,null,"Manfacturer submitted 30 day notice, though it was not included in the report"]
["Tested on the proposed date","Cannot be determined",null,null,null,null,null,null,"Tested on proposed date as confirmed by 30 day notice",null,null,"Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes",null,null,null,null,null,null,null,null,null,"Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,null,null,null,"60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same"]
["Test location"]
["date lab received the unit"]
["date first day of conditioning"]
["date first day of testing"]
["first hour PM emissions reported for all runs"]
["first hour PM emissions reported in grams per hour"]
["first hour PM emissions zero or negative"]
["first hour PM emissions measured with front and back filter"]
["Zero CO emission reported"]
["Any incomplete runs"]
["Pre-ignition data reported"]
["filter changes during test run"]
["filter plugged during test run"]
["What type of filter used"]
["Negative probe weight >5% of PM"]
["Negative probe value"]
["Negative room air values"]
["Ambient background filter data"]
["Proportional sampling"]
["Leak check - pre-test leak check  reported"]
["Leak check - any filter change"]
["Leak check - post leak check reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements"]
["number of conditioning hours reported in summary"]
["number of conditioning hours with data"]
["number of hours at correct conditioning conditions"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met"]
["high test settings match high in OM"]
["Total number of runs"]
["run averaging done correctly"]
["Calibration data"]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Enerco 20kw","index":78,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Enerco"]
["Model","Cleveland Iron Works Model PS20W"]
["Prelim review recomm.","Requires a more thorough review",null,null,null,null,null,null,"OM not reviewed"]
["Red flags",2,"Orange flags",null,15,"Yellow flags",null,4,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"tested at Intertek facility"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.76900000000000002,null,"PM Highest 1-hr (g/hr)",null,null,0.372]
["Overall HHV efficiency (%)",86.5]
["Overall heat output (Btu/hr)","Not reported"]
["Overall CO (g/hr)",0,null,null,null,null,0,null,"zero CO emissions reported - how is this possible"]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"only completed 10 hours of aging/48 required by test method"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Appliance did not meet aging requirement for hours. Conditioning does not conform to test method requirements. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Partially reported",null,null,null,null,null,null,"no discussion of zero CO emissions"]
["Doc. of run validity","Partially reported",null,null,null,null,null,null,"no discussion of zero CO emissions"]
["Doc. of run anomolies","Partially reported",null,null,null,null,null,null,"no discussion of zero CO emissions"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.34,0.63,0.55000000000000004]
["Heat output (Btu/hr)",null,"NR","NR","NR",null,null,null,49000]
["CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,"NR","NR","NR"]
["Overall PM emissions (g/hr)",0.76900000000000002]
["PM 1-hr filter pull (g/hr)",0.372]
["Filter data","Reported"]
["Train precision (%)",1.22]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported",null,null,null,null,null,null,"missing co data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,"Unable to Locate OM"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete"]
["Test dates","2017-08-28",null,null,null,null,null,null,"reported completed within 3 days of test?"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 8/31/2017"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Ravelli Roma","index":79,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Ravelli"]
["Model","Roma"]
["Prelim review recomm.",null,null,null,null,null,null,null,"OM not reviewed"]
["Red flags",9,"Orange flags",null,7,"Yellow flags",null,8,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Polytests Inc.",null,null,null,null,null,null,"tested at Polytest faciity"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.74,null,"PM Highest 1-hr (g/hr)",null,null,1.33]
["Overall HHV efficiency (%)",75.5]
["Overall heat output (Btu/hr)",15631]
["Overall CO (g/hr)",9.4499999999999993,null,null,null,null,{"$f":"B17/60","v":0.1575}]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"data reported in minute configuration. No data provided to assure compliance with 48 hours at medium burn rate requirement. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low",null,null,null,"testing indicates the unit used"]
["Burn rate (kg/hr)",null,"NR","NR","NR",null,null,null,"pellets and chips but only pellet"]
["Heat output (Btu/hr)",null,"NR","NR","NR",null,null,null,"run reported"]
["CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,"NR","NR","NR"]
["Overall PM emissions (g/hr)",0.74]
["PM 1-hr filter pull (g/hr)",1.33]
["Filter data","Reported"]
["Train precision (%)",1.1200000000000001]
["Negative weights","yes"]
["Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Cannot be determined"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"hotzpellet and chips"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Not included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Not included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete"]
["Test dates","2016-03-01"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Cannot be determined"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 4/22/2016"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"695-B Gaudette St-jean-sur-Richelieu QC, Canada J3B 7S7",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2016-02-01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","Cannot be determined",null,null,null,null,null,null,"Report states last week in March putting it after the test.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2016-03-01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free (or equivalent), 47 mm diameter",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"mixing baffles shown on pg 141 & 149",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",57.41,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,5,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,"Pellet and air settings not listed",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"SBI Osburn","index":80,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Stove Builder International"]
["Model","Osburn 2500, ECO-55"]
["Prelim review recomm.",null,null,null,null,null,null,null,"OM not reviewed"]
["Red flags",1,"Orange flags",null,2,"Yellow flags",null,5,"OM not reviewed"]
["Final Determination","Pending - Minor",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek",null,null,null,null,null,null,"performed at company facility"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.96299999999999997,null,"PM Highest 1-hr (g/hr)",null,null,1.04,null,"used 3rd train for 1 hr value"]
["Overall HHV efficiency (%)",70.3]
["Overall heat output (Btu/hr)","Not reported"]
["Overall CO (g/hr)",7.6,null,null,null,null,{"$f":"B17/60","v":0.12666666666666665}]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Manufacturer"]
["Conditioning data","Reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.0499999999999998,0.96,0.52]
["Heat output (Btu/hr)",null,30086,13154,10434,null,null,null,39260]
["CO (g/min)",null,{"$f":"5.4/60","v":9.0000000000000011E-2},{"$f":"6.5/60","v":0.10833333333333334},{"$f":"9.4/60","v":0.15666666666666668}]
["HHV efficiency (%)",null,72.7,67.900000000000006,67.2]
["Overall PM emissions (g/hr)",0.96299999999999997]
["PM 1-hr filter pull (g/hr)",1.04]
["Filter data","Reported"]
["Train precision (%)",3.03]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Energex"]
["Pellet fuel certification",null,null,null,null,null,null,null,0.61499999999999999]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,"Webpage not operating shows server error when accessing manual"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete"]
["Test dates","2016-11-01"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"2016-11-25"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Thermorossi slim9","index":81,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Thermorossi"]
["Model","SlimQuatro  9 "]
["Prelim review recomm.",null,null,null,null,null,null,null,"OM not reviewed"]
["Red flags",3,"Orange flags",null,6,"Yellow flags",null,4,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Polytests Inc."]
["Third-party certifier","UL LLC"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.7,null,"PM Highest 1-hr (g/hr)",null,null,1.43]
["Overall HHV efficiency (%)",79]
["Overall heat output (Btu/hr)",16940]
["Overall CO (g/hr)",9.31,null,null,null,null,{"$f":"B17/60","v":0.15516666666666667}]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.16,1.1299999999999999,0.75]
["Heat output (Btu/hr)",null,32691,17254,11356]
["CO (g/min)",null,{"$f":"3.5/60","v":5.8333333333333334E-2},{"$f":"9.22/60","v":0.15366666666666667},{"$f":"19.13/60","v":0.3188333333333333}]
["HHV efficiency (%)",null,78.7,79.099999999999994,78.2]
["Overall PM emissions (g/hr)",0.7]
["PM 1-hr filter pull (g/hr)",1.43]
["Filter data","Reported"]
["Train precision (%)",2.98]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Holzpellets - website in German"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,"Owners Manual found written in Italian"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete"]
["Test dates","2017-03-29"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"2017-04-07"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"695-B Gaudette St-jean-sur-Richelieu QC, Canada J3B 7S7",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2017-02-25",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","Last week in Feb 2017",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2017-03-29",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free (or equivalent), 47 mm diameter filters",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 110 & 121 show mixing baffle",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",56,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"see cell I23",null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,5,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2018-03-28","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2023-03-28"]

{"sheet":"Thermorossi slim 11","index":82,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Thermorossi"]
["Model","Slimquadro 11"]
["Prelim review recomm.",null,null,null,null,null,null,null,"OM not reviewed"]
["Red flags",3,"Orange flags",null,5,"Yellow flags",null,4,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Polytests Inc."]
["Third-party certifier","UL LLC"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.6,null,"PM Highest 1-hr (g/hr)",null,null,2.16]
["Overall HHV efficiency (%)",78.900000000000006]
["Overall heat output (Btu/hr)",23237]
["Overall CO (g/hr)",3.64,null,null,null,null,{"$f":"B17/60","v":6.0666666666666667E-2}]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.39,1.53,1.23]
["Heat output (Btu/hr)",null,36548,23553,18586]
["CO (g/min)",null,{"$f":"1.61/60","v":2.6833333333333334E-2},{"$f":"1.6/60","v":2.6666666666666668E-2},{"$f":"1.61/60","v":2.6833333333333334E-2}]
["HHV efficiency (%)",null,79.400000000000006,79.7,77.900000000000006]
["Overall PM emissions (g/hr)",1.6]
["PM 1-hr filter pull (g/hr)",2.16]
["Filter data","Reported"]
["Train precision (%)",1.86]
["Negative weights","yes"]
["Negs handled appropriately","No"]
["Lowest burn rate tested","Yes"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported",null,null,null,null,null,null,"Holzpellets - website in German"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height",null,null,null,null,null,null,null,"Owners Manual found written in Italian"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete"]
["Test dates","2017-03-28"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 4/7/2017"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"695-B Gaudette St-jean-sur-Richelieu QC, Canada J3B 7S7",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2017-02-25",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","last week in feb 2017",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2016-03-28",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","no",null,null,null,null,null,null,"All CO measurements the same?",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free (or equivalent), 47 mm diameter filters.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"pg 111 & 118 show mixing baffle",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",51.83,null,null,null,null,null,null,"see cell I23",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,5,null,2,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2018-03-28","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2023-03-28"]

{"sheet":"SMG HP54","index":83,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","SMG Hearth & Home LLC"]
["Model","HP54"]
["Prelim review recomm."]
["Red flags",7,"Orange flags",null,10,"Yellow flags",null,2,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.54,null,"PM Highest 1-hr (g/hr)",null,null,1.93]
["Overall HHV efficiency (%)",83.8]
["Overall heat output (Btu/hr)",28305]
["Overall CO (g/hr)",0,null,null,null,null,0,null,"zero CO emissions reports, needs explaination"]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Partially reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"only 10 hours of aging - method requires 48 hours"]
["Conditioning data","Not reported"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,"did not identify issues with medium burn"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.95,2.27,1.29]
["Heat output (Btu/hr)",null,44391,34026,18813,null,null,null,42000]
["CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,84.3,83.9,82.1]
["Overall PM emissions (g/hr)",1.54]
["PM 1-hr filter pull (g/hr)",1.93]
["Filter data","Reported"]
["Train precision (%)",3.39]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported minor"]
["Test dates","2019-07-31"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes",null,null,null,null,null,null,"7/29-8/2/2019"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 8/30/2019"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2019-07-22",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2019-07-29",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2019-07-31",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"Mixing Baffles shown on pg 11",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",null,"lvl 2",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","no",null,null,null,null,null,null,"Medium burn rate did not meet ASTM 2779 requirements <50% of high heat output.",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2020-01-30","No EPA Compliance Date"]
["DEC Calculated Certification Expiration","2025-01-30"]

{"sheet":"SMG HP55","index":84,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","SMG Hearth & Home LLC"]
["Model","HP55"]
["Prelim review recomm."]
["Red flags",7,"Orange flags",null,9,"Yellow flags",null,2,"OM not reviewed"]
["Final Determination","Pending - Major",null,null,null,"Date: 9/1/2020",null,null,"Basis: MD, IR, NR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1599999999999999,null,"PM Highest 1-hr (g/hr)",null,null,1.37]
["Overall HHV efficiency (%)",81.400000000000006]
["Overall heat output (Btu/hr)","Not reported"]
["Overall CO (g/hr)",0,null,null,null,null,0,null,"zero CO emissions reports, needs explaination"]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Partially reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"only 10 hours of aging - method requires 48 hours"]
["Conditioning data","Not reported"]
["Lab technician notes","Partially reported"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,"did not identify issues with medium burn"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.4500000000000002,2.02,1.35]
["Heat output (Btu/hr)",null,35844,29442,19019,null,null,null,37000]
["CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,82,81.599999999999994,79.2]
["Overall PM emissions (g/hr)",1.1599999999999999]
["PM 1-hr filter pull (g/hr)",1.37]
["Filter data","Reported"]
["Train precision (%)",0.83]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Not applicable"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete"]
["Test dates","2019-07-30"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes",null,null,null,null,null,null,"7/29-8/2/2019"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined",null,null,null,null,null,null,"report date 8/5/2019"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI",null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit","2019-07-22",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning","2019-07-29",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing","2019-07-30",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used","other",null,null,null,null,null,null,"Gelman ",null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value","no negative values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements","no",null,null,null,null,null,null,"mixing baffle shown on pg 11",null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,"lvl 5",null,"lvl 2",null,"lvl 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met","no",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date","2020-01-30"]
["DEC Calculated Certification Expiration","2025-01-30"]

{"sheet":"SPA 3.4","index":85,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Extraflame S.P.A."]
["Model","V3.4"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"SPA 4.5","index":86,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Extraflame S.P.A."]
["Model","V4.5"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"SPA 5.2","index":87,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Extraflame S.P.A."]
["Model","V5.2"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Lamonox Jessica air","index":88,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Laminox"]
["Model","Jessica 11air and Veronica 11 air"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Laminox Jessica Natural","index":89,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Laminox"]
["Model","Jessica Natural and Veronica Natural"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"PAC True North 40i","index":90,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Pacific Energy Fireplace Products Limited dba True North"]
["Model","True North 40 Insert"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR","OM not reviewed"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported",null,null,null,null,null,null,"1 PAGE REPORT"]
["Third-party certifier","Not reported"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.36,null,"PM Highest 1-hr (g/hr)",null,null,"NR"]
["Overall HHV efficiency (%)",72.150000000000006]
["Overall heat output (Btu/hr)","Not reported"]
["Overall CO (g/hr)","Not reported",null,null,null,null,"NR"]
["Manufacturers Instructions to lab","Not reported"]
["Efficiency  calculations","Not reported"]
["Burn rate calculations","Not reported"]
["Raw data sheets","Not reported"]
["Conditioning completed by","Not reported"]
["Conditioning data","Not reported"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Not reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low",null,null,null,"THREE RUNS NO DATA PROVIDED"]
["Burn rate (kg/hr)",null,"NR","NR","NR"]
["Heat output (Btu/hr)",null,"NR","NR","NR"]
["CO (g/min)",null,"NR","NR","NR"]
["HHV efficiency (%)",null,"NR","NR","NR"]
["Overall PM emissions (g/hr)",1.36]
["PM 1-hr filter pull (g/hr)","Not reported"]
["Filter data","Not reported"]
["Train precision (%)","Not reported"]
["Negative weights","Not reported"]
["Negs handled appropriately","Cannot be determined"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Not reported"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Not included"]
["Location recommendation","Not included"]
["Guidance on proper draft","Not included"]
["Fuel loading & reloading","Not included"]
["Fuel selection recomm.","Not included"]
["Improper fuels warnings","Not included"]
["Fire starting procedures","Not included"]
["Proper use of air controls","Not included"]
["Proper operation low","Not included"]
["Ash removal procedures","Not included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Not included"]
["Warranty rights","Not included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Not reported"]
["All run data submitted","Not reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Not reported"]
["Test dates","Not Reported"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Cannot be determined"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Even Temp Element P","index":91,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Even Temp"]
["Model","Element Model P"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Paramax Rafael 55a","index":92,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Paramax International"]
["Model","Rafael 55a, Europa 75a"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Thermorossi Pair11","index":93,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Thermorossi"]
["Model","Pair 11, Pair11Plus"]
["Prelim review recomm."]
["Red flags","NR","Orange flags",null,"NR","Yellow flags",null,"NR","OM not reviewed"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Ravelli 120 touch","index":94,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Ravelli"]
["Model","RV120Touch"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination","Pending - Major",null,null,null,"Date: 11/13/2020",null,null,"Basis: IR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Polytests Inc."]
["Third-party certifier","CSA Group"]
["Report certified","Not reported"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.62,null,"PM Highest 1-hr (g/hr)",null,null,2.19]
["Overall HHV efficiency (%)",79.25]
["Overall heat output (Btu/hr)",18821]
["Overall CO (g/hr)",2.8,null,"Overall CO (g/min)",null,null,{"$f":"B17/60","v":4.6666666666666662E-2}]
["Manufacturers Instructions to lab","Not reported",null,null,null,null,null,null,"TOC lists instructions as appendix 13 but no appendix 13 in posted report"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab",null,null,null,null,null,null,"Lab completed pre-testing to confirm the appliance can meet the standard."]
["Conditioning data","Partially reported",null,null,null,null,null,null,"1) Pre-burn data does not meet test method requirements. 2) Insufficient data to determine conformance with med. burn rate requirement. "]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Not reported"]
["Doc. of run validity","Not reported"]
["Doc. of run anomolies","Not reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.48,1.22,0.83]
["Heat output (Btu/hr)",null,37800,18500,12900]
["CO (g/min)"]
["HHV efficiency (%)",null,77.41,78.81,81.540000000000006]
["Overall PM emissions (g/hr)",0.62]
["PM 1-hr filter pull (g/hr)",2.19]
["Filter data","Reported"]
["Train precision (%)",1.78]
["Negative weights","Yes"]
["Negs handled appropriately","No"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","not reported",null,null,null,null,null,null,"Holzpellets - website in German"]
["Pellet fuel certification","Not reported"]
["Source of the pellet specification","Not reported"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Not included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Insufficient data"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Not included"]
["Federal warning (C or NC)","Not included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported major"]
["Test dates","2017-05-12"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly","not reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2020-09-01",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Thelin Company Gnome","index":95,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Thelin Company"]
["Model","Gnome"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Thelin Company Parlour 3000","index":96,"n_rows":110,"n_cols":22,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[90,1,90,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[84,1,84,7],[85,1,85,7],[76,1,76,7],[77,1,77,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[71,1,71,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[66,1,66,7],[63,1,63,7],[64,1,64,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[65,1,65,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[54,1,54,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[14,1,14,7],[5,1,5,4],[5,5,5,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[6,1,6,7]]}
["Summary of Review"]
["Manufacturer","Thelin Company"]
["Model","Parlour 3000"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination","Disapproved",null,null,null,"Date: 9/1/2020",null,null,"Basis: NTR"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","Not reported"]
["Test Lab","Not reported"]
["Third-party certifier"]
["Report certified"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)"]
["Overall HHV efficiency (%)"]
["Overall heat output (Btu/hr)"]
["Overall CO (g/hr)"]
["Manufacturers Instructions to lab"]
["Efficiency  calculations"]
["Burn rate calculations"]
["Raw data sheets"]
["Conditioning completed by"]
["Conditioning data"]
["Lab technician notes"]
["Doc. of run appropriateness"]
["Doc. of run validity"]
["Doc. of run anomolies"]
["Doc. of run burn rates"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)"]
["Heat output (Btu/hr)"]
["CO (g/min)"]
["HHV efficiency (%)"]
["Overall PM emissions (g/hr)"]
["PM 1-hr filter pull (g/hr)"]
["Filter data"]
["Train precision (%)"]
["Negative weights"]
["Negs handled appropriately"]
["Lowest burn rate tested"]
["All run data"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height"]
["Location recommendation"]
["Guidance on proper draft"]
["Fuel loading & reloading"]
["Fuel selection recomm."]
["Improper fuels warnings"]
["Fire starting procedures"]
["Proper use of air controls"]
["Proper operation low"]
["Ash removal procedures"]
["Replacement parts"]
["Federal warning (C or NC)"]
["Warranty rights"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete"]
["All run data submitted"]
["Test report complete"]
["Owner manual complete"]
["Test dates"]
["30 Day notice submitted to EPA"]
["Tested on the proposed date"]
["Tested in one day"]
["60 Day report to EPA"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Test location",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date lab received the unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of conditioning",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["date first day of testing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported for all runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions reported in grams per hour",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions zero or negative",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["first hour PM emissions measured with front and back filter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Zero CO emission reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Any incomplete runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Pre-ignition data reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter changes during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["filter plugged during test run",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["What type of filter used",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe weight >5% of PM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative probe value",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Negative room air values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ambient background filter data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Proportional sampling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - pre-test leak check  reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - any filter change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Leak check - post leak check reported",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Dilution tunnel schematic meets ASTM 2515 requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours reported in summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of conditioning hours with data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["number of hours at correct conditioning conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Air setting data","High",null,"Medium",null,"Low",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["medium burn conditions met",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["high test settings match high in OM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Total number of runs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["run averaging done correctly",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Calibration data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Milestone Date","2022-12-06",null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"US Stove 5780e","index":97,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7]]}
["Summary of Review"]
["Manufacturer","United States Stove Company"]
["Model","5780e,  AP5780E, VG5780E, \nSP5780E, SP58E"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination",null,null,null,null,null,null,null,"Basis: NTR"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","PFS-TECO"]
["Third-party certifier","PFS-TECO"]
["Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.1000000000000001,null,"PM Highest 1-hr (g/hr)",null,null,2.2999999999999998]
["Overall HHV efficiency (%)",76]
["Overall heat output (Btu/hr)",35041]
["Overall CO (g/hr)",{"$f":"G17*60","v":30},null,"Overall CO g/min",null,null,0.5]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Page 27 includes preburn data lacking any weight additions, page 19 includes preconditioning data lacking scale weights"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.34,0.59,0.56999999999999995]
["Heat output (Btu/hr)",null,18796,8292,8215]
["CO (g/min)",null,0.1,0.1,0.1]
["HHV efficiency (%)",null,76,76,77]
["Overall PM emissions (g/hr)",1.1000000000000001]
["PM 1-hr filter pull (g/hr)",2.2999999999999998]
["Filter data","Reported"]
["Train precision (%)",10.199999999999999,null,null,null,null,null,null,"0.15 g/kg"]
["Negative weights","Yes"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Yes"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Bear Mountain Wood Pellet Fuel"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Analysis"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Included"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","All reported"]
["Owner manual complete","All reported"]
["Test dates","2021-12-03"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","No ",null,null,null,null,null,null,"OM does not specifically describe damper positioning for high burn, Manufacturer instructions to lab instruct to have damper half closed. "]
["Test location","Lab",null,null,null,null,null,null,"PFS-TECO Portland Laboratory, 11785 SE HWY 212 - Suite 305, Clackamas, OR 97015"]
["date lab received the unit","2021-11-18"]
["date first day of conditioning","2021-11-29"]
["date first day of testing","2021-12-03"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,"filter sheets do not label front or back filter"]
["Zero CO emission reported","no"]
["Any incomplete runs","no"]
["Pre-ignition data reported"]
["filter changes during test run","not reported"]
["filter plugged during test run","no"]
["What type of filter used","not reported"]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","no negatives"]
["Ambient background filter data","no negatives"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change","Meets Specification"]
["Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50]
["number of hours at correct conditioning conditions","Cannot be Determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","yes"]
["Air setting data","High",null,"Medium",null,"Low"]
[null,5,"half closed",1,"closed",1,"closed",null,"med and low have same settings"]
["medium burn conditions met"]
["high test settings match high in OM","no",null,null,null,null,null,null,"Owner manual states \"On higher feed rates, \nthe damper should be open more by having it set \nmore towards the right\", no exact high setting is designated, instructions and test notes state that the damper was set to half closed."]
["Total number of runs",1]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"Some outside of 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"US Stove KP5513","index":98,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7]]}
["Summary of Review"]
["Manufacturer","United States Stove Company "]
["Model","KP5513, KP5513-P, KP5513-L, \nUS5513, US5513-P, US5513-L, AP5613, \nAP5613-P, AP5613-L, VG5713, \nVG5713-P, VG5713-L, Little E (SP500), \n5501S-XH"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","PFS-TECO"]
["Third-party certifier","PFS-TECO"]
["Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.5,null,"PM Highest 1-hr (g/hr)",null,null,2.4]
["Overall HHV efficiency (%)",76]
["Overall heat output (Btu/hr)",42471]
["Overall CO (g/hr)",{"$f":"0.5*60","v":30},null,null,null,null,0.5]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Data included on page 19 of report does not include scale weights"]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.69,0.79,0.75]
["Heat output (Btu/hr)",null,24676,11193,10609]
["CO (g/min)",null,0.4,0.1,0.1]
["HHV efficiency (%)",null,79,76,76]
["Overall PM emissions (g/hr)",1.5]
["PM 1-hr filter pull (g/hr)",2.4]
["Filter data","Reported"]
["Train precision (%)",3.7]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Yes"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Hardwood",null,null,null,null,null,null,"Bear Mountain Wood Pellet Fuel"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Analysis"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Insufficient data",null,null,null,null,null,null,"pg 316 states \"To achieve a “medium burn” your stove should be set on setting 1 with the damper fully closed.To achieve a “low burn” your stove should be set on setting 1 with the damper open.\""]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","All reported"]
["Owner manual complete","All reported"]
["Test dates","2021-12-02"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes"]
["Tested in one day","Yes"]
["60 Day report to EPA","Yes"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","No",null,null,null,null,null,null,"no explicit setting for highest operating setting is communicated in the OM"]
["Test location","Lab"]
["date lab received the unit","2021-11-18"]
["date first day of conditioning","2021-11-22"]
["date first day of testing","2021-12-02"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported"]
["Zero CO emission reported","no"]
["Any incomplete runs","no"]
["Pre-ignition data reported"]
["filter changes during test run","no"]
["filter plugged during test run","no"]
["What type of filter used","not reported"]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","no negatives"]
["Ambient background filter data","no negatives"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change"]
["Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50]
["number of hours at correct conditioning conditions","cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","yes"]
["Air setting data","High",null,"Medium",null,"Low"]
[null,5,"open",1,"closed",1,"closed",null,"med & low have same setting"]
["medium burn conditions met"]
["high test settings match high in OM","no",null,null,null,null,null,null,"no explicit setting for highest operating setting is communicated in the OM"]
["Total number of runs",1]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"Some outside of 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"PS20W","index":99,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group Inc"]
["Model","PS20W, PS20WTS, C30XL, H30XL, J30XL, N30XL"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",null,null,"PM Highest 1-hr (g/hr)",null,null,null,null,"Three runs conducted 2 considered invalid, no First hour data or overall PM provided for run 1, all run data must be reported. Report states that Run 1 ran for 210 minutes but no 1hr or any filter data was reported. Data shows run 1 actually ran 360 minutes"]
["Overall HHV efficiency (%)",76,null,null,null,null,null,null,"Run 2 which was considered invalid had an HHV of 71"]
["Overall heat output (Btu/hr)",23945,null,null,null,null,null,null,"Run 2 which was considered invalid had an output of 22880"]
["Overall CO (g/hr)",0,null,"Overall CO (g/min)",null,null,0,null,"Run 2 which was considered invalid had a CO emission of 1.32"]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Partially reported",null,null,null,null,null,null,"Run 2 did not include CSA Calculation"]
["Burn rate calculations","Partially reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"conditioning data lacking constant weight to determine compliance with med burn rate"]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,3,3,3]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.77,0.81,0.8]
["Heat output (Btu/hr)",null,23945,10965,10796]
["CO (g/min)",null,0,0,0]
["HHV efficiency (%)",null,75,75,75]
["Overall PM emissions (g/hr)",1.22]
["PM 1-hr filter pull (g/hr)",4.0599999999999996,null,null,null,null,null,null,"run 2 - 3.93, run 1 not reported"]
["Filter data","Not reported",null,null,null,null,null,null,"no data for run 1, pg 138 for run 2, pog 181 for run 3 - filter data sheet not clearly labeled. "]
["Train precision (%)",7.7,null,null,null,null,null,null,".194 g/kg"]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Email from Manufacturer"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Insufficient data"]
["Proper operation low","Insufficient data"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported major"]
["Test dates","8/11-8/27/2021",null,null,null,null,null,null,"Three runs conducted over the course of 3 weeks"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes",null,null,null,null,null,null,"and two others"]
["Tested in one day","No"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined"]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit","2021-08-03"]
["date first day of conditioning","2021-08-03"]
["date first day of testing","2021-08-11"]
["first hour PM emissions reported for all runs","no"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","yes",null,null,null,null,null,null,"Best guess as filter data is poorly labled."]
["Zero CO emission reported","yes"]
["Any incomplete runs","yes"]
["Pre-ignition data reported"]
["filter changes during test run","not reported"]
["filter plugged during test run","not reported"]
["What type of filter used","not reported",null,null,null,null,null,null,"Gelman"]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","not reported"]
["Ambient background filter data","not reported"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"pg 115?"]
["Leak check - any filter change","not reported"]
["Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary","48+"]
["number of conditioning hours with data",50.2]
["number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[null,1,null,3,null,4]
["medium burn conditions met","yes"]
["high test settings match high in OM","not reported"]
["Total number of runs",3]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"some outside of the 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"PS60W","index":100,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[4,5,4,6],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[9,1,9,7],[10,1,10,7],[11,1,11,7],[12,1,12,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group Inc"]
["Model","PS60W, PS60WTS, C80XL, H80XL, J80XL, N80XL"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.72699999999999998,null,"PM Highest 1-hr (g/hr)",null,null,1.0369999999999999]
["Overall HHV efficiency (%)",81.400000000000006]
["Overall heat output (Btu/hr)",13862]
["Overall CO (g/hr)",{"$f":"G17/60","v":1.1283333333333334E-2},null,"Overall CO (g/min)",null,null,0.67700000000000005]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data does not include continuous weight for calculation of burnrate."]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,1.9,0.86,0.68]
["Heat output (Btu/hr)",null,28165,12537,9739]
["CO (g/min)",null,0.59,0.65700000000000003,0.76700000000000002]
["HHV efficiency (%)",null,82.1,80.900000000000006,79.099999999999994]
["Overall PM emissions (g/hr)",0.72699999999999998]
["PM 1-hr filter pull (g/hr)",1.0369999999999999]
["Filter data","Reported",null,null,null,null,null,null,"pg 124"]
["Train precision (%)",3.38]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Certificate included in report"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Insufficient data"]
["Proper operation low","Insufficient data"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported major"]
["Test dates","2021-08-09"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined",null,null,null,null,null,null,"instructions do not include fan settings"]
["Test location","Lab"]
["date lab received the unit","2021-08-03"]
["date first day of conditioning","2021-08-03"]
["date first day of testing","2021-08-09"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported"]
["Zero CO emission reported","no"]
["Any incomplete runs","no"]
["Pre-ignition data reported"]
["filter changes during test run","not reported"]
["filter plugged during test run","not reported"]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters"]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","not reported"]
["Ambient background filter data","not reported"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"Pg 106?"]
["Leak check - any filter change","not reported"]
["Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50.2]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"data  reported in 10 min increments"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met","not reported"]
["high test settings match high in OM","not reported"]
["Total number of runs",1]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"some outside of the 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"PS130W","index":101,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group Inc"]
["Model","PS130W, PS130WTS, C140XL, H140XL, J140XL, N140XL"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.42,null,"PM Highest 1-hr (g/hr)",null,null,3.42]
["Overall HHV efficiency (%)",78.7]
["Overall heat output (Btu/hr)",20414]
["Overall CO (g/hr)",{"$f":"G17*60","v":7.1999999999999993},null,null,null,null,0.12,null,"pg 131 reports CO g/hr 6.99"]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data on page 374 does not include continuous weights for calculation of burnrate."]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,2,2,2,null,null,null,"Run 1 was considered invalid due to the device shutting down after 20 minutes. "]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.86,1.17,1.1399999999999999]
["Heat output (Btu/hr)",null,39460,16644,16149]
["CO (g/min)",null,0,0.14000000000000001,0.15]
["HHV efficiency (%)",null,76.3,78.400000000000006,78.7]
["Overall PM emissions (g/hr)",1.42]
["PM 1-hr filter pull (g/hr)",3.42]
["Filter data","Reported",null,null,null,null,null,null,"pg 151"]
["Train precision (%)",1.34]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined"]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","NFI"]
["Source of the pellet specification"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Insufficient data"]
["Proper operation low","Insufficient data"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","Partially reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","Partially reported minor"]
["Test dates","2021-08-13"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes"]
["Tested in one day","No"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same"]
["Test location","Lab"]
["date lab received the unit","2021-08-03"]
["date first day of conditioning","2021-08-03"]
["date first day of testing","2021-08-13"]
["first hour PM emissions reported for all runs","no",null,null,null,null,null,null,"Run 1 was considered invalid due to the device shutting down after 20 minutes. "]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported","yes"]
["Any incomplete runs","yes"]
["Pre-ignition data reported"]
["filter changes during test run","no"]
["filter plugged during test run","no"]
["What type of filter used","other",null,null,null,null,null,null,"elman A/E 61631 binder free, 47-mm diameter filters."]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","no negatives"]
["Ambient background filter data","no negatives"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"pg 89&90?"]
["Leak check - any filter change","not reported"]
["Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Does not meet specification",null,null,null,null,null,null,"mixing baffles noted on page 8"]
["number of conditioning hours reported in summary","50+"]
["number of conditioning hours with data",52.3]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"no constant weight provided in data thus burn rate is not confirmed"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[null,1,null,2,null,4,null,null,"data does not mention fan settings"]
["medium burn conditions met","not reported"]
["high test settings match high in OM","not reported"]
["Total number of runs",2,null,null,null,null,null,null,"First run stopped at 20 min"]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"Some calibrations are outside of 6 month requirement."]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"PSBF66W","index":102,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7]]}
["Summary of Review"]
["Manufacturer","Enerco Group Inc."]
["Model","PSBF66W, PSBF66WTS, C3W80XL, H3W80XL, J3W80XL, N3W80XL"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","Intertek"]
["Third-party certifier","Intertek"]
["Report certified","Intertek"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.22,null,"PM Highest 1-hr (g/hr)",null,null,1.86]
["Overall HHV efficiency (%)",80.8]
["Overall heat output (Btu/hr)",15340]
["Overall CO (g/hr)",{"$f":"G17*60","v":3.5999999999999996},null,null,null,null,0.06]
["Manufacturers Instructions to lab","Reported"]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data does not include continuous weight for calculation of burnrate."]
["Lab technician notes","Not reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1]
["Run Category",null,"High","Med","Low"]
["Burn rate (kg/hr)",null,2.17,1.02,0.7]
["Heat output (Btu/hr)",null,31107,15340,10151]
["CO (g/min)",null,0,0.06,0.09]
["HHV efficiency (%)",null,79.2,80.099999999999994,80.8]
["Overall PM emissions (g/hr)",1.22]
["PM 1-hr filter pull (g/hr)",1.86]
["Filter data","Reported",null,null,null,null,null,null,"pg 123"]
["Train precision (%)",7.16]
["Negative weights","no"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Low test segment conducted at P1, however owner's manual indicates ability to adjust feed rate & fan speeds to lower settings, the report does not indicate fan speed for settings."]
["All run data","Not reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type",null,null,null,null,null,null,null,"Marthwood"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","certificate included in report"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Insufficient data"]
["Proper operation low","Insufficient data"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","Partially reported"]
["Test report complete","Partially reported major"]
["Owner manual complete","Partially reported major"]
["Test dates","2021-08-10"]
["30 Day notice submitted to EPA","Yes"]
["Tested on the proposed date","Yes"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Cannot be determined"]
["Test location","Lab",null,null,null,null,null,null,"Middleton, WI"]
["date lab received the unit","2021-08-03"]
["date first day of conditioning","2021-08-03"]
["date first day of testing","2021-08-10"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","yes"]
["Zero CO emission reported","yes",null,null,null,null,null,null,"During the high test segment."]
["Any incomplete runs","no"]
["Pre-ignition data reported"]
["filter changes during test run","no",null,null,null,null,null,null,"It does not appear that any changes occurred however dilter data is not adequately labeled. "]
["filter plugged during test run","no"]
["What type of filter used","other",null,null,null,null,null,null,"Gelman A/E 61631 binder free, 47-mm diameter filters"]
["Negative probe weight >5% of PM","no negatives"]
["Negative probe value","no negatives"]
["Negative room air values","not reported",null,null,null,null,null,null,"unable to locate information in report"]
["Ambient background filter data","not reported"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported",null,null,null,null,null,null,"pg 106?"]
["Leak check - any filter change","not reported"]
["Leak check - post leak check reported","not reported"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Meets Specification"]
["number of conditioning hours reported in summary","50+"]
["number of conditioning hours with data",52.3]
["number of hours at correct conditioning conditions","Cannot be determined",null,null,null,null,null,null,"Data presented in 10min increments"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)"]
["Air setting data","High",null,"Medium",null,"Low"]
[]
["medium burn conditions met","not reported"]
["high test settings match high in OM","not reported"]
["Total number of runs",1]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"some outside 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Whitney","index":103,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7]]}
["Summary of Review"]
["Manufacturer","Sun Mountain Stove Works Inc"]
["Model","Whitney"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","No Determination List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","OMNI"]
["Third-party certifier","OMNI"]
["Report certified","Omni"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",0.47199999999999998,null,"PM Highest 1-hr (g/hr)",null,null,0.85399999999999998]
["Overall HHV efficiency (%)",67.8]
["Overall heat output (Btu/hr)",11282]
["Overall CO (g/hr)",{"$f":"G17*60","v":3.48},null,"Overall CO (g/min)",null,null,5.8000000000000003E-2]
["Manufacturers Instructions to lab","Partially reported",null,null,null,null,null,null,"Although no separate document is included in report, there is a summary of instructions."]
["Efficiency  calculations","Reported"]
["Burn rate calculations","Reported"]
["Raw data sheets","Reported"]
["Conditioning completed by","Lab"]
["Conditioning data","Partially reported",null,null,null,null,null,null,"Conditioning data did not include hourly wieghts only weight added unable to calculate burn rate with supplied info."]
["Lab technician notes","Reported"]
["Doc. of run appropriateness","Reported"]
["Doc. of run validity","Reported"]
["Doc. of run anomolies","Reported"]
["Doc. of run burn rates","Reported"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,2,2,2]
["Run Category",null,"H","M","L","H","M","L","Run one was noted as invalid due to not being 50% of the high burn rate."]
["Burn rate (kg/hr)",null,1.76,1.02,0.66,1.72,0.82,0.62]
["Heat output (Btu/hr)",null,25003,12404,7651,25102,9800,7591]
["CO (g/min)",null,"NR","NR","NR","NR","NR","NR"]
["HHV efficiency (%)",null,75.8,64.400000000000006,62.1,76.099999999999994,62.6,64.099999999999994]
["Overall PM emissions (g/hr)",0.47199999999999998]
["PM 1-hr filter pull (g/hr)",0.85399999999999998]
["Filter data","Reported"]
["Train precision (%)",10.63,null,null,null,null,null,null,"11.93 - Run 1"]
["Negative weights","Yes"]
["Negs handled appropriately","Yes"]
["Lowest burn rate tested","Cannot be determined",null,null,null,null,null,null,"Noted instructions state low burn was conducted with heat slide fully open"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Golden fire Pellets - Doug Fir",null,null,null,null,null,null,"Run 1 - Blazer Pellets"]
["Pellet fuel certification","PFI"]
["Source of the pellet specification","Bag & Analytical report",null,null,null,null,null,null,"pg 58"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included"]
["Location recommendation","Included"]
["Guidance on proper draft","Included"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included"]
["Improper fuels warnings","Included"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included"]
["Proper operation low","Insufficient data"]
["Ash removal procedures","Included"]
["Replacement parts","Included"]
["Federal warning (C or NC)","Included"]
["Warranty rights","Included"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported"]
["All run data submitted","All reported"]
["Test report complete","All reported"]
["Owner manual complete","Partially reported major"]
["Test dates","7/22 - 7/29 2020"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","No"]
["60 Day report to EPA","No"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Owners manual does not address operation on a high setting only operation in general"]
["Test location","Not reported"]
["date lab received the unit","Not reported"]
["date first day of conditioning","2020-07-13"]
["date first day of testing","2020-07-22"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","no"]
["Zero CO emission reported","no"]
["Any incomplete runs","no"]
["Pre-ignition data reported","yes"]
["filter changes during test run","no"]
["filter plugged during test run","no"]
["What type of filter used","not reported"]
["Negative probe weight >5% of PM","reported and handled correctly"]
["Negative probe value","no negative values"]
["Negative room air values","no negative values"]
["Ambient background filter data","no negative values"]
["Proportional sampling","yes with allowable deviations"]
["Leak check - pre-test leak check  reported","not reported"]
["Leak check - any filter change","not reported"]
["Leak check - post leak check reported","yes with allowable deviations"]
["Dilution tunnel schematic meets ASTM 2515 requirements","not reported"]
["number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50]
["number of hours at correct conditioning conditions","Cannot be determined"]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","not reported"]
["Air setting data","High",null,"Med",null,"low"]
[null,"fully closed",null,"1.5 from fully closed",null,"fully open"]
["medium burn conditions met"]
["high test settings match high in OM","not reported"]
["Total number of runs",2]
["run averaging done correctly"]
["Calibration data","partially reported",null,null,null,null,null,null,"included though some are outside of the 6 month requirement"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]

{"sheet":"Meridian II","index":104,"n_rows":110,"n_cols":9,"rows_kept":110,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,2,4,3],[4,5,4,6],[10,1,10,7],[11,1,11,7],[12,1,12,7],[13,1,13,2],[13,3,13,5],[13,6,13,7],[5,1,5,4],[5,5,5,7],[6,1,6,7],[7,1,7,7],[8,1,8,7],[9,1,9,7],[18,1,18,7],[19,1,19,7],[20,1,20,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[14,1,14,7],[15,1,15,7],[16,1,16,2],[16,3,16,5],[16,6,16,7],[17,1,17,7],[36,1,36,7],[37,1,37,7],[38,1,38,7],[39,1,39,7],[40,1,40,7],[41,1,41,7],[24,1,24,7],[25,1,25,7],[26,1,26,7],[27,1,27,7],[28,1,28,7],[35,1,35,7],[48,1,48,7],[49,1,49,7],[50,1,50,7],[51,1,51,7],[52,1,52,7],[53,1,53,7],[42,1,42,7],[43,1,43,7],[44,1,44,7],[45,1,45,7],[46,1,46,7],[47,1,47,7],[60,1,60,7],[61,1,61,7],[62,1,62,7],[63,1,63,7],[64,1,64,7],[65,1,65,7],[54,1,54,7],[55,1,55,7],[56,1,56,7],[57,1,57,7],[58,1,58,7],[59,1,59,7],[72,1,72,7],[73,1,73,7],[74,1,74,7],[75,1,75,7],[76,1,76,7],[77,1,77,7],[66,1,66,7],[67,1,67,7],[68,1,68,7],[69,1,69,7],[70,1,70,7],[71,1,71,7],[84,1,84,7],[85,1,85,7],[86,1,86,7],[87,1,87,7],[88,1,88,7],[89,1,89,7],[78,1,78,7],[79,1,79,7],[80,1,80,7],[81,1,81,7],[82,1,82,7],[83,1,83,7],[100,0,101,0],[100,1,100,2],[100,3,100,4],[100,5,100,6],[90,1,90,7],[91,1,91,7],[92,1,92,7],[93,1,93,7],[94,1,94,7],[95,1,95,7],[102,1,102,7],[103,1,103,7],[104,1,104,7],[105,1,105,7],[106,1,106,7],[96,1,96,7],[97,1,97,7],[98,1,98,7],[99,1,99,7]]}
["Summary of Review"]
["Manufacturer","Sherwood Industries Ltd."]
["Model","Enviro Meridian-2, Meridian FPI-2, Meridian Cast Iron-2, Regency Greenfire – GF55-2, GFI55-2"]
["Prelim review recomm."]
["Red flags",null,"Orange flags",null,null,"Yellow flags"]
["Final Determination"]
["AK List Status","Disapproved List"]
["Testing Information","Determination",null,null,null,null,null,null,"Notes"]
["Test method","ASTM 2779"]
["Test Lab","PFS-TECO"]
["Third-party certifier","PFS-TECO"]
["Report certified","PFS-TECO"]
["Test Report Elements","Determination",null,null,null,null,null,null,"Notes"]
["Overall PM emissions (g/hr)",1.84,null,"PM Highest 1-hr (g/hr)",null,null,8.6,null,"integrated Pg. 7"]
["Overall HHV efficiency (%)",75.099999999999994,null,null,null,null,null,null,"pg. 7"]
["Overall heat output (Btu/hr)",13698,null,null,null,null,null,null,"pg. 7"]
["Overall CO (g/hr)",2.1700000000000001E-3,null,"Overall CO (g/min)",null,null,0.13,null,"pg. 7"]
["Manufacturers Instructions to lab","Reported",null,null,null,null,null,null,"pg. 21"]
["Efficiency  calculations","Reported",null,null,null,null,null,null,"pg. 23"]
["Burn rate calculations","Reported",null,null,null,null,null,null,"pg. 23"]
["Raw data sheets","Reported",null,null,null,null,null,null,"pg. 31"]
["Conditioning completed by","Manufacturer",null,null,null,null,null,null,"pg. 5"]
["Conditioning data","Reported",null,null,null,null,null,null,"pg. 19"]
["Lab technician notes","Reported",null,null,null,null,null,null,"pg. 56"]
["Doc. of run appropriateness","Reported",null,null,null,null,null,null,"pg. 8"]
["Doc. of run validity","Reported",null,null,null,null,null,null,"pg. 8"]
["Doc. of run anomolies","Reported",null,null,null,null,null,null,"pg. 8"]
["Doc. of run burn rates","Reported",null,null,null,null,null,null,"pg. 8"]
["Test Run Data","Determination",null,null,null,null,null,null,"Notes"]
["Run #",null,1,1,1,1,null,null,"pg. 7"]
["Run Category",null,"H","M","L","OA",null,null,"pg. 7"]
["Burn rate (kg/hr)",null,2.11,0.93,0.57999999999999996,0.95,null,null,"pg. 7"]
["Heat output (Btu/hr)",null,32739,12989,7751,13698,null,null,"pg. 7"]
["CO (g/min)",null,0.63,0.05,0.04,0.13,null,null,"pg. 7"]
["HHV efficiency (%)",null,80.7,73.099999999999994,69.7,75.099999999999994,null,null,"pg. 7"]
["Overall PM emissions (g/hr)",1.84,null,null,null,null,null,null,"pg. 7"]
["PM 1-hr filter pull (g/hr)",8.6,null,null,null,null,null,null,"pg. 7"]
["Filter data","Reported",null,null,null,null,null,null,"pg. 55"]
["Train precision (%)","Reported",null,null,null,null,null,null,"pg. 23"]
["Negative weights","Reported",null,null,null,null,null,null,"pg. 55"]
["Negs handled appropriately","Yes",null,null,null,null,null,null,"pg. 55"]
["Lowest burn rate tested","Yes",null,null,null,null,null,null,"pg. 9"]
["All run data","Reported"]
["Appliance Fueling","Determination",null,null,null,null,null,null,"Notes"]
["Pellet species/type","Lignetics",null,null,null,null,null,null,"pg. 13"]
["Pellet fuel certification","Yes",null,null,null,null,null,null,"pg. 13"]
["Source of the pellet specification","Twin Ports Testing",null,null,null,null,null,null,"pg. 14"]
["Owners Manual Req.","Determination",null,null,null,null,null,null,"Notes"]
["Stack height","Included",null,null,null,null,null,null,"pg. 92"]
["Location recommendation","Included",null,null,null,null,null,null,"pg. 89"]
["Guidance on proper draft","Included",null,null,null,null,null,null,"pg. 93"]
["Fuel loading & reloading","Included"]
["Fuel selection recomm.","Included",null,null,null,null,null,null,"pg. 115"]
["Improper fuels warnings","Included",null,null,null,null,null,null,"pg. 115 & 77"]
["Fire starting procedures","Included"]
["Proper use of air controls","Included",null,null,null,null,null,null,"pg. 117"]
["Proper operation low","Included",null,null,null,null,null,null,"pg. 118"]
["Ash removal procedures","Included",null,null,null,null,null,null,"pg. 122"]
["Replacement parts","Included",null,null,null,null,null,null,"pg. 147"]
["Federal warning (C or NC)","Included",null,null,null,null,null,null,"pg. 3"]
["Warranty rights","Included",null,null,null,null,null,null,"pg. 153"]
["Reporting","Determination",null,null,null,null,null,null,"Notes"]
["Summary tables complete","All reported",null,null,null,null,null,null,"pg. 8"]
["All run data submitted","All reported"]
["Test report complete","Partially reported minor"]
["Owner manual complete","All reported"]
["Test dates","2021-04-13"]
["30 Day notice submitted to EPA","Cannot be determined"]
["Tested on the proposed date","Cannot be determined"]
["Tested in one day","Yes"]
["60 Day report to EPA","Cannot be determined"]
["EPA additional Review Elements","Determination",null,null,null,null,null,null,"Notes"]
["check owners manual and highest setting in test are they the same","Yes"]
["Test location","Lab"]
["date lab received the unit","2021-04-12"]
["date first day of conditioning","Not Reported"]
["date first day of testing","2021-04-13"]
["first hour PM emissions reported for all runs","yes"]
["first hour PM emissions reported in grams per hour","yes"]
["first hour PM emissions zero or negative","no"]
["first hour PM emissions measured with front and back filter","not reported",null,null,null,null,null,null,"They state that the front filter was changed after the 1st hour but I am unsure if the back filter was used as well"]
["Zero CO emission reported","no"]
["Any incomplete runs","no"]
["Pre-ignition data reported","yes",null,null,null,null,null,null,"pg. 29"]
["filter changes during test run","no"]
["filter plugged during test run","no"]
["What type of filter used","glass fiber"]
["Negative probe weight >5% of PM","no negatives",null,null,null,null,null,null,"negative on O-ring pg. 55"]
["Negative probe value","no negatives"]
["Negative room air values","no negatives"]
["Ambient background filter data","no negatives"]
["Proportional sampling","yes with allowable deviations",null,null,null,null,null,null,"pg. 31"]
["Leak check - pre-test leak check  reported","Meets Specification",null,null,null,null,null,null,"pg. 56?"]
["Leak check - any filter change","Meets Specification"]
["Leak check - post leak check reported","Meets Specification"]
["Dilution tunnel schematic meets ASTM 2515 requirements","Does not meet specification",null,null,null,null,null,null,"pg. 15"]
["number of conditioning hours reported in summary",50]
["number of conditioning hours with data",50]
["number of hours at correct conditioning conditions",50]
["used lowest air settings for low burn (ASTM 3053) or Cat 1(M28R)","yes"]
["Air setting data","High",null,"Med",null,"Low",null,null,"Pg. 9"]
[null,"Heat-5","Feed-5,comb-5","Heat-2","Frrd-2, comb.-1","Heat-1","Feedd-1, Comb-1"]
["medium burn conditions met","yes"]
["high test settings match high in OM","yes"]
["Total number of runs",1]
["run averaging done correctly","yes"]
["Calibration data","yes",null,null,null,null,null,null,"pg. 155"]
["Milestone Date",null,null,null,null,null,null,null,"missing report elements"]
["Compliance Date"]
["DEC Calculated Certification Expiration"]